Release Notes:

Emulex Drivers for VMware ESXi, 

Company name :ECD,AvagoTechnologies PVT Ltd.
Driver name and description : be2net and elxnet NIC driver
Driver version: 10.7.110.5 and 10.7.110.13
Supported ESXi release(s) : ESXi 5.1, ESXi 5.5 and ESXi 6.0
List of issues fixed in the release: 
a)Added new debug stats in driver stats proc node
b)Added OCe10100 series adapter PCI IDs back into NIC driver 
c)When SR IOV is enabled in OCe11100 series adapter BIOS, Tx pkts less than equal 32 bytes can cause TX Path to stall
d)elxnet: Revisit the necessity and logic of adapter link_up,link_speed
e)PSOD Observed while running overnight load or unload the driver with mtu change elxnet driver in ESXi 6.0 with the RSS and SRIOV enable
f)ASYNC_DEBUG_EVENT_TYPE_QNQ callback check is not needed for VLAN insertion in driver
g)FTS Blade OCe11100 series LOM not able to get DHCP IP when in UMC mode with ESXi 6.0
h)Lhbacmd returning all zeros for Permanent MAC address after performing link toggle using vsish

New features (if applicable):NA
Known issues : NA
Note: For more information on software downloads and release notes, please refer to http://www.emulex.com/downloads/emulex.html
