                              Release Notes
                        QLogic CNIC VMware Driver

                          QLogic Corporation

               Copyright (c) 2015 QLogic Corporation
                           All rights reserved

cnic 2.712.70.v[50,55,60].3 (Oct 05, 2015)
====================================
  Fixes:
   ------
   1. Problem: drv_state is not properly populated in bnx2x.
 
      Change: cnic code is modified to send proper driver_state to bnx2x driver.

cnic 2.712.70.v[50,55,60].2 (Sep. 07, 2015)
====================================
	1. Change: Update driver version since storm fw has changed.

cnic 2.712.70.v[50,55,60].1 (Jul. 29, 2015)
====================================
	1. Problem: Getting incorrect physical port number for dual port adapter
		with NPAR enabled.

      Change: Populate pf_num and pf_id during cnic init.

	2. Change: Modified driver version from 712.50 to 712.70 for OEM Project.

cnic 2.712.50.v[50,55,60].5 (Jul. 17, 2015)
====================================
   Enhancements
   ------------
		1. BNX2I/BNX2FC: Added support to get physical port number
			in ioctl interface.

cnic 2.712.50.v[50,55,60].4 (Jun. 19, 2015)
====================================
   Enhancements
   ------------
      Change: Modified driver version to sync with other components.

cnic 2.712.50.v[50,55,60].3 (May. 28, 2015)
====================================
   Enhancements
   ------------
      Change: Modified driver version to sync with other components.

cnic 2.712.50.v[50,55,60].2 (May. 12, 2015)
====================================
   Enhancements
   ------------
      Change: Modified driver version to sync with other components.

cnic 2.712.50.v[50,55,60].1 (Apr. 06, 2015)
====================================
   Enhancements
   ------------
      Change: Modified driver version from 712.40 to 712.50 for OEM Project.

cnic 2.712.40.v[50,55].1 (Feb. 12, 2015)
====================================
   Enhancements
   ------------
      Change: Modified driver version from 712.30 to 712.40 for OEM Project.

cnic 2.712.30.v[50,55].3 (Feb. 16, 2015)
====================================
   Enhancements
   ------------
		1. BNX2I: Added initial IOCTL support for BNX2I.

cnic 2.712.30.v[50,55].2 (Jan. 19, 2015)
====================================
   Enhancements
   ------------
      Change: Modified driver version for release.

cnic 2.712.30.v[50,55].1 (Jan. 12, 2015)
====================================
   Enhancements
   ------------
      Change: Modified driver version from 712.10 to 712.30 for OEM Project.

cnic 2.712.10.v[50,55].3 (Nov. 25, 2014)
====================================
   Fixes:
   ------
   1. Problem: Cont00076953: bnx2fc failed to load due to missing namespace with 50.712.11
   2. Problem: Cont00076954: bnx2i failed to load due to missing namespace.

      Change: Corrected the namespace and both Cont00076953 & Cont00076954 got fixed.

      Impact: Esxi 5.0 only.

cnic 2.712.10.v[50,55].2 (Nov. 21, 2014)
====================================

   Fixes:
   ------
   1. Problem: Cont00076639: Rebranding- Driver modules namespace field shown "Broadcom" wording.
 
      Change: Corrected the namespace.

cnic 2.712.10.v[50,55].1 (Oct. 28, 2014)
====================================

   Fixes:
   ------
   1. Problem: Cont00076353- ESX 55 : Failed to load bnx2x driver due to invalid or missing namespace.
 
      Change: Corrected the namespace in cnic.sc file and changed driver version from 710.70 to 712.10 for OEM project.		

cnic 2.710.70.v[50,55].2 (Oct. 16, 2014)
====================================

   Enhancements
   ------------
   1. Rebranded from Broadcom -> QLogic

cnic 2.710.70.v[50,55].1 (Aug. 28, 2014)
====================================

   Enhancements
   ------------
   1.Release for T7.10c.

cnic 2.710.50.v[50,55].1 (Jul. 15, 2014)
====================================

   Enhancements
   ------------
   1.Release for T7.10b.	

cnic 2.710.36.v[50,55].1 (Jun. 24, 2014)
====================================

   Fixes:
   ------
   1. Problem: Cont00074054- ESX 51 : Load of <cnic> failed , Load of <bnx2i> failed : missing required namespace.
     Change: Changed 7a in driver version string to 710.		

cnic 2.7a.36.v[50,55].1 (Jun. 24, 2014)
====================================

   Enhancements
   ------------
   1. Change: Add additional parameter for debug info in bnx2i proc. 


cnic 2.7a.35.v[50,55].1 (May 13, 2014)
====================================

   Enhancements
   ------------
   1. Change: Added additional parameter to pass UFP sub mode.


cnic 2.7a.34.v[50,55].1 (May 7, 2014)
====================================
   Fixes
   -----
   1. Problem: CQ73483 - NXII drivers are throwing dependency error when trying
               to install on ESXi5.x system.
      
      Change:  Updated cnic major version to 2 to allow 'esxcli vib updates'
               command to occur.

      Impact:  All devices.

   Enhancements
   ------------
   1. Change: Added UFP FCoE support


cnic 1.7a.33.v[50,55,60].1 (May 1, 2014)
====================================
   Fixes
   -----
   1. Problem: CQ73608 - Incorrect driver name displayed in CNIC messages
               ie. bnx2x: Added CNIC device: vmnic1 
      
      Change:  The macro used to define PFX is incorrect and not pointing to
               the correct CNIC namespace

      Impact:  All devices.

cnic 1.7a.32.v[50,55].1 (Apr. 23, 2014)
====================================
   Enhancements
   ------------
   1. Change: Added printk()'s on the error paths.

cnic 1.7a.31.v[50,55].2 (Apr. 15, 2014)
====================================
   Enhancements
   ------------
   1. Change: Sync'ed with the latest bnx2x-1.7a.33.v[50,55].1 header files

cnic 1.7a.31.v[50,55].1 (Apr. 10, 2014)
====================================
   Fixes
   -----
   1. Problem: DMA to address 0x0 IOMMU fault on memory allocation failures.

      Change:  Properly return the correct error code in
               cnic.c::cnic_alloc_bnx2_resc() when there is a failure in
               allocating any of the context tables.  Without the proper
               return code the setup for the offload process will continue
               and eventually pass 0x0 to the FW to DMA which causes the
               IOMMU PSOD.

      Impact:  570x iSCSI only.

cnic 1.7a.30.v[50,55].2 (Mar. 06, 2014)
====================================
   Enhancements
   ------------
   1. Change: Sync'ed with the latest bnx2x-1.7a.31.v[50,55].1 header files

cnic 1.7a.30.v[50,55].1 (Feb. 25, 2014)
====================================
   Enhancements
   ------------
   1. Branched for T7.10a


cnic 1.7a.05.v[50,55,60].1 (Feb. 05, 2014)
====================================
   Fixes
   -----
   1. Problem: CQ72694 - PSOD at bnx2x_cnic_notify after upgrade driver.
      
      Change:  For per device operations, cnic needs to derefernce the 
               ulp_ops from the RCU protected cp->ulp_ops instead of 
               the global cnic_ulp_tbl.  In 2 locations, 
               cnic_send_nlmsg() and cnic_copy_ulp_stats(),it was referencing 
               the global table. If the device has been unregistered, this bug 
               can lead to a crash.

      Impact:  All devices without iSCSi or FCOE licenses.

   Enhancements
   ------------
   1. Change: Sync'ed with the latest bnx2x-1.7a.08.v[50,55].1 header files

 
cnic 1.7a.04.v[50,55,60].2 (Jan. 30, 2014)
====================================
   Enhancements
   ------------
   1. Change: Sync'ed with the latest bnx2x-1.7a.07.v[50,55].1 header files

cnic 1.7a.04.v[50,55,60].1 (Jan. 23, 2014)
====================================
   Enhancements
   ------------
   1. Change: Sync'ed with the latest bnx2x-1.7a.06.v[50,55].2 header files
              and HSI and bnx2-2.2.5d header files

   2. Change: Update Copyrights to 2014


cnic 1.7a.03.v[50,55,60].2 (Jan. 15, 2014)
====================================
   Fixes
   -----
   1. Problem: Fix build error for ESX6.0.

      Change:  Take out compiler switch that excludes ESX 6.0
               when using new irq handler definition.

      Impact:  ESX 6.0 only.

   Enhancements
   ------------
   1. Change: Sync'ed with the latest bnx2x-1.7a.06.v[50,55].1 header files
              and HSI

cnic 1.7a.03.v[50,55].1 (Jan. 07, 2014)
==========================
   Enhancements
   ------------
   1. Change: Sync'ed with the latest bnx2x-1.7a.05.v[50,55].1 header files
              and HSI

cnic 1.7a.02.v[50,55].1 (Dec. 20, 2013)
====================================
   Enhancements
   ------------
   1. Corrected driver version to allow future upgrades to occur.

   2. Change: Changes to match the new 5709 6.2.1.c firmware to flush the
              iSCSI OOO ring.

      Impact: 5709 iSCSI.

cnic 1.710.01.v[50,55].1 (Oct. 10, 2013)
====================================
   Enhancements
   ------------
   1. Branched for T7.10

cnic 1.78.75.v[50,55].1 (Oct. 4, 2013)
====================================
   Enhancements
   ------------
   1. Branched for T7.8c

cnic 1.78.53.v[50,55].2 (Sept 26, 2013)
==========================
   Enhancement
   -----
   1. Change: Sync'ed with the latest bnx2x-1.78.56.v[50,55].2 header files
              and HSI

   2. Change:  Compiled against ESX 5.5 Build 1331820.

      Impact:  ESX5.5 only

cnic 1.78.53.v[50,55].1 (Sept 23, 2013)
==========================
   Enhancements
   ------------
   1. Change: Clean up CNIC RELEASE.TXT

   2. Change: Sync'ed with the latest bnx2x-1.78.56.v[50,55].1 header files
              and HSI

cnic 1.78.52.v[50,55].2 (Sept 13, 2013)
==========================
   Enhancements
   ------------
   1. Change: Sync'ed with the latest bnx2x-1.78.55.v[50,55].1 header files
              and HSI

cnic 1.78.52.v[50,55].1 (Sept 10, 2013)
==========================
   Enhancement
   -----
   1. Change: Re-structured code to use common bnx2x macros for Chip ID,
              port ID, pfid.

      Impact: iSCSI and FCoE on all bnx2x devices.

   2. Change:  Compiled against ESX 5.5 Build 1302513.

      Impact:  ESX5.5 only


cnic 1.78.51.v[50,55].1 (Aug 27, 2013)
==========================
   Fixes
   -----
   1. Problem: (CQ70631) Update the VMWARE_ESX_DDK_VERSION with
               correct ESX5.5 version.

      Change:  In the cnic.sc file the VMWARE_ESX_DDK_VERSION is
               now set correctly for ESX5.5

      Impact:  ESX only.

   Enhancements
   ------------
   1. Change: Sync'ed with the latest bnx2x-1.78.52.v[50,55].1 header files
              and HSI


cnic 1.78.50.v[50,55].2 (Aug 13, 2013)
==========================
   Enhancements
   ------------
   1. Change: Sync'ed with the latest bnx2x-1.78.51.v[50,55].1 header files
              and HSI

   2. Change:  Compiled against ESX 5.5 Build 1260114.

      Impact:  ESX5.5 only

cnic 1.78.50.v[50,55].1 (Aug 1, 2013)
====================================
   Enhancements
   ------------
   1. Branched to T7.8a

cnic 1.78.12.v[50,55].1 (July 23, 2013)  
=============================
   Fixes
   -----
   1. Problem: System hangs when attempting iSCSI connections on 57711E.

      Cause: iSCSI license changes from supported to unsupported between
             bnx2x probe and bnx2x open.  bnx2i is unaware that the device
             does not support iSCSI and attempts to do offload which never
             completes.  The recent change to eliminate symbol_get() to
             obtain bnx2x_cnic_probe() exposed the problem.

      Change: Check iSCSI license again during ->drv_register_cnic().  If
              there is no iSCSI license, skip ->ulp_start().

      Impact: iSCSI on these bnx2x devices where the iSCSI license can only be
              fully determined after firmware is loaded.


cnic 1.78.11.v[50,55].5 (July 11, 2013)  
==========================
   Enhancements
   ------------
   1. Change: Sync'ed with the latest bnx2x-1.78.24.v[50,55].1 header files
              and HSI

cnic 1.78.11.v[50,55].4 (July 02, 2013)  
==========================
   Enhancements
   ------------
   1. Change: Sync'ed with the latest bnx2x-1.78.23.v[50,55].1 header files
              and HSI

   2. Change:  Compiled against ESX 5.5 Build 1198610.

      Impact:  ESX5.5 only

cnic 1.78.11.v[50,55].3 (June 28, 2013)  
==========================
   Enhancements
   ------------
   1. Change: Sync'ed with the latest bnx2x-1.78.22.v[50,55].2 header files
              and HSI


cnic 1.78.11.v[50,55].2 (June 27, 2013)  
==========================
   Enhancements
   ------------
   1. Change: Sync'ed with the latest bnx2x-1.78.22 header files
              and HSI


cnic 1.78.11.v[50,55].1 (June 20, 2013)  
==========================
   Fixes
   -----
   1. Problem: (CQ69621) bnx2x ref count not getting updated when
               CNIC driver is unloaded

      Cause:   The ref count for the bnx2/bnx2x is incremented by
               cnic_register when CNIC is loaded but not decremented
               when CNIC is unloaded.

      Change:  When the CNIC is unloaded properly the unregister
               with cnic_register so that the ref count is properly
               decremented.

      Impact:  ESX iSCSI only.

   Enhancements
   ------------
   1. Change:  Compiled against ESX 5.5 Build 1168834

      Impact:  ESX5.5 only

cnic 1.78.10.v[50,55].2 (June 3, 2013)  
==========================
   Enhancements
   ------------
   1. Change: Sync'ed with the latest bnx2x-1.78.20 header files
              and HSI

   2. Change:  Compiled against ESX 5.5 Build 1158824

      Impact:  ESX5.5 only

cnic 1.78.10.v[50,55].1 (May 24, 2013)  
==========================
   Fixes
   -----
   1. Problem: (CQ69177) MTU change causes PSOD at bnx2x_drv_ctl

      Cause:  The OOO handler was falsely triggered to handle OOO tx
               completions even when bnx2x has failed to allocate resources
               for the OOO ring.  This has caused bnx2x to hit a NULL
               ptr dereference.

      Change: Fixed the cnic OOO handler.

      Impact: bnx2x iSCSI only.

   Enhancements
   ------------
   1. Change: Removed unused function declarations:
              bnx2x_cnic_probe(2), and bnx2_cnic_probe(2)
              from cnic_if.h header file

cnic 1.78.09.v[50,55].2 (May 13, 2013)  
==========================
   Enhancements
   ------------
   1. Change: Sync'ed with the latest bnx2x-1.78.18 header files
              and HSI


cnic 1.78.09.v[50,55].1 (Apr. 12, 2013)  
==========================
   Enhancements
   ------------
   1. Change: Sync'ed with the latest bnx2x-1.78.17 header files
              and HSI

   2. Change:  Compiled against ESX 5.5 Build 1108855

      Impact:  ESX5.5 only

cnic 1.78.08.v[50,55].1 (Apr. 12, 2013)  
==========================
   Enhancements
   ------------
   1. Added IPv6 support.

   2. Change: Sync'ed with the latest bnx2x-1.78.16 header files

   3. Change:  Compiled against ESX 5.5 Build 1080575

      Impact:  ESX5.5 only

cnic 1.78.07.v[50,55].1 (Mar. 21, 2013)  
==========================
   Fixes
   -----
   1. Problem: (CQ68009) ESX41: ESX Test Certifcation HeavyIOLoadUnload
                runs forever

      Cause:   Previously, the L2 driver's refernce count was automatically
               incremented when calling vmk_ModuleGetSymbol().  Moving
               to the new method of calling cnic_probe via the private data,
               the module's reference count was not incremented.

      Change:  Properly increment the module reference count for the
               assoicated L2 driver.

      Introduced: cnic-1.76.56

      Impact:  iSCSi 1G and 10G for ESX.

   2. Problem: BDKL152:HWiSCSI: BCM57711 10GigE(1500, 9000) VM=1:
               IOmeter Regressions: Read(64K, 128K) Throughput.

      Cause:   The NetApp target with Qlogic card doesn't like
               TCP window of 0xffc0 and behave oddly.

      Change:  Add workaround to change window scaling factor to 0
               and set TCP window to 0xfff0.

      Impact:  ISCSi offload.

   Enhancements
   ------------
   1. Change:  (CQ67948) Using VMware macro VMKAPI_MODULE_CALL() to make
               inter-module calls      


cnic 1.78.06.v[50,55].2 (Mar. 06, 2013)  
==========================
   Enhancements
   ------------
   1. Change: Sync'ed with the latest bnx2x-1.78.14 header file


cnic 1.78.06.v[50,55].1 (Feb. 25, 2013)  
==========================
   Fixes
   -----
   1. Problem: (CQ67914) ESX41:iSCSI-OOO engine does not appear to be working
                correctly.

      Cause:   CNIC driver is referencing to the wrong BNX2_RX_DESC_CNT value.

      Change:  CNIC driver should use 256 as the correct value for
               BNX2_RX_DESC_CNT.

      Impact:  iSCSi 1G for ESX.

   2. Problem:  CQ67613 - iSCSI HBA's are not seen on the sytem

      Cause:   bnx2x does not export the probe() functions
               so that the CNIC can't find the bnx2x devices

      Change:  Use the Linux upstream method on calling the probe
               function via the probe call in the bnx2x private data 

      Impact:  iSCSI 10G ESX 4.1 only.

   Enhancements
   ------------
   1. Change:  (CQ67948) Using VMware macro VMKAPI_MODULE_CALL() to make
                inter-module calls

   2. Change:  Compiled against ESX 5.5 Build 1023671

      Impact:  ESX5.5 only


cnic 1.78.05.v[50,55].2 (Feb. 13, 2013)  
==========================
   Enhancements
   ------------
   1. Change: Sync'ed with the latest bnx2x-1.78.11 header file


cnic 1.78.05.v50.1 (Feb. 5, 2013)  
==========================
   1. Problem: CQ67270 - ESX51:iscsi: with Delayed ack enabled
               (by default), initiator is acking one packet at a time.

       Cause:  The 10G firmware added a new way to set the TCP
               delayed ACK setting in the ram I/O but introduced
               a bug in the old way which utilizes connection
               buffers
       Change: Migrated the TCP delayed ACK setting to use the
               ram I/O instead
       Impact: 10G

   2. Problem: CQ67220 - bnx2x firmware assert during "Random TCP errors" test.

      Cause:   Firmware bug and cnic error handling bug for TCP_CLOSE ramrod.

      Change:  Added check for iscsi completion error when receiving the
               TCP_CLOSE ramrod completion.

      Impact:  bnx2x iSCSI only.


cnic 1.78.04.v50.5 (Jan. 14, 2013)  
==========================
   Enhancements
   ------------
   1. Change: Sync'ed with the latest bnx2x-1.78.08.v50.1 header file

cnic 1.78.04.v50.4 (Dec. 28, 2012)  
==========================
   Enhancements
   ------------
   1. Change: Sync'ed with the latest bnx2x-1.78.07.v50.1 header file

cnic 1.78.04.v50.3 (Dec. 10, 2012)  
==========================
   Enhancements
   ------------
   1. Change: Sync'ed with the latest bnx2x-1.78.06.v50.1 header file

cnic 1.78.04.v[41,50].2 (Nov. 16, 2012)  
==========================
   Enhancements
   ------------
   1. Change: Sync'ed with the latest bnx2x-1.78.04.v[41,50].1 header file


cnic 1.78.04.v[41,50].1 (Nov. 13, 2012)  
==========================
   Fixes
   -----
    1. Problem: CQ64479 - ESX41-iscsi: bnx2x asserted while running async
               logout test "bnx2x: [bnx2x_attn_int_deasserted1:4143(vmnic7)]
               FATAL HW block attention set1 0x8"

      Cause:   If remote reset is still pending (SRCH_DEL and TERM_OFFLOAD sequence),
               a local close/reset needs to wait for this sequence to complete.
               Otherwise, CFC_DEL can proceed before TERM_OFFLOAD is completed
               and it can cause bnx2x assert.

      Impact: Both 1G/10G device running iSCSi offload.

cnic 1.78.03.v[41,50].2 (Nov. 08, 2012)  
==========================
   Enhancements
   ------------
   1. Change: Sync'ed with the latest bnx2x-1.78.02.v[41,50].2 HSI header file


cnic 1.78.03 (Nov 05, 2012)
==========================
   Fixes
   -----
   1. Problem: (CQ65178) Panic when loading and unloading cnic with bnx2i and
               bnx2fc.

      Cause: The iSCSI EQ does not get reset during cnic init.  When we
             get the first cnic IRQ, the iSCSI EQ index may be non-zero
             in the status block, causing the cnic driver to dereference
             NULL pointer.

      Change: Added code to clear the iSCSI EQ index in the STORM memory.

      Impact: 10G iSCSI.

cnic 1.78.02 (Oct. 29, 2012)
==========================
   Enhancements
   ------------
   1. Change: Added the ability to pass the outer VLAN
              tag(e1hov_tag) from bnx2x to bnx2fc where it can
              be used during VLAN notification

   2. Change: Copy the mf_mode from bnx2x to cnic to allow bnx2fc
              to determine which mf mode the chip is running

   3. Change: Update cnic_eth_dev and  cnic_dev versioning to T7.8


cnic 1.78.01 (Oct. 18, 2012)
==========================
   Enhancements
   ------------
   1. Change: Sync'ed with the latest cnic_if.h header file


cnic 1.74.0x.v[41,50].x (Sept. 10, 2012)  
==========================
   Fixes
   -----
   1. Problem: CQ65538 - [PR924880] CNIC PSOD when running on 
               extreme lossy network.
      
      Cause: Under extreme lossy networking environment, there is
             a chance of race condition between cm_detroy() and
             cnic_handle_bnx2_ooo_tx_event() threads, which could
             cause the same packet descritor get free up more than
             once. The leads to PSOD on ESX memory manager. 

      Change: Both these threads should take lock before access 
              ooo related resources. 

      Impact: Both 1G/10G device running iSCSi offload.

cnic 1.74.03.v[41,50].2 (Sept. 10, 2012)
==========================
   Enhancements
   ------------
   1. Change: Sync'ed with bnx2x-1.74.15 bnx2x_hsi.h header file

cnic 1.74.03 (Sept. 05, 2012)
==========================

   Fixes
   -----
   1. Problem: BDKL146: [PR 919240, 917781] #GP Exception PSOD in
               memcpy called from cnic_submit_bnx2_kwqes PSOD during
               ESX 6.0 boot
     
      Cause:   Under extreme conditions, CNIC cnic.c::cnic_init() thread
               during CNIC module initialization could race against

               bnx2.c::bnx2_change_ring_size()
               bnx2.c::bnx2_self_test()
               bnx2.c::bnx2_reset_task()
               bnx2.c::bnx2_set_coalesce()

               causing memory to be freed unintentionally.

      Change: In this case, CNIC driver should properly take the rtnl_lock
              during the cnic.c:cnic_init() call

      Impact: bnx2 iSCSI, bnx2x iSCSI.

cnic 1.74.02 (Aug. 20, 2012)
==========================
   Enhancements
   ------------
   1. Change: Sync'ed with the latest cnic_if.h header file


cnic 1.74.01 (July 03, 2012)
=============================
   Fixes
   -----
   1. Problem: Kernel panic under iSCSI OOO condition.

      Cause: Bug in cnic when max OOO resource is reached

      Change: Initailized packet descriptor to fix the bug.

      Impact: iSCSI only.


cnic 1.74.00 (June 26, 2012)
=============================
   Fixes
   -----
   1. Problem: (CQ63666) ESX 4.1: cnic driver summary incorrectly
               lists bnx2 driver information

      Change: Updated the cnic bulletin.xml file to refect the correct driver

      Impact: ESX4.1 only.

   2. Problem: (CQ62298 Partial fix) When running in INTA mode, MTU change
               does not work.  iSCSI/FCoE does not resume after MTU change.

      Cause: During mtu change, bnx2x does not know that cnic is no longer
             handling IRQs.

      Change: Added a new flag to let bnx2x know that cnic is no longer
              handling IRQ during reset.

      Impact: bnx2x iSCSI and FCoE.

   3. Problem: (CQ62937) bnx2x asserts during iSCSI test with corrupted
               TCP NOP-IN.

      Cause: Corrupted NOP-IN falls outside of TCP window, causing FW to
             go into OOO mode.  TCP close with outstanding OOO causes
             problem and the close does not complete.

      Change: FW change to return an error in this case and cnic driver
              change to handle this error by proceeding to clean up the
              connection.

      Impact: bnx2x iSCSI.

   4. Problem: CNIC PSOD when servicing OOO_OPCODE_JOIN. 
     
      Cause: Under extreme condition, CNIC driver could run out of ooo 
             blocks.  However, firmware doesn't know that and may request
             OOO block join with a unknown block. 
 
      Change: In this case, CNIC driver should safe guard the block search 
              and drop the invalid block join request. 

      Impact: bnx2x iscsi.

cnic 1.72.50 (May. 1, 2012)
=============================
   Fixes
   -----
   1. Problem: (CQ62298 Partial fix) Fix for CQ62026 in cnic 2.5.9d introduced
               a regression of clearing the CNIC_UP flag before all CIDs have
               been deleted.  The regression is causing warning messges that
               some CIDs have not been deleted.  After fixing this, we're
               still encountering further bnx2x error messages in the INTA
               code path.

      Change: Wait for all CIDs to be deleted before clearing CNIC_UP flag.

      Impact: iSCSI and FCoE on all bnx2x devices.


cnic 1.72.9 (Mar. 30, 2012)
=============================
   Fixes
   -----
   1. Problem: CQ62401: NCSI Get FCoE Capabilities fields are
               incorrect
      Cause:   The driver was not properly setting the 
               capabilities field which is passed to NCSI
      Change:  Properly set values from the FCoE driver
               to the fcoe_capabilities strcuture
               passed to NCSI

cnic 1.72.8 (March 7, 2012)
==========================
   Enhancements
   ------------
   1. Change: Enhanced FCoE driver registration to provide FCoE
              capabilities to bnx2x driver.  Removed
              CNIC_CTL_FCOE_ENHANCED_STATS_CMD and
              CNIC_CTL_FCOE_CAPABILITIES_GET_CMD.

      Impact: Systems with Management support of these features. These
              changes were made to match bnx2x 1.72.07.

   2. Change: (CQ60867) Backed out earlier changes related to this CQ.
              genksyms checksums are based on structure names and type
              names, so the scheme of using an identical structure with
              a different name will not work.

      Impact: None.

cnic 1.72.7 (Feb. 29, 2012)
==========================
   Fixes
   -----
   1. Problem: (CQ61584) bnx2x asserts during middle-box iSCSI tests.

      Cause: Middle-box test corrupts packets and causes iSCSI fw to
             generate 0x4 (NIC_ERR) completion code.  This conflicts
             with new logic that uses NIC_ERR to convey parity error.

      Change: Redefined parity error completion code to be 0x81 for
              L4, iSCSI, and FCoE.

      Impact: FCoE and iSCSI.


cnic 1.72.6 (Jan. 10, 2012)
==========================
   Fixes
   -----
   1. Problem: When there is parity error, it causes disconnect timeout 
               on bnx2i driver and resulted in cid losses. 

      Cause:   cnic didn't set SK_F_HW_ERR when iscsi connection fail to 
               connect due to parity error and resulted in unneccessary
               long disconnect timeout for bnx2i driver.
     
      Change:  cnic set SK_F_HW_ERR flag when encounter connection failure
               due to parity error. 

      Impact:  all 10g devices support iSCSi and error recovery flow. 

cnic 1.72.5 (Jan. 04, 2012)
==========================
   Enhancements
   ------------
   1. Change: Update copyright headers to 2012

   2. Sync'ed the cnic_if.h header file so that the Driver Control Commands
      would be in sync with the Linux and ESX code

      The following commands for NPAR have been updated

      DRV_CTL_START_NPAR_CMD 0x110
      DRV_CTL_STOP_NPAR_CMD 0x111


cnic 1.72.4 (Dec. 22, 2011)
==========================
   Fixes
   -----
   1. Problem: the stats_addr is not getting initialized properly.
	
      Cause:  There is no code to retrieve stats_addr from bnx2x.

      Change: Added code to retreive stats_addr from bnx2x driver.

      Impact: Newly introduced in cnic 1.72.3.

   2. Problem: (CQ60184) cnic parity error recovery fails.

      Cause: SPQ errors during parity error recovery was not propagated to
             L4 and ULP, causing unnecessary long timeouts.

      Change: Added immediate KCQ error completion for L4 and iSCSI kwqes if
              SPQ fails.

      Impact: iSCSI on bnx2x.   
 
cnic 1.72.3 (Dec. 08, 2011)
==========================
   Enhancements
   ------------
   1. Change: Added iSCSI and FCoE driver status and counters support.

      Impact: Systems with Management support of these features.


cnic 1.72.2 (Dec. 01, 2011)
==========================
   Fixes
   -----
   1. Problem: (CQ59828) ESX5.0 GA: Unable to connect to iSCSI target with 
               VNTag enabled on OEM card.

      Cause:   LLH is not getting initialized in vntag mode. 

      Change:  Make sure cnic to ask bnx2x to initialize LLH when configure
               in VNTag mode. 

      Impact:  VNtag capable devices.

cnic 1.72.1 (Nov. 14, 2011)
==========================
   Initial Branch


cnic 1.11.18 (Oct. 19, 2011)
==========================
   Fixes
   -----
   1. Problem: (CQ58986) Bnx2x driver asserted when running MTU change
               test with heavy iSCSi traffic. 
	
      Cause:   There is a race condition where vmk_IscsiTransportGetPmtu
	       could return old PMTU value and causes cnic to program 
               incorrect mss value to iSCSi context. 

      Change:  Make sure cnic always use the MTU value from net device. 

      Impact:  ISCSI only. 
    
cnic 1.11.17 (Sept. 27, 2011)
==========================
   Fixes
   -----
   1. Problem: (CQ58879) Incorrect WWPN/WWNN Prefixes is seen with
               bnx2fc

      Cause:  The WWPN/WWNN from bnx2x extracted from shared memory
              were not stored by CNIC.
             
      Change: WWPN/WWNN bnx2fc can access this information via the
              cnic_dev structure

      Impact: FCoE only.

cnic 1.11.16 (Sept. 1, 2011)
==========================
   Enhancements
   ------------
   1. Change: Integrated VMware Code review comments:
              *  Clean up cnic_netdev_event_esx()

cnic 1.11.15 (Aug. 18, 2011)
==========================
   Enhancements
   ------------
   1. Change: Added versioning to the CNIC ULP structure to help futher
              prevent the mismatching and mixing of cnic/bnx2i/bnx2fc
              drivers.

cnic 1.11.14 (Aug. 5, 2011)
==========================
   Fixes
   -----
   1. Problem: Unable to allocate context memory for bnx2x with the
               following message seen
		[cnic_alloc_bnx2x_context:1162(vmnic10)]blks(1028)
                  > cp->ethdev->ctx_tbl_len(36)

      Cause: The max_fcoe_conn used to determine the context size was
             set to 0xFFFF which is the value given by the driver.
             The value has a special meaning which should set the
             max_fcoe_conn value to BNX2X_FCOE_NUM_CONNECTIONS

      Change: Properly cap the max_fcoe_conn value to 1024.

      Impact: FCoE only.

cnic 1.11.13 (Aug. 3, 2011)
==========================
   Enhancements
   ------------
   1. Change: Added ability to cache the vlan group from the bnx2x driver
              so that this information can be passed to the bnx2fc driver
	      which can use this information to drop non-register VLAN
	      traffic.

cnic 1.11.12 (July 21, 2011)
==========================
   Fixes
   -----
   1. Problem: FCOE_DESTROY_FUNC ramrod not completing, causing timeout
               and OOO cleanup timeout during MTU change.

      Cause: FCOE_DESTROY_FUNC was sent before all FCoE CIDs have been
             deleted.

      Change: Wait for all (2 seconds delayed) FCoE CFC_DELETE ramrods to
              be completed before sending FCOE_DESTROY_FUNC.

      Impact: FCoE only.

cnic 1.11.11 (June 22, 2011)
==========================
   Enhancements
   ------------
   1. Change: Added ability to propagate WWN info up to bnx2fc driver
              Update cnic_eth_dev versioning because of of the WWW info
              proprogation

cnic 1.11.10 (June 9, 2011)
==========================
   Fixes
   -----
   1. Problem: (CQ54938) iSCSI timeout during async logout.

      Cause: TCP reset request may not complete if there is a race with
             firmware receiving a remote RST.

      Change: Added code to handle TCP reset racing with remote RST and
              TCP close racing with remote FIN.

      Impact: iSCSI

   Enhancements
   ------------
   1. Change: Check CFC delete error code during completion.  If it is set,
              do not reuse the CID.  This change is only compatible with
              bnx2x 1.64.30 or newer.

      Impact: iSCSI and FCoE.


cnic 1.11.9 (May 13, 2011)
================================
   Fixes
   -----
   1. Problem: When sytem is going down (reboot, or power off) with
               iSCSI connections, a PSOD is seen.

      Cause:  When system is going down the interface will already be
              down when bnx2x calls cnic_stop() and cnic has to wait
              for all connections to be cleaned up before it returns.
              If it doesn't which is the case a PSOD will be seen

      Change: Remove netif running check in cnic_cm_stop_bnx2x_hw()
              to allow for connections to be cleaned up.

      Impact: iSCSI

   2. Problem: When in non-NPAR mode, an offloaded connection
               to a iSCSI target could not be established or would
               cause the driver to panic.

      Cause:  The NIG was always configured reguardless if in NPAR
              mode or not.

      Change: Only enable the NIG hardware blocks if in NPAR mode.

      Impact: bnx2x iSCSI only.

cnic 1.11.8 (May 06, 2011)
================================
   Enhancements
   ------------
   1. Sync'ed missing code from Linux CNIC driver
         *  Added missing barrier() in cnic_service_bnx2_queues

cnic 1.11.7 (May 3, 2011)
============================
   Fixes
   -----
   1. Problem: cnic may lose interrupts after processing 64 kcq entries.

      Cause: The driver handles a maximum of 64 entries before calling
             the ulp drivers.  If the chip has more entries, the driver
             does not handle the rest but acknowledges the latest
             status block index.

      Change: Changed the logic to keep looping until all kcq entries
              are handled.

      Impact: iSCSI and FCoE on all devices.

cnic 1.11.6 (May 2, 2011)
============================
   Enhancements
   ------------
   1.  Added Inital support for FCoE support

cnic 1.11.5 (Apr 13, 2011)
============================
   Fixes
   -----
   1. Problem: (CQ49586) iSCSI reboot test fails after a few iterations.

      Cause: TCP port 60000 is used every time during boot.  During reset,
             the TCP connection is never terminated so using the same port
             to connect to the target during reboot will not work.

      Change: Added randomization of the first TCP port to use.

      Impact: iSCSI.

cnic 1.11.4 (Apr 07, 2011)
================================
   Enhancements
   ------------
   1. Change: Updated cnic to with with bnx2x 1.70.x
   2. Change: Update version constant for cnic_dev and cnic_eth_dev

cnic 1.11.3 (Apr 04, 2011)
================================
   Fixes
   -----
   1. Problem: When NPAR is enabled, an offloaded connection
               to a iSCSI target could not be established.

      Cause:  The NIG was not configured properly.

      Change: The interface to enable/disable the NIG is now agreed upon
              and the CNIC will explictly call the proper bnx2x driver
              control commands to configure the NIG.


cnic 1.11.2 (Apr 02, 2011)
================================
   Enhancements
   ------------
   1.  Add the proper extern's for the CNIC probe functions
       for the Async and Inbox bnx2x/bnx2 drivers

cnic 1.11.1.v41.1 (Mar 29, 2011)
================================
   Enhancements
   ------------
   1.  Initial port for T7.0 driver set.  Backported changes
       from Linux version cnic-2.4.0b

cnic 1.10.3g.v41.1 (Mar 29, 2011)
================================
   Enhancements
    ------------
   1.  Print cnic_eth_dev structure information from the
       init_bnx2x_cnic() routine for debugging purposes.

cnic 1.10.3f.v41.1 (Mar 24, 2011)
================================
   1. Problem: (CQ48797) When NPAR is enabled, an offloaded connection
               to a iSCSI target could not be established.

      Cause:  The NIG was not configured properly

      Change: The NIC will now explictly call the proper bnx2x driver
              control commands to configure the NIG.

      Impact: 57712 NPAR iSCSI.

   Enhancements
   ------------
   1.  Unify the cnic error printk's using CNIC_INFO() macro.
   2.  Explictly print in the log when iSCSI OOO is being used.

cnic 1.10.3e.v41.1 (Mar 22, 2011)
================================
   Enhancements
   ------------
   1.  Backported debug code from Linux cnic-2.3.5d to dump
            KWQ/KCQ to the logs

cnic 1.10.3d.v41.1 (Mar 19, 2011)
================================
   Enhancements
   ------------
   1.  Updated cnic to utilize cnic_register module for ESX 5.0 Async
       drivers

cnic 1.10.3c.v41.2 (Mar 14, 2011)
================================
   Enhancements
   ------------
   1.  Synced header files from bnx2x-1.64.19 from Linux

cnic 1.10.3c.v41.1 (Mar 07, 2011)
================================
   Enhancements
   ------------
   1.  Re-synced cnic-2.3.5d from Linux

cnic 1.10.3b.v41.1 (Feb 28, 2011)
================================
   Fixes
   -----
   1. Problem: Resync'ed with Linux cnic-2.3.5d to fix the following problem
               (CQ53174) iSCSI detected conn error and ping timeout.

      Cause: Race condition between cnic driver and hardware DMA'ing a
             new status block with new iSCSI events.  The bug was
             introduced when adding FCoE support.

      Change: 1. Add proper memory barrier after reading status block.
              2. After servicing FCoE EQ, we must loop back and check the
                 iSCSI EQ again because we may have a newer status block
                 index that is read after servicing the iSCSI EQ.

      Impact: 57712 iSCSI and FCoE.

   Enhancements
   ------------
   1.  Unify the cnic error printk's using CNIC_ERR() macro


cnic 1.10.3a.v41.1 (Feb 17, 2011)
================================
   Enhancements
   ------------
   1. Updated bnx2x code pathes to use T6.4 HSI

   2. Updated CNIC versioning in cnic_if.h

cnic 1.10.2q.v41.7 (Jan 11, 2011)
================================
   Fixes
   -----
   1. Problem: iSCSI may not work if multi-function is disabled in NPAR NICs.

      Cause: Bug in logic in detecting NPAR mode.

      Change: Offload bit should not be checked if iSCSI MAC address is invalid.

      Impact: iSCSI on 57712 NPAR NIC.

cnic 1.10.2q.v41.6 (Jan 11, 2011)
================================
   Fixes
   -----
   1. Problem: SPQ RAMROD type field does not consistently contain the
               function ID.

      Change: Fixed in cnic_submit_kwqe_16() for HSI 6.0 and above.

      Impact: iSCSI in NPAR mode.


cnic 1.10.2q.v41.5 (Dec 15, 2010)
================================
   Fixes
   -----
   1.  Problem: Even when NPAR is disabled, the NIC will still
                show NPAR mode and the MAC address will be
		ff:ff:ff:ff:ff:ff.

       Cause:   CNIC didn't check if the MAC address is valid.

       Change:  Detect invalid MAC address and use port MAC address
                if function is 0 or 1.

       Impact: 57712 iSCSI.

   2.  Problem: PSOD after multiple MTU changes

       Cause:   CNIC deferenced a NULL context table

       Change:  Have the CNIC driver properly wait until all the iSCSI
                connections have cleaned up.

       Impact: 10G iSCSI only.

cnic 1.10.2q.v41.4 (Dec 14, 2010)
================================
   Fixes
   -----
   1.  Problem: PSOD seen during OOO operations

       Cause:   OOO ring was not properly unlinking the packet
                descriptors

       Change:  During the OOO send routine, the unlinking of the
                packet descriptors are done before memory is freed

cnic 1.10.2q.v41.3 (Dec 7, 2010)
================================
   Fixes
   -----
   1.  Problem: During iSCSI offload with OOO the firmware could panic
                during shutdown

       Cause:   OOO ring was not properly cleaned up

       Change:  Because the iSCSI IRQ is used by both bnx2x and CNIC
                the IRQ is marked shared.

cnic 1.10.2q.v41.3 (Dec 7, 2010)
================================
   Fixes
   -----
   1. Problem: PSOD would occur after OOO was triggered multiple times.

      Cause: The OOO code was not properly cleaning up the packet
             descriptors.

      Change: Properly free the packet descriptors and unlink them when
              they are not in use.

cnic 1.10.2q.v41.2 (Dec 2, 2010)
================================
   Fixes
   -----
   1. Problem: Firmware panic would occur during a change MTU

      Cause: The OOO code was not properly cleaned up.  This is becuase
             the IRQ used to cleanup the OOO ring was not requested.

      Change: Properly allow bnx2x to aquire the CNIC IRQ by marking the
              IRQ shared rather then exclusive.

cnic 1.10.2q.v41.1 (Dec 1, 2010)
================================
   Fixes
   -----
   1. Problem: ESX iSCSI couldn't connect because of a digest error

      Cause: The OOO code was initializing the connection flags
             incorrectly by setting the bits to check the digest.

      Change: Properly set the connection flags, by setting the proper
              OOO bits only.

cnic 1.10.2m.v41.2 (Nov 5, 2010)
=============================
    Enhancements

cnic 1.10.2p.v41.1(Nov 18, 2010)
================================
   Enhancements
   ------------
	1. Added stats counter to visualize iSCSI OOO being executed

cnic 1.10.2o.v41.1(Nov 16, 2010)
==============================
    Enhancements
    ------------
    1.  Request: Add NIC partioning support for iSCSI

        Change:  As requested


cnic 1.10.2n.v41.1 (Nov 9, 2010)
=============================
   Fixes
   -----
   1. Problem: PSOD when during boot with BCM57712 only

      Cause: The producer pointer in the cnic_local structure was
             not properly initialized

      Change: Initialize the proudcer prointer and remove the stale
              code which updated the improper pointer

      Impact: BCM57712 only

cnic 1.10.2m.v41.2 (Nov 5, 2010)
=============================
    Enhancements
    ------------
    1.  Request: Sync'ed with VMware code:
                 1.  Added cnic_registration support
                 2.  Added additionial OOO support macro's functions

        Change:  As requested by VMware

        Impact:  bnx2/bnx2x


cnic 1.10.2j.v41.2 (Aug 2, 2010)
=============================

    Enhancements
    ------------
    1.  Request: Add NIC Partitioning support

        Change:  As requested

        Impact:  bnx2/bnx2x

    2.  Request: Add Initial Support for OOO

        Change:  As requested

        Impact:  bnx2/bnx2x

    3.  Request: Add debug print statement when the connect completion
                 fails

        Change:  As requested

        Impact:  bnx2/bnx2x


bnx2 v2.0.15g.v40.1 (Jul 1, 2010)
=============================

    Enhancements
    ------------
    1.  Request: Port the bnx2-2.0.15g.v40.1 driver to the ESX 4.1 platform

        Change:  As requested

        Impact:  None


bnx2 v2.0.15g (June 10, 2010) cnic 2.2.3g (June 10, 2010)
=========================================================
   Enhancements
   ------------
   1. Change: Added FCoE statistics SPQ command.

      Impact: FCoE.

bnx2 v2.0.15f (June 4, 2010) cnic 2.2.3f (June 4, 2010)
=========================================================
   Fixes
   -----
   1. Problem: (CQ46648) CID leaks while running iLAB 5.12 connection closure
               test.

      Cause: Race condition between bnx2i initiated TCP close and an
             asynchronous RESET_COMP from firmware.

      Change: Re-structured cnic code that handles close, abort, and various
              completion events to ensure all scenarios are accounted for
              with no race conditions.

      Impact: All iSCSI connection termination scenarios.

   Enhancements
   ------------
   1. Change: Added host iSCSI IP address to the cnic_dev structure so that
              bnx2i can report it to sysfs.  This is needed for iSCSI boot
              during pivot_root.

      Impact: iSCSI boot.

bnx2 v2.0.15e (June 3, 2010) cnic 2.2.3d (June 2, 2010)
=========================================================
   Fixes
   -----
   1. Problem: (CQ48133) bnx2 fails to compile on older 2.6 kernels.

      Cause: PCI MSIX attributes not defined in kernel .h files.

      Change: Added compatibility code.

      Impact: None.

bnx2 v2.0.15d (June 2, 2010) cnic 2.2.3d (June 2, 2010)
=========================================================
   Fixes
   -----
   1. Problem: (CQ47942) rmmod hangs if the device has been opened and closed
               more than once.

      Cause: netif_napi_add() called once during every ->open().
             netif_napi_del() is only called once during rmmod.

      Change: Call netif_napi_del() in ->close().

      Impact: None.

bnx2 v2.0.15c (May 21, 2010) cnic 2.2.3c (April 21, 2010)
=========================================================
   Fixes
   -----
   1. Problem: service iscsid restart on 5709 does not work.

      Cause: Not restarting KWQ correctly due to stale context.

      Change: Fixed by correctly zeroing KWQ/KCQ/RX context
              memory.

      Impact: bnx2 iSCSI.

   2. Problem: iSCSI license not read correctly on 57711E in single
               function mode.

      Cause: Bug in reading the mf_cfg block.

      Change: Bug fixed.

      Change: 57711E iSCSI.

   Enhancements
   ------------
   1. Change: Added GRO support.

      Impact: All devices on kernels supporting GRO.

bnx2 v2.0.15b (May 12, 2010) cnic 2.2.3b (April 12, 2010)
=========================================================
   Fixes
   -----
   1. Problem: iSCSI does not work on 57712.

      Cause: License checking always disabled on 57712.

      Change: Added proper checking for 57712 iSCSI license.

      Impact: None.

   2. Problem: (CQ47360) Compile errors on older kernels not supporting
               UIO and latest iSCSI.

      Cause: New cnic driver will only compile on kernels newer than
             2.6.31 and some selected distros that have the backport.

      Change: Makefile changes to compile cnic only on supported kernels.

      Impact: None.

   Enhancements
   ------------
   1. Change: Changed bnx2_cnic_probe() to bnx2_cnic_probe2() so
              that out-of-tree driver componenets will not inter-
              operate with upstream components.  This avoids
              compatibility problems that often lead to kernel
              crashes.

      Impact: Out-of-tree cnic will not operate with upstream
              L2 drivers and vice versa.

   2. Change: Revert the PRS_REG_NIC_MODE change done in 2.0.11h.  Newer
              bnx2x driver (1.60.18+) do not require this setting.

      Impact: None.

bnx2 v2.0.14b (April 28, 2010) cnic 2.2.2b (April 28, 2010)
============================================================
   Enhancements
   ------------
   1. Change: Added compatibility code for RHEL5.4+ kernels.

      Impact: None.

   2. Change: Added VLAN ID to netdev event callback.

      Impact: bnx2i.

bnx2 v2.0.13b (April 22, 2010) cnic 2.2.1c (April 30, 2010)
============================================================
   Enhancements
   ------------
	Add debug code to dump all KWQE's (RAMROD) posted to 5771x chipset.
	This feature can be enabled/disabled using module parameter, by default
	this feature is disabled. Also a exported function is introduced to
	dump 3 pages worth of KCQE's

bnx2 v2.0.13b (April 22, 2010) cnic 2.2.1b (April 22, 2010)
============================================================
   Enhancements
   ------------
   1. Change: cnic has been updated to be similar to the upstream versions
              using UIO with added T6.0 iSCSI support for 10G and other bug
              fixes.

      Impact: iSCSI now requires UIO, new bnx2i, and bnx2x 1.60.16+.

bnx2 v2.0.11j (April 22, 2010) cnic 1.10.2j (April 22, 2010)
============================================================
   Fixes
   -----
   1. Problem: (CQ47298) Does not compile with bnx2x 1.60.16.

      Cause: cnic_if.h has changed.

      Change: Updated code to be compatible with new cnic_if.h.

      Impact: None.

bnx2 v2.0.11i (April 15, 2010) cnic 1.10.2i (April 15, 2010)
============================================================
   Fixes
   -----
   1. Problem: (RHBZ 511368) Driver loses one MSI-X vector after many hours
               of traffic.

      Cause: Chip timing out on write cycle to the MSI-X mask bit, causing
             the unmask operation to be dropped.

      Change: Increase GRC timeout in register 0x8cc.
              (Same fix from 2.0.8e).

      Impact: bnx2x MSI-X mode.

   2. Problem: (RHBZ 554706) scheduling while atomic warning when bonding and
               VLANs are used with cnic loaded.

      Cause: bond_del_vlans_from_slave() holds bond->lock when calling
             ndo_vlan_rx_register().  bnx2 calls bnx2_netif_stop() to
             stop the rx handling while changing the vlgrp.  The call
             also calls bnx2_cnic_stop() which has many sleeping functions.

      Change: Do not stop cnic when VLANs are changed.  Since there is no
              reset during VLAN change, there is no need to stop cnic.
              (Same fix from 2.0.8e).

      Impact: VLAN and iSCSI.

   3. Problem: (CQ46940) Poor small packet performance on 5709.

      Cause: FTQ discards caused by bottlenecks in firmware.

      Change: Upgraded to 5.0.0.j15 MIPS firmware for 5709.
              (Same fix from 2.0.8c)

      Impact: 5709.

   Enhancements
   ------------
   1. Change: Improved rx performance by prefetching next entry's descriptor
              header and SKB.

      Impact: All chips.

   2. Change: Updated cnic interface to support out-of-order processing.  This
              is needed for bnx2x 1.60.15 but the feature is not available in
              cnic yet.

      Impact: None.

bnx2 v2.0.11h (Mar 29, 2010) cnic 1.10.2h (Mar 29, 2010)
========================================================
   Fixes
   -----
   1. Problem: iSCSI not functional with bnx2x 1.60.11.

      Cause: PRS_REG_NIC_MODE set to 1, causing L2 to receive iSCSI traffic.

      Change: Cleared PRS_REG_NIC_MODE.

      Impact: bnx2x iSCSI.

bnx2 v2.0.11g (Mar 17, 2010) cnic 1.10.2g (Mar 17, 2010)
========================================================
   Enhancements
   ------------
   1. Problem: iSCSI not functional on 57712.

      Cause: Bugs and incomplete support of 57712 in cnic driver.

      Change: Fixed and completed 57712 support.

      Impact: iSCSI.

bnx2 v2.0.11f (Mar 15, 2010) cnic 1.10.2f (Mar 15, 2010)
======================================================
   Fixes
   -----
   1. Change: More 6.0.12 firmware HSI changes (bnx2x 1.60.10).

      Impact: bnx2x iSCSI.

bnx2 v2.0.11e (Mar 9, 2010) cnic 1.10.2e (Mar 9, 2010)
======================================================
   Enhancements
   ------------
   1. Change: Updated to 6.0.12 firmware HSI (bnx2x 1.60.10).

      Impact: bnx2x iSCSI.

bnx2 v2.0.11d (Feb 25, 2010) cnic 1.10.2d (Feb 25, 2010)
========================================================
   Enhancements
   ------------
   1. Change: Fixed shared memory base checking for T6.0 bnx2x HSI.

      Impact: bnx2x iSCSI.

   2. Change: Added new igu status block ID to handle iSCSI status
              block acknowledgement in T6.0 HSI.

      Impact: bnx2x iSCSI.

   3. Change: Allow multiple ethtool speed advertisments when using
              newer ethtool 6.

      Impact: ethtool -s.

   Fixes
   -----
   1. Problem: Statistics 64-bit counters may not be accurate after MTU
               change.

      Cause: Bug missing the carry when summing 64-bit counters.

      Change: Fixed the missing carry.

      Impact: statistics.

bnx2 v2.0.11c (Feb 04, 2010) cnic 1.10.2c (Feb 04, 2010)
========================================================
   Enhancements
   ------------
   2. Change: Added 57712 support in cnic driver.

      Impact: None.
 
bnx2 v2.0.11b (Jan 28, 2010) cnic 1.10.2b (Jan 27, 2010)
========================================================
   Enhancements
   ------------
   1. Change: Saved bnx2 statistics block before MTU change, ring change,
              etc.

      Impact: bnx2 statistics.

bnx2 v2.0.10b (Jan 12, 2010) cnic 1.10.1b (Jan 12, 2010)
========================================================
   Enhancements
   ------------
   1. Change: Improved cnic's MTU change/reset logic to fix multiple problems
              in VMWare.

      Impact: iSCSI.

   2. Change: Converted to bnx2x T6.0 HSI.

      Impact: bnx2x iSCSI.
 
bnx2 v2.0.8e (April 13, 2010) cnic 1.9.13b (Dec 16, 2009)
=========================================================
   Fixes
   -----
   1. Problem: (RHBZ 511368) Driver loses one MSI-X vector after many hours
               of traffic.

      Cause: Chip timing out on write cycle to the MSI-X mask bit, causing
             the unmask operation to be dropped.

      Change: Increase GRC timeout in register 0x8cc.

      Impact: bnx2x MSI-X mode.

   2. Problem: (RHBZ 554706) scheduling while atomic warning when bonding and
               VLANs are used with cnic loaded.

      Cause: bond_del_vlans_from_slave() holds bond->lock when calling
             ndo_vlan_rx_register().  bnx2 calls bnx2_netif_stop() to
             stop the rx handling while changing the vlgrp.  The call
             also calls bnx2_cnic_stop() which has many sleeping functions.

      Change: Do not stop cnic when VLANs are changed.  Since there is no
              reset during VLAN change, there is no need to stop cnic.

      Impact: VLAN and iSCSI.

bnx2 v2.0.8d (April 02, 2010) cnic 1.9.13b (Dec 16, 2009)
=========================================================
   Enhancements
   ------------
   1. Change: Improved rx performance by prefetching next entry's descriptor
              header and SKB.

      Impact: All chips.

bnx2 v2.0.8c (Mar 31, 2010) cnic 1.9.13b (Dec 16, 2009)
=======================================================
   Fixes
   -----
   1. Problem: (CQ46940) Poor small packet performance on 5709.

      Cause: FTQ discards caused by bottlenecks in firmware.

      Change: Upgraded to 5.0.0.j15 MIPS firmware for 5709.

      Impact: 5709.

bnx2 v2.0.8b (Dec 16, 2009) cnic 1.9.13b (Dec 16, 2009)
=======================================================
   Fixes
   -----
   1. Problem: (CQ44964) RHEL5.4 crashes when bnx2 driver is updated with
               out-of-tree version.

      Cause: Newer out-of-tree driver's cnic_eth_dev structure has been
             updated, making it incompatible with RHEL5.4's cnic driver.

      Change: Reverted the structure update for RHEL5.4.

      Impact: None.

   Enhancements
   ------------
   1. Change: Improved the reset logic to prevent NETDEV WATCHDOG when
              TSS is enabled.

      Impact: MTU change, ring size change, selftest, etc.

   2. Change: Fixed some compiler warnings when compiling bnx2 and cnic
              drivers.

      Impact: None.

bnx2 v2.0.7b (Dec 7, 2009) cnic 1.9.12b (Dec 7, 2009)
=======================================================
   Fixes
   -----
   1. Problem: (CQ44620) Spurious KCQ entries leading to bnx2x assert.

      Cause: Stale status block with old KCQ index after restarting hardware.

      Change: Added some additional cleanup and initialization steps including
              zeroing the status block.

      Impact: None.

   Enhancements
   ------------
   1. Change: Updated RV2P P1 for 5709 to 5.0.0.j10 to address a flow control
              issue that can lead to context corruption.  Flow control
              watermarks have also been optimized.

      Impact: 5709 flow control.

bnx2 v2.0.6b (Dec 4, 2009) cnic 1.9.11b (Nov 19, 2009)
=======================================================
   Fixes
   -----
   1. Problem: (CQ44801) Unable to compile bnx2 on most 2.6 kernels.

      Cause: print_mac() kernel compatibility not defined correctly.

      Fix: Simple compatibility fix.

      Impact: None.

bnx2 v2.0.5b (Dec 4, 2009) cnic 1.9.11b (Nov 19, 2009)
=======================================================
   Enhancements
   ------------
   1. Change: Sync'ed up with latest upstream bnx2 driver.  Please see
              ChangeLog for details.

      Impact: Yes, Linux and VMWare.

bnx2 v1.9.42b (Dec 1, 2009)
=======================================================
   Fixes
   -----
   1. Problem: Compile error against the VMware ESX 4.0 DDK

      Cause: vmk_IscsiNetHandle is not defined with the
             VMware ESX 4.0 DDK

      Change: Added compile flag

      Impact: None.


   Enhancements
   ------------

   1. Change: Add BMAPILNX ioctl to allow for FW upgrade

      Impact: bnx2 VMware ESX 4.0


bnx2 v1.9.41b (Nov 19, 2009) cnic 1.9.11b (Nov 19, 2009)
=======================================================
   Fixes
   -----
   1. Problem: (CQ44617) Compile error on SLES10 and RHEL4 kernels.

      Cause: bool not defined on older kernels.

      Change: Added compatibility code.

      Impact: None.

   2. Problem: (CQ42096) iSCSI sessions do not recover after running
               selftest/ifdown/etc with max sessions connected.

      Cause: cnic_lock mutex has circular dependency, causing deadlock
             when iscsid tries to cleanup connections.

      Change: Merged in upstream cnic patches to avoid circular
              dependency.

      Impact: None.

   Enhancements
   ------------
      Change: (CQ43088) Changed the firmware version string format.

      Impact: None.

bnx2 v1.9.40b (Nov 18, 2009) cnic 1.9.10b (Nov 12, 2009)
=======================================================
   Fixes
   -----
   1. Problem: (CQ44528) Kernel runs out of memory after load/unload bnx2.

      Cause: RX SKB buffers were not freed.

      Change: Fixed the regression introduced by VMWare development.

      Impact: None.

   2. Problem: (CQ44399) iLAB 5.10 connection establishment test failure.

      Cause: Firmware SYN-ACK handling issue.

      Change: Updated firmware to 5.0.0.j6 in bnx2_fw.h and 5.0.0.j9 in
              bnx2_fw2.h. 

      Impact: iSCSI.

   Enhancements
   ------------
      Change: (CQ43088) Added VPD-R V0 firmware version string to ethtool -i.

      Impact: None.

bnx2 v1.9.39b (Nov 6, 2009) cnic 1.9.10b (Nov 12, 2009)
=======================================================
   Fixes
   -----
   1. Problem: (CQ44470) Kernel panics when bnx2/bnx2x is unloaded with
               active iSCSI sessions.

      Cause: NETDEV_UNREGISTER will cause bcm570x_* transport to be
             destroyed while sessions may still be active.

      Change: Use module referencing to prevent bnx2/bnx2x from unloading.
              This is a simple interim solution to revert back to the
              old behavior.  In T6.0, we will migrate to the upstream
              driver architecture and network drivers will be able to be
              unloaded again.

      Impact: None.

   Enhancements
   ------------
      Change: Added a short register dump during NETDEV_WATCHDOG.

      Impact: None.

bnx2 v1.9.38b (Nov 6, 2009) cnic 1.9.9b (Nov 6, 2009)
=====================================================
   Fixes
   -----
   1. Problem: (CQ44446) cnic panics during 10G iSCSI initialization.

      Cause: Recent interface changes introduced this regression.
             cnic_service_bnx2x() panics when accessing uninitialized
             status block pointer.

      Change: Added state checking in cnic_service_bnx2x().

      Impact: None.

   2. Problem: (CQ44439) bnx2 does not compile on older 2.6 kernels.

      Cause: mutex not defined on older kernels.

      Change: Use rtnl_lock() to protect bnx2_reset_task().

      Impact: None.

bnx2 v1.9.37b (Nov 4, 2009) cnic 1.9.8b (Nov 3, 2009)
=====================================================
   Enhancements
   ------------

   1. Change: Updated 5708/5706 firmware to 5.0.0.j5 for better small packet
              performance.

      Impact: 5706/5708.

   Fixes
   -----
   1. Problem: (CQ43280) Cannot unload cnic after bnx2/bnx2x is loaded.

      Cause: module referencing.

      Change: Changed module referencing scheme.

      Impact: None.

bnx2 v1.9.36b (Oct 22, 2009)
=======================================================
   Enhancements
   ------------

   1. Change: Expand on NetQueue module parameters.

      Impact: bnx2 VMware NetQ.

bnx2 v1.9.35b (Oct 22, 2009)
=======================================================
   Fixes
   -----
   1. Problem: If only 1 queue is used on VMware ESX, iSCSI
               offload would fail.

      Cause: The inboxed VMware driver would only use
             1 MSI-X vector.  Because of this the driver
             would not setup MSI-X

      Change: Always setup MSI-X reguardless of the
              number of MSI-X vectors used.

      Impact: 5709 iSCSI on VMware

bnx2 v1.9.34b (Oct 20, 2009)
=======================================================
   Fixes
   -----
   1. Change: Updated xinan firmware to 5.0.0.j8
              Nop timeout tuning (VMware PR467194)
              Added a new data fw heartbeat to work with
              the new bootcode and also handle older
              bootcode.

      Impact: 5709.

bnx2 v1.9.33b (Oct 8, 2009)
=======================================================
   Enhancements
   ------------

   1. Change: Make NetQueue module parameters more explict.

      Impact: bnx2 VMware NetQ.

bnx2 v1.9.32b (Oct 8, 2009) cnic v1.9.7c (Oct 8, 2009)
=======================================================
   Fixes
   -----
   1. Problem: CNIC unable to handle an unsolicited
               RESET COMPLETE which would result in a hung
               session.

      Cause: The CNIC driver couldn't handle unexpected SYN.

      Change: The CNIC driver will now handle an unsolicited
              RESET COMPLETE and cleanup properly.

      Impact: cnic

   Enhancements
   ------------

   1. Change: Allow the default NetQueue options to be
              controlled through the macro,
              BNX2_ENABLE_NETQUEUE.

      Impact: bnx2 VMware NetQ.

bnx2 v1.9.31b (Oct 6, 2009)
=======================================================
   Fixes
   -----
   1. Problem: PSOD would occur when alloc()'ing NetQueue's

      Cause: With the removal of the global 'disable_netq' 
             parameters, the NetQueue CID's weren't being
             mapped in some cases

      Change: Always map the NetQueue CID's

      Impact: bnx2 VMware ESX NetQueue

bnx2 v1.9.30b (Oct 5, 2009)
=======================================================
   Fixes
   -----
   1. Problem: PSOD would occur because of TX timeouts

      Cause: The VMware netdev watchdog timer was ran before
             the reset task got a chance to run on a loaded
             system. 

      Change: Elongated the TX timeout value for VMware ESX
              only to allow for the reset task to run.

      Impact: bnx2 VMware ESX


   Enhancements
   ------------

   1. Change: Updated vmkernel module parameter, 'force_netq',
              to allow NetQueue setting to be adjusted per
              function rather then globally for all functions.

      Impact: bnx2 VMware ESX


bnx2 v1.9.29b (Oct 1, 2009)
=======================================================
   Fixes
   -----
   1. Change: Updated xinan firmware to 5.0.0.j7 and
              teton firmware to 5.0.0.j4 which will fix
              L2 hang due to iSCSI PDU's padding byte
              extended to another TCP segment

      Impact: 5706/5708/5709.


bnx2 v1.9.28b (Sep 25, 2009)
=======================================================
   Fixes
   -----
   1. Change: Updated firmware to 5.0.0.j6 which will add
              the corresponding flow control trip point.

      Impact: 5709.


bnx2 v1.9.27b (Sep 24, 2009) cnic v1.9.7b (Sep 24, 2009)
=======================================================
   Fixes
   -----
   1. Problem: For the cnic users would see in the kernel logs:

               "kcq abs(hw_prod(0) - sw_prod(65534)) >
                MAX_KCQ_IDX(2047)"

      Cause: The function was not taking into account the
             wrapping of the software and hardware producer
             indexes.

      Change: Recaculate the difference between the index with
              wrapping taken into account.

      Impact: cnic


   Enhancements
   ------------

   1. Change: Updated firmware to 5.0.0.j5 which increased the
              rxpq depth from 32 to 256 to enhance the performance 
              on systems without flow control.

      Impact: 5709.


bnx2 v1.9.26c (Sep 17, 2009)
=======================================================
   Enhancements
   ------------
   1. Change: Cleanup the VMware NetQueue code.  Eliminate unneeded
              RX flush routine, fix the number of queues to be the
              same on 1500 and 9000 MTU sized packets.

      Impact: bnx2 VMware NetQ.

bnx2 v1.9.26b (Sep 14, 2009)
=======================================================
   Fixes
   -----
   1. Problem: VMware PSOD on MTU change

      Cause: MSI-X window was remapped to the beginning of the PCI
             config space.  The driver would disable the bar space
             because the MSI-X window was remapped incorrectly.  This
             would eventually cause a PSOD.

      Change: Before the chip reset, the driver would disable MSI-X,
              after the chip reset, MSI-X is re-enabled.

      Impact: VMware NetQueue


bnx2 v1.9.25b (Aug 21, 2009) cnic v1.9.6 (Aug 21, 2009)
=======================================================
   Fixes
   -----
   1. Problem: (CQ 43182/43252) Compile error on RHEL4

      Cause: struct mutex not defined on older kernels.

      Change: Wrap cnic_lock mutex structure and code with #ifdef BCM_CNIC.

      Impact: None.

   2. Problem: Unloading cnic after ifdown may crash.

      Cause: cnic unregisters with bnx2/bnx2x twice.

      Change: Fixed logic to unregister only once.

      Impact: None.

bnx2 v1.9.24b (Aug 13, 2009) cnic v1.9.6 (Aug 13, 2009)
=======================================================
   Fixes
   -----
   1. Problem: (CQ 42778) Kernel occasionally panics when enabling jumbo
               frames.

      Cause: If the driver is unable to allocate memory for the buffers,
             the device is not properly shutdown.

      Change: Added logic to shutdown device if unable to allocate buffers
              and complete the setup of the device.

      Impact: bnx2, changing MTU and ring sizes.

   Enhancements
   ------------
   1. Change: Updated firmware to 5.0.0.j3 for better small packet rx
              performance.  Firmware also fixes header digest error during
              I/O.

      Impact: All bnx2 devices.

bnx2 v1.9.23b (July 29, 2009) cnic v1.9.5 (July 29, 2009)
==========================================================

   Fixes
   -----
   1. Problem: (CQ 42723) KCQ not resetting to 0 problem

      Cause:   RCU deadlock during shutdown

      Change:  Move the bnx2_register_cnic() call out of the
               above sequence. Instead, register and
               unregister during NETDEV_UP/NETDEV_DOWN events.

               Change all slow path RCU read locks to mutex.
               In cnic, we also use reference counting to
               protect some slow paths.

      Impact: bnx2 iSCSI, bnx2x iSCSI


bnx2 v1.9.22b (July 23, 2009) cnic v1.9.4 (July 23, 2009)
==========================================================

   Enhancements
   ------------
   1. Change: If a TX timeout occurs, there could be the possiblity that the
              chip is hung. By printing chip state into the kernel ring buffer,
              it will be easier to determine this.

      Impact: bnx2 iSCSI.

   2. Change: The bnx2 firmware should always be matched with the proper bnx2
              driver. The bnx2 firmware version string are now printed.
              It will be easier to identify the running firmware.

      Impact: bnx2

   3. Change: When a TX timeout occurs and the chip is reset, the ability to
              debug the chip further is lost.  This is because the chip state
              information is lost during the reset.  The users have a choice
              to prevent the chip reset.

      Impact: bnx2

   4. Change: Add a check to see if there was a KCQ overflow was
              in the bnx2x firmware.  Now this check has been moved to the
              CNIC so that the driver could control the cleanup/recovery.
              
      Impact: bnx2 iSCSI.


bnx2 v1.9.21b (July 16, 2009)
==========================================================
   Enhancements
   ------------
   1. Change: Updated firmware to 5.0.0.j2  to fix remote reset problem

      Impact: bnx2 iSCSI.


bnx2 v1.9.20b (July 09, 2009), cnic v1.9.3 (July 09, 2009)
==========================================================
   Fixes
   -----
   1. Problem: (CQ42534) cnic.c does not compile on older kernels.

      Cause:   Some iscsi_proto constants not defined in <scsi/iscsi_proto.h>

      Change:  Added the constant definitions if not already defined.

      Impact: None.

   Enhancements
   ------------
   1. Change: Updated firmware to 5.0.0.j to fix TMF releated iSCSI issues.

      Impact: bnx2 iSCSI.

bnx2 v1.9.19b (July 01, 2009), cnic v1.9.2 (July 01, 2009)
==========================================================
   Fixes
   -----
   1. Problem: (CQ42399) 10G iSCSI fails when initiator and target MTUs
               don't match.

      Cause: cnic driver sets the MSS without knowing the actual MSS
             option and timestamp option during TCP connection.

      Change: Changed driver to set MSS to 0xffff so that firmware can
              calculate MSS on its own.

      Impact: bnx2x iSCSI.

   2. Problem: 1G iSCSI fails when initiator and target MTUs don't
               match and timestamp is enabled.

      Cause: Firmware was not adjusting for the 12-byte timestamp option
             if MSS was reduced by MSS option.

      Change Updated firmware to 5.0.0.i

      Impact: bnx2 iSCSI.

   3. Problem: (CQ42353) Unable to disable TCP timestamp on 10G iSCSI.

      Cause: Timestamp was hardcoded to be enabled for 10G.

      Change: Update global timestamp option during each TCP connection.

      Impact: bnx2x iSCSI.

   4. Problem: (CQ42329) bnx2x MC assert during IPv6 login/logout.

      Cause: EQ filled with more than 128 L4 kcqes without MSI-X interrupt
             for 2 seconds.  The driver can only buffer 128 L4 kcqes.

      Change: Increased L4 kcqe buffer to 256 entries as a temporary solution.
              Need to understand the delayed interrupt issue.

      Impact: None.

bnx2 v1.9.18b (June 25, 2009), cnic v1.9.1 (June 24, 2009)
==========================================================
   Enhancements
   ------------
   1. Change: Added FTQDiscard counter to the list of counters being
              reported.  During small packet test, there may be FTQ
              overflow and this counter is very useful.

      Impact: None.

   2. Change: Updated firmware to 5.0.0.h to improve small packet L2
              performance and to enhance iSCSI TMF handling.

      Impact: 5706/5708/5709.

bnx2 v1.9.17b (June 24, 2009), cnic v1.9.1 (June 24, 2009)
==========================================
   Fixes
   -----
   1. Problem: Leaking NetQueues if the firmware did not respond in time

      Cause: System might be clogged and there is not enough time to 
             process the KCQ

      Change: Updated driver/firmware to allow the calling of the free RX
              queue request before a RX alloc request is issued

      Impact: 5709

   2. Problem: An offloaded iSCSI connection would get stuck

      Cause: Issing an offload request might fail, and this was not handled
             properly.

      Change: Updated driver/firmware to return the proper return code and
              handle offload connection failures.

      Impact: 5706/5708/5709

   3. Problem: tasklet_init() is being called on a task that is scheduled

      Cause: When the CNIC calls register_device(), that task might already
             be schedled.

      Change: tasklet_disable() is insufficient because the tasklet remains
              scheduled and stays on the tasklet list, instead tasklet_kill() 
              is now used.

      Impact: 5706/5708/5709



bnx2 v1.9.16b (June 10, 2009), cnic v1.9.0 (June 10, 2009)
==========================================================
   Enhancements
   ------------
   1. Change: (CQ38228) Use symbol_get() for ipv6 symbols so that the
              cnic driver will load without necessarily loading ipv6
              modules.

      Impact: iSCSI over IPv6.

   2. Change: Updated 5706/08/09 MIPS firmware to 5.0.0.g.

      Impact: 5706/08/09.

   3. Change: Backported some dma_mapping_error() checking.

      Impact: None.

bnx2 v1.9.15b (June 1, 2009), cnic v1.8.6 (June 1, 2009)
========================================================
   Enhancements
   ------------
   1. Change: Upstream bnx2 tx path optimizations.  Please see ChangeLog.

      Impact: bnx2 tx path.

   2. Change: In the cnic driver, save the last allocated TCP port during
              unregistration so that previously used TCP ports will not
              be immediately re-used.

      Impact: iSCSI.

   3. Change: VMWare TCP port allocation changes.

      Impact: VMWare iSCSI.

bnx2 v1.9.14b (May 21, 2009)
==========================================
   Fixes
   -----
   1. Problem: NOPOUT timeouts on 570x iSCSI connections.

      Cause: Bugs in TCP timestamp implementation.

      Change: Updated MIPS firmware to 5.0.0.f.

      Impact: 5706/5708/5709.

bnx2 v1.9.13b (May 18, 2009)
==========================================
   Fixes
   -----
   1. Problem: Potentially exceeding the NetQueue limit recommendations
               by VMware which could stress system resources

      Cause:  When system resources are strained.

      Change: There are now limits on the number of NetQueues which the
              driver will request:
              When the MTU is 1500 the max number of queues per port is 8
              When the MTU is 9000 the max number of queues per port is 4

      Impact: NetQueue enabled version of VMware ESX

   2. Problem: Getting conflicting NetQueue and iSCSI completions

      Cause:  When MSI-X is not used on a 5709, NetQueue is still enabled

      Change: NetQueue is not disabled is MSI-X is not used.

      Impact: NetQueue enabled version of VMware ESX


bnx2 v1.9.12b (May 13, 2009)
==========================================
   Fixes
   -----
   1. Problem: Potentially returning a negative number of NetQueues

      Cause: When calculating the number of rings, we use the calculation from
             the number of msi-x vectors returned,  The number of NetQueues
             returned could potentially be negitive if only 1 vector was
             returned.  This is because the driver was subtracting 2
             instead of subtracting 1 (for the default queue) from the total
             number of rings.

      Change: Return the proper number of queues not including the default
              queue.

      Impact: NetQueue enabled version of VMware ESX

bnx2 v1.9.11b (May 12, 2009), cnic v1.8.5 (May 13, 2009)
========================================================
   Fixes
   -----
   1. Problem: TCP Delay ACK not working on bnx2x iSCSI

      Cause: Disabled in cnic driver.

      Change: Fixed csk->tcp_flags definitions and enabled the proper storm
              bit for delay ACK.

      Impact: bnx2x iSCSI.

bnx2 v1.9.11b (May 12, 2009)
==========================================
   Fixes
   -----
   1. Problem: iSCSI timestamp TCP option not working.

      Cause: Disabled in firmware.

      Change: Updated to 5.0.0e MIPS firmware.

      Impact: 5709.

bnx2 v1.9.10b, cnic v1.8.4 (May 11, 2009)
==========================================
   Fixes
   -----
   1. Problem: NetQ and iSCSI do not work in Vmware environment.

      Cause: 1. cnic driver is overwriting CP and COM mailbox bit values newly
                defined to support multiple kcqs.

             2. Firmware is completing some iSCSI kcqes on the NetQ's kcq.

      Change: Fixed cnic driver to only set and clear bit 0 of the CP
              and COM mailbox.

              Firmware has been updated to 5.0.0d. This firmware also
              supports TCP timestamp option for iSCSI connections.

      Impact: 5706/5708/5709 iSCSI, NetQ.

bnx2 v1.9.9b (May 1, 2009)
==========================================
   Fixes
   -----
   1. Problem: There is link, but can't pass traffic on ESXi

      Cause: Bits in the RX context are being trampled during the
             renegotiation of the link.

      Change:  RX context offset 0x6 should only be initialized once
               during init and not be updated during run-time.  Offset
               4 contains the BIDX that's mapped to the mailbox.

      Impact: VMware with NetQueue

bnx2 v1.9.8b, cnic v1.8.2 (April 27, 2009)
==========================================
   Enhancements
   ------------
   1. Change: Updated cnic driver to support 1.50.x HSI as well as the older
              1.48.107 HSI.  A compile flag will be used to select one or the
              other.

      Impact: iSCSI on bnx2x.

   2. Change: Spec file and Makefile changes detect the proper module
              install directory.

      Impact: installation.

bnx2 v1.9.7b, cnic v1.8.1 (April 22, 2009)
==========================================
   Fixes
   -----
   1. Problem: Compile error with redfinition of struct kwqe.

      Cause: Both the CNIC and bnx2 defined this structure.

      Change: Because the bnx2 definition is L2 specific, it was renamed to
              struct l2_kwqe.

      Impact: None.

   2. Problem: Add context memory DMA alignment for 57710.

      Cause: For the 57710 context memory needs to be 16k aligned.
             Without this alignment you will see errors when trying to
             establish more then 5 iSCSI connections on VMware ESX 4.0 U1.

      Change: Properly aligned the context memory by allocating a bigger 
              chunk of memory and then finding the proper alignment.
              This reduces the number of possible connections in half
              but now we can properly establish more then 5 connections
              on VMware.

      Impact: iSCSI.


bnx2 v1.9.6b (April 17, 2009)
=============================
   Enhancements
   ------------
   1. Change: Added NetQueue support for VMware.

      Impact: 5709.

bnx2 v1.9.5b (April 17, 2009)
=============================
   Enhancements
   ------------
   1. Change: Updated to 5.0.0.a firmware with NetQ support and iSCSI max
              connection license information. RV2P firmware unchanged:
              4.6.16 for 5706, 4.6.15 for 5709.

      Impact: All chips.

   2. Change: Set USE_INT_PARAM on 5709.  This will switch the chip in
              use "interrupt mode" coalescing after MSI/MSI-X.

      Impact: 5709.

   3. Change: Included 5706 when doing statistics block DMA workaround.

      Impact: 5706.

bnx2 v1.8.8b (March 12, 2009)
=============================
   Enhancements
   ------------
   1. Change: Updated to latest 4.6.17 CP firmware for 5709.

      Impact: iSCSI licensing on 5709.

bnx2 v1.8.7b, cnic v1.7.8 (March 10, 2009)
==========================================
   Enhancements
   ------------
   1. Change: Reverted 5706/5708 firmware to 4.6.16.  Low latency interrupt
              mode does not work on 5706/5708.

      Impact: None.

   2. Change: VMWare changes to expose max. number of iSCSI connections in
              the cnic_device structure.

      Impact: VMware iSCSI.

   Fixes
   -----
   1. Problem: (CQ39867) Compile error on RHEL5.3 Xen kernel.

      Cause: msi related symbols undefined because CONFIG_PCI_MSI is not
             enabled on Xen kernels.

      Change: Added CONFIG_PCI_MSI around the msi related code.

      Impact: None.

   2. Problem: (CQ39818) iSCSI targets do not reconnect after running self test.

      Cause: Interrupt is disabled by bnx2 before notifying CNIC to clean up
             and stop.  As a result, bnx2i will not receive interrupts when
             closing the connections if sharing INTA/MSI with network.

      Change: Disable interrupt after notifying CNIC to stop.

      Impact: iSCSI.

bnx2 v1.8.6b, cnic v1.7.7 (March 2, 2009)
=========================================
   Enhancements
   ------------
   1. Change: Updated to new 5706 firmware (4.6.17) and 5709 firmware (4.6.16).
              New interrupt coalescing mode for improved latency and iSCSI
              cache line fix on 5709.

      Impact: All bnx2 chips.

   2. Change: CNIC iSCSI changes for VMWare.

      Impact: VMWare only.

bnx2 v1.8.5b, cnic v1.7.6 (Feb 9, 2009)
=======================================
   Fixes
   -----
   1. Problem: (CQ39380) bnx2x iSCSI license not read correctly.

      Cause: Using wrong variable to check the license.

      Change: Fixed the logic.

      Impact: bnx2x iSCSI.

   2. Problem: Driver accesing MMIO registers during VLAN operations when
               the device is in D3hot state in older kernels.

      Cause: VLAN registration functions do not check for device state.

      Change: Added if_running check before MMIO access in VLAN registration
              functions.

      Impact: VLAN operations on all bnx2 chips.

   Enhancements
   -----------
   1. Problem: Updated 5706/5708 firmware to 4.6.16.

      Impact: 5706/5708.

bnx2 v1.8.4b, cnic v1.7.5 (Jan 30, 2009)
========================================
   Fixes
   -----
   1. Problem: (CQ39281) Management firmware stops passing traffic when
               bnx2 driver is loaded with jumbo frames enabled.

      Cause: Firmware bug.

      Change: Updated to 4.6.15 firmware.

      Impact: 5706/5708/5709.

   2. Problem: iSCSI does not work on 57711 in single function mode.

      Cause: Driver only allows iSCSI on 57711 if iSCSI is enabled.

      Change: iSCSI config. not required in single function mode.

      Impact: bnx2x iSCSI.

   Enhancements
   ------------
   1. Change: (CQ38576) Add 5709 to bnx2.4 man page.

      Impact: None.

bnx2 v1.8.3b, cnic v1.7.4 (Jan 23, 2009)
========================================
   Fixes
   -----
   1. Problem: (CQ38610, CQ39000, CQ39015, CQ39071, CQ39133) Various Jumbo
               frames related data corruption issues.

      Cause: Bug in RV2P firmware causing jumbo frames to be DMA'ed without
             the frame header control structure occasionally.

      Change: New firmware.

      Impact: 5706/5708/5709.

bnx2 v1.8.2c, cnic v1.7.4 (Dec 30, 2008)
========================================
   Fixes
   -----
   1. Problem: (CQ38955) Xen kernel panic when unloading bnx2 with jumbo MTU.

      Cause: Bug in bnx2_free_rx_mem().  The jumbo page ring memory was
             freed incorrectly using the wrong local variable as array
             index.

      Change: Fixed bug by using the correct variable as array index.

      Impact: Jumbo frames.

   2. Problem: (CQ38965) iSCSI connection timeout on bnx2x.

      Cause: During CFC Delete RAMROD completion handling, the wrong (older)
             iSCSI connection ID can sometimes be retrieved using the
             harware CID.  The CID in the mapping table was not cleared
             after the CID was freed. 

      Fix: Adding clearing of the CID in the data structure after a CID
           is freed.

      Impact: bnx2x iSCSI.

   Enhancements
   ------------
   1. Change: (CQ38744) Reduced R2TQ memory usage to match new firmware
              interface (firmware 4.8.9). This reduces the amount of
              kernel memory substantially for each iSCSI connection on
              bnx2x.

      Impact: bnx2x iSCSI.

bnx2 v1.8.2b, cnic v1.7.3 (Dec 17, 2008)
========================================
   Enhancements
   ------------
   1. Change: Added iSCSI configuration check on 57711E devices before
              allowing iSCSI connections.

      Impact: bnx2x iSCSI.

bnx2 v1.8.2b, cnic v1.7.2 (Nov 25, 2008)
========================================
   Fixes
   -----
   1. Problem: bnx2x iSCSI does not work on functions 2 or above.

      Cause: This was caused by multiple problems:
             a) Status block ID specified by bnx2x was wrong.
             b) MSI-X vector assigned to CNIC was wrong.
             c) New method to ack. status block using HC register was not
                implemented.
             d) Status block ID in CSTORM status block is always 0, and
                as a result, the status block ID used to ack. the status
                block was wrong.

             All these problems only affect functions 2 and above.

     Change: All problems fixed in bnx2x and cnic.

     Impact: bnx2x iSCSI.

bnx2 v1.8.2b, cnic v1.7.1 (Nov 15, 2008)
========================================
   Enhancements
   ------------
   1. Change: Added CNIC support for Multi function bnx2x iSCSI.

      Impact: bnx2x iSCSI.

bnx2 v1.8.2b, cnic v1.6.2 (Nov 12, 2008)
========================================
   Enhancements
   ------------
   1. Change: Updated to latest 4.6.13 5709 firmware to fix context corruption
              with flow control enabled.

      Impact: 5709.

   2. Change: Added support for 5716S PCI ID.

      Impact: None.

   Fixes
   -----
   1. Problem: (CQ35904) Netdump does not work.

      Cause: Problem introduced by MSI-X multiqueue.  IRQ handlers were
             changed to take bnx2_napi parameter instead of netdev parameter.

      Change: Fixed by passing proper parameter to IRQ handler from netpoll.
              All IRQ handlers are called when using multiple MSI-X vectors.

      Impact: 5709 netpoll.

bnx2 v1.8.1f, cnic v1.6.1 (Nov 5, 2008)
========================================
   Fixes
   -----
   1. Problem: All TSO packets corrupted on 5706/5708.

      Cause: Firmware bug zeroing the wrong field in IP header.

      Change: Updated to latest 4.6.11 5706/5708 firmware and 4.6.12 5709
              Firmware.

      Impact: 5706/5708/5709.

   2. Problem: bnx2x chip asserts when trying to make iSCSI connection
               to an unknown IP address.

      Cause: When connection fails, the driver sends a command to an
             unitialized CID.

      Change: Added logic to only send deletion commands to initialized
              CIDs.

      Impact: bnx2x iSCSI.

   Enhancements
   ------------
   1. Change: Added support for one single VLAN to a bnx2x iSCSI interface.

      Impact: bnx2x iSCSI.

bnx2 v1.8.1e, cnic v1.6.0 (Oct 27, 2008)
========================================
   1. Change: Updated to latest 5709 firmware to fix iSCSI data integrity
              problem.

      Impact: 5709.

bnx2 v1.8.1d, cnic v1.6.0 (Oct 23, 2008)
========================================
   Enhancements
   ------------
   1. Change: Updated to latest bnx2 firmware to fix iSCSI data integrity
              problem.

      Impact: 5706/5708/5709.

   2. Change: Updated to the latest bnx2x HSI files.

      Impact: bnx2x iSCSI.

bnx2 v1.8.1c, cnic v1.5.9 (Oct 13, 2008)
========================================
   Fixes
   -----
   1. Problem: (CQ37905) Unable to compile on SLES10 SP2.

      Cause: DIV_ROUND_UP macro not defined in this kernel.

      Change: Added it for compatibility.

      Impact: None.

   Enhancements
   ------------
   1. Change: Updated to latest 5709 firmware that fixes an NCSI problem.

      Impact: 5709.

   2. Change: Handle TCP reset in the middle of TCP close more appropriately.

      Impact: iSCSI.

   3. Change: Handle iSCSI license checking in the same way as 5708/5709.

      Impact: iSCSI on bnx2x.

bnx2 v1.8.1b, cnic v1.5.8 (Oct 13, 2008)
========================================
   Fixes
   -----
   1. Problem: bnx2x iSCSI CIDs may be allocated outside the range of allocated
               host memory.

      Cause: CID range bigger than the amount of allocated host context
             memory.

      Change: Changed to match the CID range with memory range.

      Impact: bnx2x iSCSI.

   Enhancements
   ------------
   1. Change: Sync'ed with the latest upstream driver bnx2 1.8.1.

      Impact: None.

   2. Change: Implemented iSCSI connection license enforcement for bnx2x
              devices.

      Impact: bnx2x iSCSI.

bnx2 v1.8.0j, cnic v1.5.7 (Oct 6, 2008)
========================================
   Fixes
   -----
   1. Problem: (CQ37610) Chip hangs when changing MTU with active iSCSI
               connections.

      Cause: Both cnic and bnx2 drivers setting up the chip at the same
             time.

      Change: Added check so that the register_cnic function will fail
              if the bnx2 driver is in reset.

      Impact: iSCSI.

   2. Problem: (CQ37762) Able to unload bnx2/bnx2x drivers while there are
               active iSCSI connections.

      Cause: CNIC driver does not have a reference count on the BNX2/BNX2X
             drivers.

      Change: This became a problem after the register_cnic function was
              no longer exported.  To solve the problem, the CNIC driver
              will now get an explicit reference during register_cnic.

      Impact: iSCSI.

   3. Problem: (CQ37429) MMIO access while the chip is in D3hot state.

      Cause: The driver does not check if_running state consistently during
             ethtool operations.

      Change: Added proper checks to all ethtool and multicast change
              functions.

      Impact: ethtool operations and multicast operations.

   Enhancements
   ------------
   1. Change: Simplified ipv4 TSO logic in the driver.  This was made
              possible with newer 5708 firmware.

      Impact: 5708 TSO and other traffic.

   2. Change: ethtool -p now blinks forever.  This is the standard behavior
              in most other net drivers.

      Impact: ethtool -p.

bnx2 v1.8.0i, cnic v1.5.5 (Sep 30, 2008)
========================================
   Fixes
   -----
   1. Problem: (CQ36787) iSCSI login/logout commands fail on 5709 after a
               while.

      Cause: Not handling the KWQ completion properly on 5709 in INTA/MSI
             mode.

      Change: Changed to handle KWQ completions by checking the
              cmd_consumer_index instead of the rx_quick_index15.

      Impact: 5709 ISCSI in INTA/MSI mode.

   2. Problem: (CQ37497) CNIC driver does not compile on powerpc.

      Cause: csum_ipv6_magic() not defined.

      Change: Added #include <net/ip6_checksum.h>

      Impact: None.

v1.8.0g (Sep 24, 2008)
========================
   Fixes
   -----
   1. Problem: (CQ37511) System locks up when loading cnic driver on 2.6.16
               kernel.

      Cause: symbol_put_addr() in 2.6.16 tries to acquire the same lock twice.

      Change: Workaround by using __symbol_put() which does not have the same
              problem.

      Impact: None.

v1.8.0f (Sep 23, 2008)
========================
   Fixes
   -----
   1. Problem: (CQ37405) Kernel panic when performing ifup/ifdown with iSCSI
               connections on bnx2x devices.

      Cause: Sending searcher delete to bnx2x devices when connection was
             not established (due to Spanning Tree or other reasons).

      Change: Check PG offload state before sending searcher delete.

      Impact: iSCSI on bnx2x.

v1.8.0e (Sep 22, 2008)
========================
   Enhancement
   -----------
   1. Change: Updated to latest driver firmware 4.6.6 for 5709.

      Impact: 5709.

   2. Change: Updated cnic so that it will not crash even if using older
              bnx2/bnx2x drivers without CNIC support.  The net driver
              can also be loaded after cnic and it will still work without
              crashing.

      Impact: iSCSI.

   3. Change: (CQ 37381) Updated driver to check Vaux PRESET before allowing
              WoL.  This is needed to support 5709 quad-port boards.

      Impact: WoL on all devices.

v1.8.0d (Sep 15, 2008)
========================
   Enhancements
   ------------
   1. Change: Updated CNIC iSCSI setup for bnx2x devices.

      Impact: iSCSI on bnx2x devices.

v1.8.0c (Aug 25, 2008)
========================
   Fixes
   -----
   1. Problem: Does not compile on older kernels.

      Cause: "__maybe_unused" undefined on older kernels.  "num_online_cpus()"
              undefined on 2.4 kernels.

      Change: Added compatibility code to workaround.

      Impact: None.

v1.8.0b (Aug 25, 2008)
========================
   Enhancement
   -----------
   1. Change: Updated to latest driver firmware 4.6.2 for 5709.

      Impact: 5709.

v1.7.9c (Aug 5, 2008)
========================
   Fixes
   -----
   1. Problem: bnx2 does not compile on older kernels.

      Cause: <linux/log2.h> is missing on 2.6.19 and older kernels.

      Change: Added compatibility code to check for kernel version before
              including the file.

      Impact: none.

v1.7.9b (Aug 5, 2008)
========================
   Enhancements
   ------------
   1. Change: Added multi-tx ring for 5709.  This fetaure is available on
              2.6.27 kernel when using MSI-X.

      Impact: 5709

   2. Change: Added support for 57710 iSCSI in the CNIC driver.

      Impact: iSCSI.

v1.7.7c (July 14, 2008)
========================
   Fixes
   -----
   1. Problem: Source RPM fails to build.

      Cause: New file missing in tarball.

      Change: Added missing file.

      Impact: None.

v1.7.7b (July 9, 2008)
========================
   Enhancements
   ------------
   1. Change:  Added probe function so that the CNIC driver can get the
               pci_device pointer earlier before registration.

      Impact:  iSCSI.

   2. Change:  Added support for 5716.

      Impact:  None.

v1.7.6c (June 6, 2008)
========================
   Enhancements
   ------------
   1. Change:  Added multi-ring RX support on 5709 using MSI-X.  This feature
               is only available on 2.6.24 and newer kernels running on SMP
               machines.

      Impact:  5709.

   2. Change:  Added secondary unicast address support.  We now support up
               to 5 unicast addresses.  This feature is only available on
               2.6.23 and newer kernels.

      Impact:  All chips.

v1.7.6b.1 (Aug 14, 2008)
========================
   Fixes
   -----
   1. Problem: (CQ36808) VLAN tagged packets received by host stack without
               the VLAN tag.

      Cause: If no VLANs are set up using vconfig, and if the driver
             configures the chip to strip the VLAN tag, the problem can
             happen.  With IPMI or UMP enabled, the driver is likely to
             configure the chip to strip the VLAN tag.

      Change: Modified the driver to re-insert the VLAN tag when necessary.
              I.e. when IPMI/UMP is enabled and vconfig has not setup any
              VLANs.

      Impact: All chips receiving VLAN traffic.

v1.7.6b (May 29, 2008)
========================
   Fixes
   -----
   1. Problem: IPv4 TSO generates bad packet when the TSO packet size
               is 1-MSS.

      Cause: Probably firmware does not expect this boundary condition.

      Change: Detect this 1-MSS condition in driver and skip the TSO logic.
              1-MSS TSO packet will be treated like a regular TX checksum
              offload packet.

      Impact: TSO on all chips.

   2. Problem: Cannot disable VLAN stripping even when management firmware
               is disabled.

      Cause: The new logic to check firmware VLAN stripping capability
             was buggy.

      Change: Fixed the code so that VLAN stripping can always be disabled
              if management firmware is disabled.

      Impact: VLAN/management firmware.

v1.7.5d (May 13, 2008)
========================
   Enhancements
   ------------
   1. Change: Incorporated latest firmware 4.4.18. Bug fix is in
              RV2P.

      Impact: All chips.

v1.7.5c (May 7, 2008)
========================
   Enhancements
   ------------
   1. Change: Incorporated latest firmware 4.4.17. Bug fix is in
              RV2P.

      Impact: All chips.

v1.7.5b (May 5, 2008)
========================
   Fixes
   -----
   1. Problem: (CQ35080) Hard lock when running ethtool -s on the device
               that is in the down state.

      Cause: I/O to the device to set link speed in D3-hot state can cause
             lockup because the chip does not respond to I/O.

      Change: ethtool -s will just store the new settings without configuring
              the new speed.  When the device is later brought up, the new
              speed will be set as part of chip init.

      Impact: All chips.

   2. Problem: (CQ35075 CQ35042) Various compile errors on SuSE SLES 9 and SLES
               10 distro kernels.

      Cause: ip_hdr() and __le32/__le32 backported to the distro kernels.

      Change: Adjusted compatibility defines.

      Impact: None.

   Enhancements
   ------------
   1. Change: Incorporated latest 5709 firmware 4.4.16.  Timer context
              scanning is reduced with this firmware to 500us.  With this,
              the temporary enhancement in 1.7.4c #2 has been removed.

      Impact: 5709 iSCSI.

v1.7.4e (April 26, 2008)
========================
   Fixes
   -----
   1. Problem: (CQ34841) 5709 does not link up on some remote PHY systems.

      Cause: No initial link interrupt.

      Change: Added code to poll for link when remote PHY is present.

      Impact: Remote PHY systems.

   2. Problem: (CQ34767) Kernel panic on 5709 when using jumbo frames
               with NCSI traffic.

      Cause: RV2P bug causing RX packets to overwrite kernel memory.

      Change: Updated to latest RV2P code for 5709 and 5708.

      Impact: 5706/5708/5709.
               
v1.7.4d (April 17, 2008)
========================
   Fixes
   -----
   1. Problem: IPv6 iSCSI does not work.

      Cause: Added code in the last version 1.7.3c to check for CONFIG_IPV6
             before enabling the IPv6 CNIC support.  This failed to check
             for CONFIG_IPV6_MODULE if IPv6 is configured as module in the
             kernel configuration.

      Change: Changed the checking to CONFIG_IPV6 or CONFIG_IPV6_MODULE.

      Impact: None.

v1.7.4c (April 16, 2008)
========================
   Fixes
   -----
   1. Problem: (CQ34814, CQ33984) Driver does not compile on 2.4 kernels.

      Cause: __le32 and __be32 not defined in 2.4 kernels.

      Change: Defined these as u32 on 2.4 kernels.

      Impact: 2.4 kernels.

   Enhancements
   ------------
   1. Change:  Incorporated latest 5709 4.4.12 firmware to fix various iSCSI
               problems.

      Impact:  5709.

   2. Change:  Slowed down the timer block reload time.  It was noticed that
               after the CNIC driver was unloaded, the timer context memory
               was reloaded in a tight loop by the chip.  This issue needs
               to be properly addressed in the firmware at a future date.

      Impact:  iSCSI.

v1.7.4b (April 11, 2008)
=======================
   Enhancements
   ------------
   1. Change:  Incorporated latest 5709 4.4.11 firmware to fix various iSCSI
               problems.

      Impact:  5709.

v1.7.3k (April 9, 2008)
=======================
   Enhancements
   ------------
   1. Change:  Incorporated latest 5709 4.4.10 firmware to fix various iSCSI
               problems.  CID ranges are now read directly from shared memory.

      Impact:  5709.

v1.7.3j (April 7, 2008)
=======================
   Fixes
   -----
   1. Problem: (CQ33967) Ethtool register test fails.

      Cause: Register 0x1004 context status register should not be tested.

      Change: Removed 0x1004 from register test.

      Impact: None.
 
   Enhancements
   ------------
   1. Change:  Incorporated latest 5709 4.4.9 firmware to fix various iSCSI
               problems.

      Impact:  5709.

v1.7.3i (April 4, 2008)
=======================
   Fixes
   -----
   1. Problem: (CQ33948) iSCSI over IPv6 does not work on SLES10.

      Cause: The CNIC driver does not handle IPv6 on older kernels without
             NETEVENTS support.

      Change: Modified the logic to support older kernels.

      Impact: All iSCSI connections using IPv4 or IPv6.

   2. Problem: (CQ34315) Scanning iSCSI disks during max sessions test causes
               connection problems.

      Cause: 5709 context memeory allocated by CNIC driver does not match
             the iSCSI and PG CID range used by the firmware.

      Change: Changed to the matching CID range.

      Impact: 5709 iSCSI.

v1.7.3h (March 28, 2008)
=======================
   Fixes
   -----
   1. Problem: (CQ33984, CQ34210, CQ34310, CQ34597) Various compiler warnings
               and errors on RHEL, SuSE, and 2.4 kernels.

      Cause: New features not compatible with older kernels, or older
             vendor kernels backported with newer features.

      Change: Fine-tuned compatibility compiler directives.

      Impact: All kernels.

v1.7.3g (March 10, 2008)
=======================
   Enhancements
   ------------
   1. Change: Updated to latest 5709 firmware version 4.4.7.

      Impact: 5709.

v1.7.3f (March 10, 2008)
=======================
   Fixes
   -----
   1. Problem: CNIC takes a long time to resolve ARP, causing iSCSI to fail.

      Cause: NETEVENT_NEIGH_UPDATE event notifier sometimes takes a long time
             to be called.

      Change: This is under investigation.  For now, the workaround is to
              use the existing neighbour entry if it is in NUD_VALID state.
              Previously, we would only use it if it was in NUD_CONNECTED
              state.

      Impact: iSCSI neighbour resolution.

   2. Problem: iSCSI sometimes fails to initialize.

      Cause: The KWQ is in full condition and prevents any KWQE to be sent
             to the firmware.  This is caused by the KWQ consumer index in
             the status block not initializing to 0.

      Change: Added workaround to skip the KWQ full condition check when
              sending the first KWQE.  This should be properly fixed in
              firmware.

      Impact: None.

v1.7.3d (February 15, 2008)
============================
   Fixes
   -----
   1. Problem: System hangs with iSCSI traffic.

      Cause: Infinite loop in NAPI poll.

      Change: Fixed the problem of not comparing the CNIC tag properly when
              determining whether there is more work in NAPI poll.

      Impact: None.

   2. Problem: iSCSI does not work on 5709

      Cause: Not initializing 5709 properly for iSCSI.  The chip_id field was
             not propagated to the CNIC driver.

      Change: Fixed the chip_id field.

      Impact: None.

v1.7.3c (February 09, 2008)
============================
   Enhancements
   ------------
   1. Change: Updated 5708 and 5709 firmware to version 4.4.2.

      Impact: All devices.

   2. Change: Updated RV2P firmware to the latest.  This may fix the jumbo
              frame issue.

      Impact: All devices, especially jumbo frames on 5709 Bx.

   3. Change: Modified CNIC interface in preparation for 57710 devices.

      Impact: iSCSI.

v1.7.2f (February 04, 2008)
============================
   Fixes
   -----
   1. Problem: Temporary workaround for one prototype 5709S mezz. card not
               working.

      Cause: The driver was looking at the wrong shared memory location to
             identify the card.

      Change: Fixed the code to check the correct BNX2_SHARED_HW_CFG_CONFIG
              location.

      Impact: 5709S.

v1.7.2e (January 31, 2008)
============================
   Fixes
   -----
   1. Problem: (CQ33704) CNIC driver fails MSI-X mode on 5709.

      Cause: When implementing the fix, the wrong constant was used
             for the CNIC MSI-X vector.

      Change: Corrected to use the correct constant BNX2_CNIC_VEC.

      Impact: None.

   2. Problem: iSCSI outgoing packets over IPv6 are bigger than 1518 bytes.

      Cause: MSS calculation was based on IPv4 and did not accout for the
             IPv6 header size.

      Change: Adjusted MSS calculation for IPv6.

      Impact: None.

v1.7.2c (January 30, 2008)
============================
   Fixes
   -----
   1. Problem: CNIC driver does not work in MSI-X mode on 5709.

      Cause:  This is a regression caused by moving the CNIC MSI-X
              vector from 8 to 2.  The context memory did not get
              updated with the new vector.

      Change: Changed the definition.  All bits that depend on the
              MSI-X vector will now have the proper definitions automatically.

      Impact: None.

v1.7.2b (January 30, 2008)
============================
   Enhancements
   ------------
   1. Change: Updated 5709 firmware to 4.4.1.

      Impact: 5709.

   2. Change: Added temporary workaround for one prototype 5709S mezz. card.
              The workaround will be removed once newer cards are available.

      Impact: 5709S.

v1.7.1e (January 14, 2008)
============================
   Enhancements
   ------------
   1. Change: Updated 5709 firmware to 4.1.1 for IPv6 iSCSI support.

      Impact: 5709.

   2. Change: Updated 5708 RXP firmware to 4.1.1.

      Impact: 5706/5708.

   3. Change: Updated RV2P firmware for 5709.

      Impact: 5709.

   4. Change: Added IPv6 support to CNIC driver.

      Impact: New BNX2I driver must be used with this new CNIC driver.

v1.7.1d.3 (February 7, 2008)
============================
   Fixes
   -----
   1. Problem: 5706S continues to not link down occasionally on some blade
               systems.

      Cause:  In some cases, even turning off the tx current does not
              cause the link to go down.

      Change: Link transition can be triggered based on the SYNC_FAILED bit
              in the AN_DEBUG register when all else fails.

      Impact: 5706S.

v1.7.1d.1 (February 1, 2008)
============================
   Fixes
   -----
   1. Problem: 5706S still not linking down occasionally on some blade
               systems when the switch blade is disconnected.

      Cause:  Occasionally, all the bits that we check will falsely
              indicate link up and trigger the parallel detect logic on
              this blade platform. Once in parallel detect mode with
              autoneg disabled, the driver will never detect link down.

      Change: Disabled parallel detect on this platform by checking
              PCI sub IDs to identify the device.

      Impact: Parallel detect not supported on this vendor device.

v1.7.1d (January 25, 2008)
============================
   Fixes
   -----
   1. Problem: 5706S still not linking down on some blade systems when the
               switch blade is disconnected.

      Cause:  This is the same problem that was fixed in 1.7.0b.  After
              switch module is removed, the SYNC_FAILED bit sometimes
              toggles low, and this causes the parallel detect logic in the
              driver to trigger and disable autoneg.  Disabling autoneg
              causes false link to come up immediately.

      Change: It seems that the RUDI_INVALID bit can be used to prevent the
              above from happening.  Modified parallel detect code to
              additionally check the RUDI_INVALID bit and trigger only when
              the bit is cleared.

      Impact: Parallel detect logic in 5706S.

v1.7.1c (December 27, 2007)
============================
   Fixes
   -----
   1. Problem: Driver crashes when adding VLAN and bonding.

      Cause: Bonding calls driver's VLAN function in interrupt context with lock
             held.  We recently added a VLAN feature in 1.6.8b which requires
             chip reset when VLANs are added or removed.  The reset will call
             vmalloc/vfree which must not be called in interrupt context.

      Change: Reverted the VLAN feature for now.  Will workaround it in the
              future.

      Impact: 5709 only. This new VLAN feature is no longer available.

v1.7.1b (December 24, 2007)
============================
   Fixes
   -----
   1. Problem: Driver crashes when using jumbo frames on 5709 A1.

      Cause: RV2P firmware problem.

      Change: Disabled jumbo page ring on 5709 Ax chips.

      Impact: Jumbo receive page rings not supported on 5709 Ax.

   2. Problem: CNIC driver prints "Failed waiting for ref count to go to zero"
               when unloading the driver. This is a minor cosmetic issue.

      Cause: Minor bug in driver comparing ref_count to 1 instead of zero
             during exit.

      Change: Fixed the code to check for ref_count == 0.

      Impact: None.

v1.7.0b (December 12, 2007)
============================
   Fixes
   -----
   1. Problem: (CQ33032) CPU utilization increases dramatically when TSO
               is enabled.

      Cause: Driver is spending a lot of unnecessary time in TX handling
             code when TSO is enabled.  This regression was introduced when
             the TX handling code was changed to match the RX handling code.
             The RX handling code was changed to fix a packet rot problem.
             When TSO is enabled, the tx index can stop at non-packet
             boundaries and the code will keep waiting until it gets to the
             next packet boundary.

      Change: Fixed it to handle this condition properly.

      Impact: None.

   2. Problem:  5706S does not link down in some blade systems.

      Cause: Hardware problem.

      Change: Added workaround logic to check periodically and force a
              link down when the PHY reports SYNC status failed.  This
              only works when autoneg is enabled.

      Impact: 5706S.

v1.6.8e (December 10, 2007)
============================
   Fixes
   -----
   1. Problem: When using jumbo MTU with large RX ring sizes, system will
               crash or the driver won't load.

      Cause: Bug in driver where the page descriptor array was declared
             too small.

      Change: Fixed the array size.

      Impact: None.

   2. Problem: CNIC driver won't compile on kernels without CONFIG_PCI_MSI.

      Cause: Some code needs to be conditionally compiled only when
             CONFIG_PCI_MSI is set.

      Change: Added #ifdef CONFIG_PCI_MSI where necessary.

      Impact: None.

   3. Change: Disabled iSCSI on 5709 until next release.

      Impact: None.

v1.6.8d (December 07, 2007)
============================
   Change: Reverted the 5706S workaround made in 1.6.8c because it was
           unreliable.

   Impact: None.

v1.6.8c (December 07, 2007)
============================
   Fixes
   -----
   1. Problem: (CQ32794) Kernel panic (skb_over_panic) with jumbo frames.

      Cause: RV2P firmware incorrectly placed jumbo data into SKB.

      Change: New RV2P firmware.

      Impact: Jumbo frames on all hardware.

   2. Problem: (CQ32817) ethtool loopback test fails.
   3. Problem: (CQ32842) Chariot test fails.

      Cause: RX buffer size too small to contain MTU-sized frame.
             This was introduced by the new Jumbo RX logic.

      Change: Fixed RX buffer size logic.

      Impact: Traffic on all hardware.

   4. Problem: (CQ32862) Fails to compile on RH9u9.

      Cause: Kernel API skb_fill_page_desc() backported to RH kernel
             causing duplicate definition.

      Change: Adjusted compatibility code.

      Impact: None.

   5. Problem: (CQ32866) ISCSI driver fails to compile with 1.6.8b.

      Cause: print_mac() multiply defined when bnx2.h is included
             in the bnx2i driver.

      Change: Changed print_mac() to static inline.

      Impact: None.

   6. Problem:  5706S does not link down in some blade systems.

      Cause: Hardware problem.

      Change: Added workaround logic to check periodically.

      Impact: 5706S.

   Enhancements
   ------------
   1. Change: Added flow control logic on 5709.

      Impact: 5709.

   2. Change: Updated all firmware to 4.0.5.

      Impact: All hardware.

v1.6.8b (November 28, 2007)
============================
   Enhancements
   ------------
   1. Change:  Added MSIX support for 5709 B0.

      Impact: 5709 B0.

   2. Change:  Added multi-page buffer support for Receive Jumbo frames.

      Impact: All chips.  This feature is experimental at this point.

   3. Change:  Allow VLAN tags in receive packets when management firmware
               is enabled.

      Impact: 5709 only. This feature is experimental and requires new
              boot code and UMP/IPMI code.

   4. Change: Updated firmware to 4.0.3.

      Impact:  All chips.

v1.6.7b (October 16, 2007)
============================
   Fixes
   -----
   1. Problem: (CQ31861) Remote copper PHY does not link up if WoL is enabled.

      Cause: bnx2_set_power_state() assumes that only copper devices support
             WoL and proceeds to configure the copper PHY to 10/100 Mbps.
             This assumption is no longer valid after Serdes WoL support
             was added in 1.6.3c.

      Change: Fixed the code to take check for Serdes and copper when setting
              up the PHY for WoL.

      Impact: WoL.

v1.6.6b (October 10, 2007)
============================
   1. Change: Update 5708 firmware to 3.7.19.

v1.6.5k (October 10, 2007)
============================
   1. Problem: Will not compile on 2.6.23 kernel.

      Cause: get_perm_addr no longer defined in struct ethtool_ops

      Change: Adjusted kernel compatibility #ifdef.

      Impact: None.

v1.6.5j (October 10, 2007)
============================
   No change to bnx2.  Updated cnic driver to 1.1.24.

v1.6.5i (October 8, 2007)
============================
   Enhancements
   ------------
   1. Change: Update 5708 firmware to 3.7.18.

v1.6.5h (October 4, 2007)
============================
   Enhancements
   ------------
   1. Change: Update 5708 firmware to 3.7.17.

v1.6.5g (October 1, 2007)
============================
   Enhancements
   ------------
   1. Change: Update 5708 firmware to 3.7.16.

v1.6.5f (September 30, 2007)
============================
   Enhancements
   ------------
   1. Change: Update 5708 firmware to newer 3.7.15.

v1.6.5e (September 29, 2007)
============================
   Enhancements
   ------------
   1. Change: Update 5708 firmware to 3.7.15.

v1.6.5d (September 28, 2007)
============================
   Enhancements
   ------------
   1. Change: Combined RPM package and tar file with CNIC driver.

v1.6.5c (September 26, 2007)
============================
   Enhancements
   ------------
   1. Change: Update 5708 firmware to 3.7.14.

v1.6.5b (September 25, 2007)
============================
   Fixes
   -----
   1. Problem: (CQ30086) 5709 A1 does not link up when connected to
               some Broadcom devices.

      Cause: Early DAC wakeup workaround needed for 5709 A1.

      Change: Added workaround.

      Impact: None.

   Enhancements
   ------------
   1. Change: Added CNIC support for iSCSI.

      Impact: Only enabled on 2.6.16 and newer kernels.

v1.6.3c (July 23, 2007)
=======================
   Fixes
   -----
   1. Problem: (CQ30591) ethtool -t fails on remote PHY systems.

      Cause: Link test and loopback test were not modified to support
             remote PHY.

      Change: Added remote PHY support to link test and changed the code
              to skip PHY loopback on remote PHY since it's not supported.

      Impact: None.

   2. Problem: (CQ30625) ethtool speed settings are lost after ifdown.

      Cause: The remote PHY settings stored in firmware is not the same
             as the driver's last setting.

      Change: Modified the code to keep the driver's setting unless there's
              is change in the remote PHY media.

      Impact: ethtool -s on remote PHY systems.

   Enhancements
   ------------
   1. Change: Change ethtool's wol setting to NVRAM's default and
              add support for Serdes WoL if NVRAM supports it.

      Impact: ethtool wol's default setting.

v1.6.3b (July 13, 2007)
=======================
   1. Problem: Problems reading and writing flash on 5709.

      Cause: Hardware changes in 5709.

      Change: Rearranged current flash code to properly support 5709.

      Impact: Changes will impact flash operations on 5706/5708/5709 devices.

   2. Problem: (CQ30516) Management firmware version string disappears
               on 2nd modprobe of the driver.

      Cause:  The 2nd modprobe will program the device back to D0 from D3hot.
              This causes a reset and it will take some time before the
              management firmware information will be available.

      Change: Added a proper wait loop to wait for the firmware information
              to be deposited in shared memory.

      Impact: None.

v1.6.2f (July 3, 2007)
=======================
   1. Problem: The fix for CQ29488 in the previous version is problematic
               and needs to be reverted.

      Cause: Adding the netif_carrier_off() call before register_netdev()
             in bnx2_init_one() can cause problems if register_netdev()
             fails.  netif_carrier_off() can queue a link watch event
             that can run later.  If register_netdev() fails, the netdev
             structure will be freed and the link watch event may panic
             when it is scheduled to run.

      Change: Moving the netif_carrier_off() to after register_netdev()
              also will not work as it can cause race conditions with
              the interrupt handler.  So the best thing to do is to
              revert the earlier fix and not address the CQ29488 issue.

      Impact: CQ29488 is not fixed.

v1.6.2e (July 3, 2007)
=======================
   Fixes:
   ------
   1. Problem: (CQ29528) Link does not come up using remote PHY (continued).

      Cause: ifup script may be using mii-tool to obtain link status,
             and interfering with remote PHY firmware.

      Change: Block mii-tool ioctl access when remote PHY firmware is present.

      Impact: None.

   2. Problem: (CQ29488) Driver reports link up in ethtool before the interface
               is brought up.

      Cause: The netdevice structure's initial link setting is up and that
             gets reported directly by ethtool.

      Change: Added netif_carrier_off() call in bnx2_init_one().

      Impact: None.

v1.6.2d (June 22, 2007)
=======================
   Fixes:
   ------
   1. Problem: (CQ29528) Link does not come up using remote PHY.

      Cause: The fix in 1.6.2b still has a problem.  The copper or Serdes
             default link setting does not follow the correct port when
             the port is changed during chip reset.

      Change: Fix the code to always refresh the port and link setting
              during chip reset.

      Impact: None.

   2. Problem: (CQ30181) Cannot compile on 2.4 kernels.

      Cause: USEC_TO_SEC constant is not defined on older kernels.

      Change: Added conditional #define for this constant on older kernels.

      Impact: None.

   Enhancements:
   -------------
   1. Change: Update 5709 firmware to 3.7.1.

      Impact: 5709 devices.

v1.6.2b (June 21, 2007)
=======================
   Enhancements:
   -------------
   1. Change: Added management firmware version to ethtool -i.

      Impact: None.

   Fixes:
   ------
   1. Problem: (CQ29528) Link does not come up using remote PHY.

      Cause: The driver is using the wrong port when setting up the remote
             PHY link.

      Change: Fixed bug to always use the correct requested port or
              default port when setting remote PHY link.

      Impact: None.

   2. Problem: (CQ30028) Advertised Autoneg not set in ethtool.

      Cause: Remote PHY code is not setting the flag which is for
             information only.

      Change: Added code the set the flag for consistency.

      Impact: None.

v1.6.1c (May 22, 2007)
=====================
   Enhancements:
   -------------
   1. Change: (CQ28907) Added support for setting copper and fibre speeds.

      Impact: Only available on Remote PHY systems.

v1.6.1b (May 7, 2007)
=====================
   Fixes:
   ------
   1. Problem: (CQ29301) Setting invalid speed setting causes driver to
               crash.

      Cause: Lock taken without unlock when exiting iwith error the
             procedure to set speed.

      Change: Fixed the code with proper unlock.

      Impact: None.

v1.6.0b (April 30, 2007)
========================
   Enhancements:
   -------------
   1. Change: Improved handshake with remote PHY firmware.

      Impact: None.

v1.5.10c (May 4 , 2007)
=======================
   Fixes:
   ------
   1. Problem: Extremely low TSO performance when destination has a
               smaller MSS than the source.

      Cause: Packets smaller than MTU are not processed as TSO packets.

      Change: Removed the SKB length check when doing TSO.

      Impact: None.

v1.5.10b (May 1, 2007)
=========================
   Enhancements:
   -------------
   1. Change: Removed Remote PHY until next release.

      Impact: No Remote PHY support.

   2. Change: Added check for 2.5G capability before enabling 2.5G on
              5709S.

      Impact: None.

   Fixes:
   ------
   1. Problem: (CQ28438) NETDEV WATCHDOG after OS boot.

      Cause:  The mailbox queue is halted after the OS reads config.
              register 0x94.

      Change: Set MQ_CONFIG_HALT_DIS in register MQ_CONFIG on 5709 A0 and
              A1.

      Impact: None.

v1.5.9b (April 20, 2007)
=======================
   Enhancements:
   -------------
   1. Change: Enhanced remote PHY support for 5708S.

      Impact: None.

   Fixes:
   ------
   1. Problem: (CQ29056) Driver does not compile on SLES 10 SP1 kernel.

      Cause:   Backported netif_tx_lock() causes compatibility problem.

      Change:  Adjuested compatibility #ifdef.

      Impact:  None.

   2. Problem: (CQ28880) Driver fails register test after running traffic.

      Cause:   A reserved register 0x500c was mistakenly included in the test.

      Change:  Removed this register from the test.

      Impact: None.

v1.5.8b (March 13, 2007)
=======================
   Enhancements:
   -------------
   1. Change: Added remote PHY support for 5708S.

      Impact: None.

v1.5.7b (March 2, 2007)
=======================
   Enhancements:
   -------------
   1. Change: Added IPV6 TSO for 5709.

      Impact: None.

   2. Change: Added 2.5G parallel detection for 5709s.

      Impact: None.

v1.5.6b (February 28, 2007)
===========================
   Enhancements:
   -------------
   1. Change: Added Serdes support for 5709.

      Impact: None.

   Fixes:
   ------
   1. Problem: (CQ28433) Driver does not compile on some early 2.6 and
               2.4 kernels.

      Cause: Kernel compatibility issue.

      Change: Added some missing #ifdef CONFIG_PCI_MSI.

      Impact: None.

   2. Problem: (CQ28527) System hangs when running bonding scripts on 5709.

      Cause: Bonding driver reads MDIO registers after the device is in
             D3hot state.

      Change: Added check to disallow MDIO access after the device is down.

      Impact: None.

v1.5.5b (January 31, 2007)
===========================
   Fixes:
   ------
   1. Problem: (CQ28252) Driver reports the same MAC address for both
               ports of 5709.

      Cause: The driver was obtaining the MAC address from the same
             shared memory area for both ports.

      Change: Updated driver to read from the deicated shared memory
              area for each port.

      Impact: None.

   2. Problem: (CQ28226) 5709C does not link up when connected to certain
               switches.

      Cause:  PHY's Early DAC Wakeup Enable bit's strapped value is set.

      Change: Disable Early DAC Wakeup enable on 5709 A0 after PHY reset.

      Impact: None.

v1.5.4b (January 8, 2006)
===========================
   Fixes:
   ------
   1. Problem: 5709 copper device detected as serdes.

      Cause:  Media detection code not complete.

      Change: Added complete media detection code.

      Impact: None.

   Enhancement:
   ------------
   1. Change: Add IPv6 checksum support.

      Impact: None.

v1.5.2b (December 22, 2006)
===========================
   Merged in all latest changes.

v1.5.1c (November 30, 2006)
===========================
   Enhancement:
   ------------
   1. Change: Remove 5709 FPGA code.

      Impact: None.

v1.5.1b (November 15, 2006)
===========================
   Enhancement:
   ------------
   1. Change: Added support for 5709.

      Impact: None.

v1.4.52c (March 07, 2007)
=========================
   Enhancement:
   ------------
   1. Change: Increase maximum receive ring size to 4080.
              The default is kept the same at 255.

      Impact: None.

v1.4.51b (December 21, 2006)
============================
   Fixes:
   ------
   1. Problem: (CQ27802) Cannot enable flow control in some cases.

      Cause:  In some cases when flow control is forced to on, the
              driver detects no changes in advertisement, and as a
              result, will not re-autoneg.  Without the link change,
              flow control settings will not change.

      Change:  Added some code to setup flow control when no other
               PHY settings are made.  This will ensure that flow
               control changes will take effect immediately.

      Impact: None.

v1.4.50b (December 15, 2006)
============================
   Fixes:
   ------
   1. Problem: (CQ27424) Panic when writing to nvram.

      Cause:  Bug in driver when an alignment buffer is used

      Change: Fixed the bug so that the alignment buffer is freed with the
              correct pointer.

      Impact: None.

v1.4.49b (December 13, 2006)
============================
   Fixes:
   ------
   1. Problem: (CQ27459) Driver reports link down when link is up.

      Cause:  Hotplug scripts can cause bnx2_open() to be called immediately
              after bnx2_init_one() calls register_netdev().  The initial
              link state set after register_netdev() may overwrite the actual
              link state set by the link handler on SMP systems.

      Change:  Move all initial state setup code to before calling
               register_netdev().

      Impact : None.

v1.4.48b (December 08, 2006)
============================
   Fixes:
   ------
   1. Problem: (RHBZ 212055)  Panic in bnx2_poll().

      Cause: Bug in determining tx ring space when the tx ring is
             completely full.

      Change: Fixed the flawed logic in bnx2_tx_avail().

      Impact: None.

   2. Problem: (CQ27424) Buffer overflow when writing to nvram.

      Cause:  Bug in driver when the beginning NVRAM offset is
              not 4-byte aligned.

      Change: Fixed the bug to allocate enough buffer space.

      Impact: None.

   3. Problem: (CQ27543) Loopback failed if MAC address is changed.

      Cause: Driver uses permanent MAC address for loopback which may
             be different from a locally administered address.

      Change: Fixed by alwaysing using the current MAC address in the
              netdevice structure.

      Impact: None.

v1.4.47b (November 02, 2006)
===========================
   Fixes:
   ------
   1. Problem: (CQ25922) 5708S does not pass PHY loopback test on
               some blade servers.

      Cause:  It takes longer (about 100msec) to link up in some
              backplane environments when the Serdes is set to PHY
              loopback mode.

      Change: Increase delay loop to up to 1 sec when waiting for
              link up after PHY loopback.  Previous wait time was
              100usec.

      Impact: None.

v1.4.46b (October 30, 2006)
===========================
   Fixes:
   ------
   1. Problem: (CQ25916) Device does not receive packets when configured
               by the Xen bridge script and when IPMI is enabled.

      Cause: Firmware does not forward packets to the host when the
             device is in promiscuous mode in some cases.

      Change: Firmware change and driver change to enable the
              BNX2_RPM_SORT_USER0_PROM_VLAN bit when going into
              promiscuous mode.

      Impact: None.
             
v1.4.45b (October 19, 2006)
===========================
   Enhancement:
   ------------
   1. Change: Added software parallel detection on 5708S to link at
              1000Mbps or 2500Mbps automatically if the link partner is
              forced at 2500Mbps.

      Impact: None.

   2. Change: Added 2500Mbps forced speed setting.  Setting it requires
              a future version of ethtool or custom apps.

      Impact: None.

   3. Change: Port driver to compile on 2.6.19 kernel.

      Impact: None.

   Fixes:
   ------
   1. Problem: Driver does not complile on 2.4 kernels.

      Cause: TSO symbols not defined in 2.4 kernels.

      Change: Added #ifdef for compatibility.

      Impact: None.

   2. Problem: MSI doesn't work on 5706 when the host bridge is AMD8132.

      Cause: Compatibility issue.

      Change: Added code to disable MSI when 5706 is on a systems with
              AMD8132.

      Impact: 5706 cannot use MSI on such systems.

v1.4.44b (August 10, 2006)
==========================
   Fixes:
   ------
   1. Problem: A rare tx race window exists in the tx path.

      Cause: CPU re-ordering can cause the tx queue to be stopped
             forever when the tx ring is full in a very rare
             condition.  See ChangeLog for more details.

      Change: Fixed the race condition with memory barriers.
              See ChangeLog for more details.

      Impact: None.

   Enhancement:
   ------------
   1. Change: Increase default rx ring size to 255 to prevent
              packet drops under heavy load.

      Impact: Higher memory usage.

   2. Change: Port driver to run on 2.6.18 kernel.

      Impact: None.


v1.4.43b (June 26, 2006)
=======================
   Enhancement:
   ------------
   1. Change: (CQ25508) Use DRV_MSG_CODE_UNLOAD_LNK_DN message on
              5708 B1 and older chips so that the link will turn
              off after ifdown.

      Impact: None.

v1.4.42b (June 2, 2006)
=======================
   Fixes:
   ------
   1. Problem: (CQ22585) WoL cannot be enabled on 5708 B2.

      Cause: Hardware limitation in previous 5708 versions required
             driver to always disable driver WoL on 5708.

      Change: With the issue fixed in B2, the driver was changed to
              allow 5708 B2 and above to support driver WoL.

      Impact: None.

   2. Problem: (CQ21779) Driver does not report dropped receive packets.

      Cause: Packets dropped by firmware are reported in a scratch pad
             location in memory separate from other counters.

      Change: Added code to report this firmware counter.

      Impact: None.

   Enhancements:
   -------------
   1. Change: (CQ24690) Allow driver to be compiled for non-running kernels.

      Impact: None.

v1.4.41b (May 17, 2006)
=======================
   Fixes:
   ------
   1. Problem: Driver writes wrong data to non-buffered flash.

      Cause: Bug in driver causing the unchanged portion of the page
             to be corrupted.

      Change: Fixed bug.

      Impact: None.

v1.4.40b (April 17, 2006)
=========================
   Enhancements:
   -------------
   1. Change: Combine 2 small memory allocations into 1.

      Impact: None.

   2. Change: Separate tx consumer and producer entries into separate
              cache lines for better performance.

      Impact: None.

   3. Change: Compress firmware data to reduce driver size.

      Impact: Driver now requires zib_inflate library which should be
              available on most vendor kernels.

v1.4.39b (Mar. 10, 2006)
=======================
   Fixes:
   ------
   1. Problem: (CQ23181) Driver loses track of link changes in some cases.

      Cause: In some cases, the status block gets a link change indication
             that contradicts with the MII link status. This is due to
             transient link signals during link changes.

      Change: Add coalesce_now at the end of link change interrupt to flush
              out the transient behavior.

      Impact: None.

   2. Problem: 5708 only supports 40-bit DMA addresses.

      Cause: Limitation of the built-in PCIE-to-PCIX bridge.

      Change: Add workaround code to make sure all DMA addresses are
              less than 40 bits.

      Impact: Some minor impact on performance on some 64-bits systems.
              There should be practically no performance impact on i386 and
              x86_64 systems.

   3. Problem: "Copyright" deprecated in RPM spec file.

      Change: Changed to "License".

      Impact: Should be none on the distributions that we support.

v1.4.38b (Feb. 10, 2006)
=======================
   Fixes:
   ------
   1. Problem: Setting rx ring size to 255 causes memory allocation errors.

      Cause: Multiple bugs that do not handle the full ring properly.

      Change: Fixed all bugs related to full ring handling and changed
              maximum ring size from 4080 to 1020 after discussion with
              Dave Miller.

      Impact: Maximum rx ring size is now smaller.

   2. Problem: Compile warnings and panic on IA64.

      Cause: <vmalloc.h> not included.

      Change: Added include <vmalloc.h>.

      Impact: None.

v1.4.36b (Jan. 19, 2006)
=======================
   Version number update.

v1.3.36 (Jan. 17, 2006)
=======================
   Fixes:
   ------
   1. Problem: (CQ22827) bnx2 does not compile on 2.6.6 and earlier
               kernels. 

      Cause: Introduced bug while fixing CQ22666.

      Change: Fix compatibility code.

      Impact: None.

   2. Problem: (CQ22823) bnx2 reports extra .5 at the end of firmware
               version string.

      Change: Skip the last digit in the firmware version string.

      Impact: None.

   3. Problem: (CQ22585) WoL still does not work on 5708.

      Cause: New WoL mechanism introduced in 1.3.34 has a flaw.

      Change: Removed the workaround code and disabled WoL support
              on 5708. During shutdown and suspend, the driver will
              shutdown the device and WoL will be setup by the
              bootcode according to the nvram's out-of-box WoL
              setting.

      Impact: 5708 will not support driver-initiated (ethtool-intiated)
              WoL.
              
v1.3.35 (Jan. 17, 2006)
=======================
   Fixes:
   ------
   1. Problem: (CQ22666) bnx2 driver does not compile on RHEL3 U7.

      Cause: if_mii() back-ported to RHEL3 U7.

      Change: Adjusted the compatibility code.

      Impact: None.

   2. Problem: (CQ22718) UMP connection is lost after enabling WoL.

      Cause: FORCE LINK was mistakenly set during WoL setup.

      Change: Do not set FORCE LINK.

      Impact: None.

v1.3.34 (Jan. 13, 2006)
=======================
   Fixes:
   ------
   1. Problem: (CQ22585) WoL does not work on 5708.

      Cause: Internal bridge not in proper PME state.

      Change: Added new firmware message to allow bootcode to help set up
              WoL.

      Impact: None.

   Enhancements:
   -------------
   1. Change: Added compile option to include crc32 function for RH2.4
              boot kernels.

      Impact: None.

   2. Change: Updated TSO firmware to handle ECN.

      Impact: None.

v1.3.33 (Dec. 12, 2005)
=======================
   Enhancements:
   -------------
   1. Change: Increased firmware hand-shake timeout from 50 msec to
              100 msec. Also changed the delay from busy-wait udelay
              to non-busy-wait msleep.

      Impact: None.

   2. Change: Added code to read nvram size from shared memory if
              available. Otherwise, the size will come from the
              flash table which only gives the smallest size for
              that type of flash.

      Impact: None.

   3. Change: Added workaround to issue 2 separate IOs for interrupt
              acknowledgement. The workaround is only used for INTA
              (non-MSI) interrupts.

      Impact: Slightly higher overhead for INTA interrupts.

v1.3.32 (Dec. 01, 2005)
=======================
   Enhancements:
   -------------
   1. Change: Added PHY loopback to the loopback selftest.

      Impact: None.

   2. Change: (CQ21810) Added ethtool -d register dump.

      Impact: None.

   3. Change: Reduce the number of registers tested in selftest to make
              the driver smaller.

      Impact: None.

   4. Change: Increased maximum rx ring size to 4080.

      Impact: None.

   5. Change: Changed rx checksum logic for better reliability.

      Impact: None.

   6. Change: Added 5708 B1 workarounds.

      Impact: None.

v1.3.31 (Nov. 18, 2005)
=======================
   Fixes:
   ------
   1. Problem: (CQTO2080) Cannot pass traffic during 2nd ifup if IPMI
               is enabled.

      Cause: A flaw in driver/firmware handshake.

      Change: Changed driver/firmware handshake by doing WAIT0 first before
              writing the first signature.

      Impact: None.

   2. Problem: (CQTO2056) VLAN-tagged IPMI traffic fails after driver is
               loaded.

      Cause: Driver configures the NIC to keep the VLAN tag by default,
             causing VLAN-tagged IPMI traffic to fail.

      Change: Changed driver to always strip VLAN tags if IPMI is enabled.

      Impact: VLAN will always be stripped when IPMI is enabled. This may
              affect some applications that rely on raw VLAN packets.

   Enhancements:
   -------------
   1. Change: Sync'ed up with latest upstream bnx2.

v1.3.29 (Oct. 6, 2005)
=======================
   Fixes:
   ------
   1. Problem: (CQTO1929) Traffic stops when MTU is greater than 1500
               with TSO enabled.

      Cause: TSO firmware bug.

      Change: Updated to latest firmware.

      Impact: None.

v1.3.28 (Sep. 29, 2005)
=======================
   Fixes:
   ------
   1. Problem: (CQTO1875) Traffic stops when running Nettack with TSO
               turned on.

      Cause: TSO firmware bug.

      Change: Updated to latest firmware.

      Impact: None.

   2. Problem: (CQTO1575) ethtool -S shows non-zero rx_error_bytes.

      Cause: Hardware errata.

      Change: Ignore this counter and always report zero.

      Impact: None.

v1.3.27 (Sep. 21, 2005)
=======================
   Enhancements:
   -------------
   1. Change: Enabled ethernet@wirespeed on copper devices.

      Impact: None.

   2. Change: Enabled customized pre-emphasis and other serdes control
              settings on 5708S backplane devices. A special PHY
              register will be programmed according to the NVRAM value.

      Impact: None.

   3. Change: Modified Makefile to check for the source symbolic link
              in the kbuild environment.

      Impact: None.

   4. Change: Improved NAPI poll processing so that all events will be
              processed before interrupts are re-enabled. This will
              reduce the number of unnecessary interrupts.

      Impact: None.

   5. Change: Add support for ETHTOOL_GPERMADDR (from John Linville)

      Impact: None.

   Fixes:
   ------
   1. Problem: Bug in irq handler causing extra register read.

      Cause: Bug in bnx2_interrupt() reading BNX2_PCICFG_MISC_STATUS
             register when it is not necessary.

      Change: Fixed the logic bug and added prefetch of status block in
              msi handler.

      Impact: None. 

v1.3.25 (Aug. 22, 2005)
=======================
   Fixes:
   ------
   1. Problem: Ethtool register and memory tests fail on 5708.

      Cause: Some code was not merged properly many versions ago.

      Change: Merged in properly code.

      Impact: None.

   Enhancements:
   -------------
   1. Change: Slow down flash clock speeds

      Impact: None.

   2. Change: Code re-sync'ed with upstream driver.

      Impact: None.

v1.3.24 (Aug. 16, 2005)
=======================
   Enhancements:
   -------------
   1. Change: Changed all spin_lock_irqsave locks to spin_lock_bh for
              better overall system performance. All code requiring
              spin_lock runs in BH or user context.

      Impact: None.

   2. Change: Removed atomic operations in the transmit fast path.
              Code should run a bit faster as atomic operations can be
              quite slow.

      Impact: None.

v1.3.23 (Aug. 10, 2005)
=======================
   Enhancements:
   -------------
   1. Change: Added reporting of link speed to firmware.

      Impact: None.

   2. Change: Added shared memory base look-up.

      Impact: None.

   3. Change: Possible sparse fixes (from Peter Hagervall)
              - use C99 struct initializers
              - make a few arrays and structs static
              - remove a few uses of literal 0 as NULL pointer
              - use convenience function instead of cast+dereference in
                bnx2_ioctl()
              - remove superfluous casts to u8 * in calls to readl/writel

      Impact: None.

   4. Change: Updated documentation with the crc32 library requirement and
              other minor updates.

      Impact: None.

v1.3.22 (July 25, 2005)
=======================
   Enhancements:
   -------------
   1. Change: Added check for default link speed setting in shared memory.
              This allows some blade servers that don't support autoneg to
              default to forced speed to speed up link-up time.

      Impact: None.

   2. Change: Changed timer code to speed up the timer after serdes autoneg.
              This speeds up the time for parallel detection when the link
              partner does not autoneg. After autoneg or parallel detction
              completes, timer goes back to normal 1 HZ interval. With the
              new scheme, link should be detected up using parallel detection
              in less than 0.7 seconds. Autoneg normally completes in 120
              msec exchanging base pages and 3 next pages. 

      Impact: None.

v1.3.21 (July 21, 2005)
=======================
   Enhancements:
   -------------
   1. Change: Updated firmware to properly handle TSO packets with ECN
              bits set.

      Impact: None.

   2. Change: Updated to latest rxp firmware.

      Impact: None.

   3. Change: Added check for the 2.5G capability in shared memory.

      Impact: None.

   4. Change: Expanded nvram support for 5708.

      Impact: None.

   Fixes:
   ------
   1. Problem: (CQTO1511) Downing a team of bnx2 adapters causes hang.

      Cause: Deadlock when the second adapter's close routine calls
             flush_scheduled_work() because the linkwatch_event
             is scheduled on the work queue when the first adapter
             is closed. The linkwatch_event will try to get the rtnl_lock
             which is already held by the bnx2_close routine.

      Change: Fixed by not calling flush_scheduled_work(). Instead,
              use a flag to indicate work is pending and wait until
              the flag is cleared.

      Impact: None.

   2. Problem: (CQTO1439) ethtool -S on 5708 causes oops.

      Cause: A pointer is not initialized if the device is 5708.

      Change: Added proper initialization.

      Impact: None.

   3. Problem: Some error counters are mis-reporting.

      Cause: The workaround for the hw errata is not applied properly
             on the chips with the errata.

      Change: Added proper checks for the workaround.

      Impact: None.

   4. Problem: High BER on 5708 SerDes.

      Cause: hardware errata.

      Change: Added workaround for 5708 A0 and B0.

      Impact: None.

v1.3.19 (May 27, 2005)
=======================
   Enhancements:
   -------------
   1. Change: Merged 5708 code with the latest 1.1.19.

      Impact: None.

   Fixes:
   ------
   1. Problem: (CQTO1260) 5708S does not link at 1000Mbps when forced. It
               links at 2500Mbps when connected back-to-back with another
               5708S.

      Cause: 2.5G bit is still turned on.

      Change: Fixed by turning off 2.5G when the speed is forced.

      Impact: None.

v1.1.19 (May 26, 2005)
=======================
   Enhancements:
   -------------
   1. Change: Made significant changes to merge into the kernel. Among
              them, consolidate all source files into bnx2.[ch] and
              bnx2_fw.h, change structure style register definitions
              to offset based.

      Impact: None.

   Fixes:
   ------
   1. Problem: Excessive stack usage.

      Cause: Use of local variable array.

      Change: Fix excessive stack usage in bnx2_alloc_bad_rbuf() by
              replacing local variable array with kmalloc array. Also
              changed function to return error code, and changed some
              of the callers to check for the return code.

      Impact: None.

   2. Problem: Bug in receive checksum.

      Cause: Software bug.

      Change: Fix bug in rx checksum by indicating CHECKSUM_UNNECESSARY
              only when the hw calculated checksum is 0xffff.

      Impact: None.

   3. Problem: Excessive busy loop.

      Cause: Software bug.

      Change: Replaced one excessive udelay of 15msec with msleep since
              the calling context is always process.

      Impact: None.

  4.  Problem: Need to call flush_scheduled_work() and bnx2_netif_stop().

      Cause: Bug in bnx2_close().

      Change: Fix bug in bnx2_close() by calling flush_scheduled_work()
              since we are using a work queue in netdev watchdog. Also
              added bnx2_netif_stop() call in bnx2_close().

      Impact: None.

   5. Problem: Some symbols do not have bnx2 prefix and are not static.

      Change: Add bnx2_ prefix to some remaining names and mark some
              remaining names static.

      Impact: None.

v1.1.17 (Apr. 7, 2005)
=======================
   Fixes:
   ------
   1. Problem: Driver does not compile on 2.6.12 kernel.

      Cause: pci_dev->slot_name has been deprecated.

      Change: replaced with pci_name.

      Impact: None. All kernels supported by bnx2 including 2.4.21-*EL have
              pci_name defined.

v1.1.16 (Mar. 16, 2005)
=======================
   Fixes:
   ------
   1. Problem: (CQTO936 & 1004) Tx carrier and rx_byte_errors reported
               during normal operations.

      Cause: 5706 hardware errata on these 2 statistics counters.

      Change: Modified driver to skip these 2 counters.

      Impact: These 2 counters will always report 0 and not the true
              statistics.

v1.3.15 (Mar. 11, 2005)
======================
   Enhancements:
   -------------
   1. Change: Added SGMII 10/100/1000 Mbps and fiber mode 1000/2500 Mbps
              support.

      Impact: None.

v1.1.15 (Mar. 09, 2005)
=======================
   Enhancements:
   -------------
   1. Change: Added code to program proper phy settings for jumbo
              frames on copper and serdes devices.

      Impact: None.

   2. Change: Changed INTx ISR to handle a valid case where INTx
              arrives before status block update.

      Impact: None.

   3. Change: Added a separate ISR for MSI to handle subtle differences
              between INTx and MSI.

      Impact: None.

v1.1.14 (Mar. 03, 2005)
======================
   Fixes:
   ------
   1. Problem: netdump does not work on latest RH3EL errata kernel.

      Cause: #define RED_HAT_LINUX_KERNEL removed from kernel
             include files, causing netdump poll function to
             be compiled wrong for RH kernels.

      Change: Changed Makefile to workaround the problem.

      Impact: None.

v1.1.12 (Feb. 25, 2005)
======================
   Fixes:
   ------
   1. Problem: (CQTO1062) Driver allows ethtool to set illegal speed/duplex
               on fiber cards.

      Cause: Missing checks for the case where autoneg is off.

      Change: Added proper checks.

      Impact: No.

v1.1.11 (Feb. 18, 2005)
======================
   Enhancements:
   -------------
   1. Change: (CQTO901) Added bnx2(4) man page.

      Impact: None.

v1.1.10 (Feb. 16, 2005)
======================
   Fixes:
   ------
   1. Problem: Wrong device ID in pci_dev_id table.

      Change: Fixed ID.

      Impact: None.

v1.1.9 (Feb. 10, 2005)
======================
   Fixes:
   ------
   1. Problem: (CQTO771) Driver fails to compile on RHEL3 update 4.

      Cause: The RH kernel has back-ported some netif functions
             not found in the same vanilla kernel version. Duplicate
             function names are defined.

      Change: Added intelligence in Makefile to detect such conditions
              and change the CFLAGS accordingly.

      Impact: None.

   2. Problem: (CQTO1017) Driver allows 1000 half duplex autoneg off.

      Cause: Missing validity check.

      Change: Added check.

      Impact: None.

   Enhancements:
   -------------
   1. Change: The code to handle tx queue full condition was redone
              to properly handle all boundary and race conditions.

      Impact: Minimum tx ring size is now MAX_SKB_FRAGS+1.

   2. Change: Tx timeout code was changed to work queue context.
              This allows netif to be shutdown gracefully before
              chip reset.

      Impact: None.

   3. Change: Added memory barriers to ISR and NAPI poll for
              correctness.

      Impact: None.

v1.1.8 (Feb. 01, 2005)
======================
   Fixes:
   ------
   1. Problem: (CQTO969) No interupts on a system that does not
               support MSI.

      Cause: On this system, the MSI generated in the MSI test
             terminates with Master Abort which is a fatal
             condition for the chip.

      Change: A chip reset is added when MSI test fails to bring
              the chip back to normal operations again (in INTx mode).

      Impact: None.

   Enhancements:
   -------------
   1. Change: Removed register 0x84 from the ethtool register test.
              This is an interrupt control register that should
              not be touched to prevent unwanted interrupts.

      Impact: None.

v1.1.7 (Jan. 28, 2005)
======================
   Enhancements:
   -------------
   1. Change: Added interrupt test when MSI is enabled. If MSI test
              fails, driver will fallback to INTx mode.

      Impact: None.

   2. Change: Added test for certain chipsets where MSI is known
              to fail, and disable MSI unconditionally when
              such chipsets are found.

      Impact: None.

   3. Change: Removed support for 1000 Mbps half duplex.

      Impact: 1000 Mbps half duplex will no longer work.

v1.1.6 (Jan. 26, 2005)
======================
   Fixes:
   ------
   1. Problem: (CQTO940) MTU size not set properly when device is down.

      Cause: bnx2_change_mtu only handled the "up" case.

      Change: Simple fix to handle the "down" case as well.

      Impact: None

   2. Problem: (CQTO926) 5706S does not autoneg properly after the
                tx cable is pulled.

      Cause: If the link partner is autonegotiating, autoneg will
             fail when the tx cable is pulled. The software will
             turn off autoneg seeing that the rx cable is still
             attached with SIGNAL_DETECT. When the tx cable is
             re-attached, autoneg is still off and the link partner
             will not establish link.

      Change: Added code to poll another PHY register to check if
              configs are received when autoneg is disabled.
              
      Impact: None
              
   Enhancements:
   -------------
   1. Change: Added OEM product name strings.

      Impact: None.

v1.1.5 (Jan. 25, 2005)
======================
   Fixes:
   ------
   1. Problem: PCI-X bus speed may not be detected correctly by the driver,
               causing failure because certain register settings are done
               based on bus speed.

      Cause: hardware problem.
 
      Change: Use a different register to detect PCI-X speed.

      Impact: None.

v1.1.4 (Jan. 17, 2005)
======================
   Fixes:
   ------
   1. Problem: 5706S does not reliably detect link up or down.

      Cause: hardware problem.

      Change: Enabled hardware workaround which is effective in
              A2 and newer chips only.

      Impact: None.

v1.1.3 (Jan. 13, 2005)
======================
   Fixes:
   ------
   1. Problem: netdump does not work.

      Cause: poll_controller routine does not work in NAPI mode.

      Change: Fixed poll_controller routine for NAPI mode.

      Impact: None.

   Enhancements:
   -------------
   1. Change: Added the new mmiowb macro which is used mainly in NUMA
              machines to guarantee PCI ordering.

      Impact: None.

   2. Change: Added OEM product name strings.

      Impact: None.

   3. Change: Changed ONE_TDMA workaround on systems with P64H bridge to
              PING_PONG_DMA on all systems using PCI.

      Impact: Better performance and better compatibility on all PCI
              systems.

   4. Change: Added "disable_msi" parameter to allow disabling MSI.

      Impact: None.

   5. Change: Reduced default tx coalescing parameters for better
              tx only performance such as ttcp.

      Impact: None.

   6. Change: Changed NIC detection console message to display more
              information.

      Impact: None.

   7. Change: Cleaned up some Linux .h files that are not needed.

      Impact: None.

   8. Change: Cleaned up the nvram routines.

      Impact: None.

v1.1.2 (Nov. 11, 2004)
======================
   Fixes:
   ------
   1. Problem: Unable to load the driver on more than 2 or 3 devices.

      Cause: Default register space is too big. System fails to map
             the register space on the 3rd or 4th device.

      Change: Changed driver to map a smaller register space as the higher
              registers are not needed for standard operations.

      Impact: None.

v1.1.1 (Nov. 9, 2004)
======================
   Fixes:
   ------
   1. Problem: (CQTO656) One remaining ethtool parameter can be set out of
               range.

      Cause: Wrong upper bounds in code.

      Change: Fixed upper bound.

      Impact: None.

   1. Problem: 5706 A1 cannot be run on a PCI bus.

      Cause: Hardware errata.

      Change: Added workaround to detect 5706 A1 on PCI bus and abort.

      Impact: Driver will not load 5706 A1 on PCI bus.

v1.1.0 (Oct. 29, 2004)
======================
   Fixes:
   ------
   1. Problem: (CQTO663) No link on fiber NIC set to autoneg when
               the link partner is set to forced speed.

      Cause: No code to handle this case.

      Change: Added code to check SIGNAL DETECT when autoneg fails,
              and turn off autoneg when appropriate. Also added code
              to force a link down when speed settings are changed.

      Impact: None.

    2. Problem: (CQTO649) ifconfig up/down can cause system to
                hang on 2.6 kernels using mmconfig.

       Cause: Dummy read in the kernel's pci_mmcfg_write routine
              may cause system to hang during D3hot -> D0
              transition. The PLL may lose lock during the internal
              D0 transition chip reset and cause the dummy read to
              hang.

       Change: The PLL problem will be fixed in A2. Meanwhile, the
               driver is changed to go into D3hot only if wol is
               enabled.

       Impact: Minor impact in increased power consumption when
               the driver is shutdown with wol disabled.
              
    3. Change: Changed to use pci_get_device as pci_find_device
               will be deprecated soon.

       Impact: None.

    4. Problem: (CQTO656) Some ethtool parameters can be set out of range.

       Cause: Wrong upper bounds in code or documentation.

       Change: Fixed code and documentation.

       Impact: None.

v1.0.15 (Oct. 15, 2004)
======================
   Fixes:
   ------
   1. Problem: (CQTO644) Data corruption when sending FTP traffic

      Cause: PCI bridge errata.

      Change: Added code to enable ONE_TDMA workaround when P64H
              PCI bridge is detected.

      Impact: Slower tx performance on systems using P64H bridge.

   2. Problem: (CQTO643) Driver allows MTU to be set up to 9004.

      Cause: Driver used the wrong upper bound limit.

      Change: Fixed the upper bound.

      Impact: None.

   3. Problem: Driver does not support forced speed on 5706S.

      Cause: Missing software logic.

      Change: Added code to support forced 1000 Full and Half duplex.

      Impact: None.

   4. Change: Added workaround to disable PERR generation on
              5706 A1 when it is in PCI 64-bit slot.

      Impact: None.

v1.0.14 (Oct. 05, 2004)
======================
   Fixes:
   ------
   1. Problem: Driver load/unload hangs on some machines.

      Cause: Transition delay required during D3hot -> D0 transition.

      Change: Added necessary delay.

      Impact: None.

v1.0.12 (Oct. 04, 2004)
======================
   Fixes:
   ------
   1. Problem: (CQTO609) New flow control parameter does not take
               effect until ifdown/ifup or link down/up.

      Cause: New flow control settings are only configured during
             link up. The driver did not check flow control
             advertisement changes and therefore no re-negotiation
             and no link down.

      Change: Fixed logic so that link will always go down whenever
              there is a change a flow control advertisement.

      Impact: None.

   2. Problem: (CQTO612) VLAN packet reception not working.

      Cause: VLAN #define not setup properly.

      Change: Fixed #define for VLAN.

      Impact: None.

   3. Problem: (CQTO628) WoL not functioning correctly.

      Cause: Multiple problems in the WoL code.

      Change: Fixed by:
                 1. using sort mode.
                 2. setting up mac address correctly.

      Impact: None.

   Enhancements:
   -------------
   1. Change: Added support for non-dword and non-aligned write access
              to eeprom, allowing ethtool -E to work.

      Impact: None.

v1.0.11 (Sep. 24, 2004)
======================
   Fixes:
   ------
   1. Problem: (CQTO600) Kernel panic when attempting to ftp on
               Fedora kernel.

      Cause: skbuffs are 4-byte aligned on Fedora, causing
             the rx headers to be misaligned. skbuffs are
             16-byte aligned on other standard kernels.

      Change: Removed any assumptions about skbuff alignment
              and added code to align all rx skbuffs to 8-byte
              boundaries.

      Impact: None.

   Enhancements:
   -------------
   1. Change: Added netif_carrier_off to Driver init code so that
              the initial link state is off.

      Impact: None.

v1.0.10 (Sep. 23, 2004)
======================
   Fixes:
   ------
   1. Problem: (CQTO599) Driver fails to compile on RH 3.0ES.

      Cause: Bug in poll_bcm5706 where bp is referenced without
             being defined.

      Change: Fixed the minor bug.

      Impact: None.

v1.0.9 (Sep. 23, 2004)
======================
   Fixes:
   ------
   1. Problem: Jumbo frames not working reliably.

      Cause: Bug in bcm5706_reuse_rx_skb.

      Change: Fixed the bug so that the host address is properly
              copied from one BD to the other.

      Impact: None.

   Enhancements:
   -------------
   1. Change: Change the locking scheme for more reliable open/close/ioctl
              operations where the spinlock is needed.

      Impact: None.

   2. Change: Added minimum MTU size check for MTU changes.

      Impact: None.

v1.0.8 (Sep. 20, 2004)
======================
   Fixes:
   ------
   1. Problem: (CQTO561) Kernel panic on RH30EL after repeated
               driver load/unload.

      Cause: Occasionally, the system is unable to map device
             registers, causing subsequent register access to fail.

      Change: Added check for the return value from ioremap, and exit
              gracefully if it fails.

      Impact: None.

   2. Problem: (CQTO574) NETDEV WATCHDOG when running 5706 A1 on
               PCIX 133MHz slot.

      Cause: Some hw register setup required for 133 Mhz.

      Change: Added the register setup code.

      Impact: None.

   3. Problem: (CQTO468) Link does not go down after changing from
               10Mbps full (forced) to 10Mbps half (forced) and vice versa
               when the link partner is also using forced speed. 

      Cause: Delay not long enough for the link to go down.

      Change: Not practical to increase delay as a very long delay is
              needed for the link to go down. Added code to record the
              proper link speed and duplex when speed is forced so that
              ethtool will return the proper speed without the link going
              down. Note that the link will go down if the link partner
              has autoneg turned on, ensuring that the link partner will
              see the link change.

      Impact: None.

   Enhancements:
   -------------
   1. Change: Added power management and WOL during device close. This
              will allow WOL to work after Linux shutdown.

      Impact: None.

   2. Change: Changed driver so that ethtool will report invalid
              speed after ifdown.

      Impact: None.

   3. Change: Updated tpatfw.h

      Impact: None.

v1.0.7 (Sep. 14, 2004)
======================
   Fixes:
   ------
   1. Problem: (CQTO523) 5706 A1 hangs after a thousand iterations of
               load/ifup/ifdown/unload.

      Cause: The driver may be servicing an interrupt
             within 15 msec of chip reset, causing the chip to hang.
             The problem was aggravated by the timer mode
             coalescing which created an excessive number of
             interrupts (hardware problem).

             The Driver may also occasionally see
             the wrong firmware signature that will cause it to abort.

      Change: Added synchronization to make sure all pending interrupts
              are serviced before resetting the chip. Also changed to
              collect mode coalescing. The firmware signature problem
              will be fixed in boot code.

      Impact: The use of collect mode coalescing may affect performance.

   2. Problem: (CQTO558) Unable to load driver on some early 2.6 kernels.

      Cause: pci_dma_sync_single_for_* routines not defined on early
             2.6 kernels.

      Change: Added compatibility defines for earlier kernels.

      Impact: None.

v1.0.6 (Sep. 08, 2004)
======================
   Fixes:
   ------
   1. Problem: (CQTO523) 5706 A1 hangs during repeated driver ifup/down. 

      Cause: No delay after chip reset for A1.

      Change: Added 15 msec delay after chip reset for A1.

      Impact: None.

   2. Problem: (CQTO468) Link does not go down after changing from
               10Mbps full (forced) to 10Mbps half (forced) and vice versa. 

      Cause: Not enough delay after forcing link down.

      Change: Added proper delay for link to go down.

      Impact: None.

v1.0.5 (Sep. 02, 2004)
======================
   Enhancements:
   -------------
   1. Change: Added support for ethtool -c, ethtool -C, ethtool -p,
              and firmware version for ethtool -i.

      Impact: None.

   Fixes:
   ------
   1. Problem: 5706C not advertising 1000 half duplex.

      Cause: 1000 full duplex overwrites 1000 half duplex.

      Change: Fixed the bug so that the 2 bits are or'ed together.

      Impact: None.

    2. Problem: ethtool -A does not change the flow control settings
                in all cases.

       Cause: Flow control settings not zeroed out before setting new
              values.

       Change: Minor bug fix to zero out the value.

       Impact: None.

v1.0.4 (Sep. 02, 2004)
======================
   Fixes:
   ------
   1. Problem: (CQTO504) Multiple NFS transfers will hang some
               connections.

      Cause: Driver discards some receive packets when the
             error status is non-zero.

      Change: Changed the driver to only discard receive packets
              when the defined error bits in the error status are
              non-zero.

      Impact: None.

v1.0.3 (Sep. 01, 2004)
======================
   Enhancements:
   -------------
   1. Problem: Driver does not support ethtool -t self test and
               ethtool -S statistics.

      Change: Added ethtool self test and statistics.

      Impact: None.

   Fixes:
   ------
   1. Problem: (CQTO478) Kernel still panics when transmitting certain
               files using NFS after many iterations

      Cause: Tx DMA stalls on certain UDP packets, causing NFS
             client to stall.

      Change: More fixes made in firmware.

      Impact: None.

v1.0.2 (Aug. 26, 2004)
======================
   Enhancements:
   -------------
   1. Problem: Driver does not work on big endian machines.

      Change: Ported and tested on SPARC64 machine.

      Impact: None.

   Fixes:
   ------
   1. Problem: (CQTO478) Kernel panics when transmitting certain
               files using NFS.

      Cause: Tx DMA stalls on certain UDP packets, causing NFS
             client to stall.

      Change: Fixed in firmware.

      Impact: None.

   2. Problem: (CQTO469) Unable to modify flow control parameters

      Cause: Did not call setup_phy after the parameters are changed.

      Change: Added call to setup_phy after parameters are changed.

      Impact: None.

   3. Problem: (CQTO467) 5706 does not autonegotiate properly after
               changing settings with ethtool.

      Cause: This is an ethtool limitation as the proper advertising
             parameters are not passed to the driver properly.

      Change: Implemented a new scheme to work around the problem to
              allow users to specify full autoneg, single speed autoneg,
              and fixed speed.

      Impact: None.

   4. Problem: ethtool -e does not work.

      Cause: Various bugs in the nvram routines.

      Change: Fixed and tested nvram routines on little endian and big endian
              machines.

      Impact: None.

v1.0.1 (Aug. 18, 2004)
======================
   Fixes:
   ------
   1. Problem: (CQTO459) 5706 NIC does not get link.

      Cause: Boot code timing out in WAIT2 state before driver is ready.

      Change: Moved the WAIT2 state ahead in the driver reset sequence
              as a temporary workaround until it is fixed in boot code.

      Impact: None.

   2. Problem: (CQTO463) Kernel panics when loading the driver on
               RH30EL (2.4.21-4.EL)

      Cause: Older kernel used different API to allocate and register
             netdev.

      Change: Added older APIs to be used on older kernels.

      Impact: None.

v1.0.0 (Aug. 13, 2004)
======================
    Initial release
