Chronograph
-----------

Time offset adjustable with bottom left button, LMB change minutes, MMB change
hours.*
The time offset will be saved between two Flightgear sessions.

At start the second hand is locked on zero. Click on the upper right button
starts the second hand and a chronometer minutes hand. Click again on the
upper right button stops the chronometer. Click again resets the chronometer
to zero.


Setting up :
------------

- Include the model in your model file.

  <model> 
    <path>Aircraft/Instruments-3d/chronograph/chronograph.xml</path>
    <offsets> 
      <x-m>xxx</x-m>
      <y-m>xxx</y-m>
      <z-m>xxx</z-m>
    </offsets>
  </model>


- Declare chronograph.nas in your foo-set.xml file. Write something like:
  </nasal>
    <chronograph>
      <file>Aircraft/foo/Nasal/chronograph.nas</file>
    </chronograph>
  </nasal>


- Open chronograph.nas and uncomment chrono_loop() and the following settimer()
if update_chrono() has to be launched standalone.
Otherwise launch foo_chronograph.update_chrono() from a centralized loop which
will save some CPU cycles.
See chronograph.nas line 48.

That's it.


* LMB Left Mouse Button, MMB midle mouse button.
