<PropertyList>
	<name>Instruments description</name>
	<description>
This tutorial describes the differents instruments
	</description>

	<timeofday>noon</timeofday>
  
	<init>
		<set>
			<property>/controls/gear/brake-parking</property>
			<value>1</value>
		</set>
		<set>
			<property>/controls/flight/flaps</property>
			<value>0.0</value>
		</set>
		<set>
			<property>/controls/switches/battery-click</property>
			<value>1.0</value>
		</set>
		<set>
			<property>/controls/switches/light_cabin-click</property>
			<value>1.0</value>
		</set>
		<set>
			<property>/sim/panel-hotspots</property>
			<value>0</value>
		</set>
	</init>
  
	<step>
		<message>In this lesson, you will learn the position and the functionnement of the instruments.</message>
	</step>
	
	<step>
		<message>At all moment, you can see the hotspots with the Ctrl-C shortcut, do it now !!!</message>
		<exit>
			<condition>
				<equals>
					<property>/sim/panel-hotspots</property>
					<value>true</value>
				</equals>
			</condition>
		</exit>
	</step>

	<step>
		<message>On the left of the pilot chair, you can see two commands, one is the rudder trim.
It's activable by joystick or by clicking on it.</message>
		<view>
			<heading-offset-deg>90.45</heading-offset-deg>
			<pitch-offset-deg>-77.1</pitch-offset-deg>
			<x-offset-m>-0.3159</x-offset-m>
			<y-offset-m>0.688</y-offset-m>
			<z-offset-m>3.7</z-offset-m>
			<field-of-view>10.38</field-of-view>
		</view>
	</step>
	
	<step>
		<message>Near the rudder trim, you can see the tail wheel lock. Click on it to unlock the tail wheel.</message>
		<view>
			<heading-offset-deg>69.3</heading-offset-deg>
			<pitch-offset-deg>-73.8</pitch-offset-deg>
			<x-offset-m>-0.2736</x-offset-m>
			<y-offset-m>0.688</y-offset-m>
			<z-offset-m>3.7</z-offset-m>
			<field-of-view>12.25</field-of-view>
		</view>
		<exit>
			<condition>
				<equals>
					<property>controls/gear/tailwheel-lock</property>
					<value>0</value>
				</equals>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>Here, you can see the main fuel valve.
You can see the left circuit breakers panel, all the breakers are clickable...</message>
		<view>
			<heading-offset-deg>25.2</heading-offset-deg>
			<pitch-offset-deg>-50.4</pitch-offset-deg>
			<x-offset-m>-0.265</x-offset-m>
			<y-offset-m>0.688</y-offset-m>
			<z-offset-m>3.7</z-offset-m>
			<field-of-view>27.9</field-of-view>
		</view>
	</step>
	
	<step>
		<message>Here is the annunciators test, click on it</message>
		<view>
			<heading-offset-deg>28.8</heading-offset-deg>
			<pitch-offset-deg>-55.8</pitch-offset-deg>
			<x-offset-m>-0.265</x-offset-m>
			<y-offset-m>0.688</y-offset-m>
			<z-offset-m>3.7</z-offset-m>
			<field-of-view>16.11</field-of-view>
		</view>
		<exit>
			<condition>
				<equals>
					<property>/sim/alarms/annunciator.test</property>
					<value>1</value>
				</equals>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>This action light up the annunciator panel for 5 seconds</message>
		<view>
			<heading-offset-deg>349.2</heading-offset-deg>
			<pitch-offset-deg>-20.7</pitch-offset-deg>

			<x-offset-m>-0.265</x-offset-m>
			<y-offset-m>0.688</y-offset-m>
			<z-offset-m>3.7</z-offset-m>
			<field-of-view>28.41</field-of-view>
		</view>
	</step>
	
	<step>
		<message>On the left side, you can see the electrical panel switches.</message>
		<view>
			<heading-offset-deg>23.4</heading-offset-deg>
			<pitch-offset-deg>-28.8</pitch-offset-deg>
			<x-offset-m>-0.265</x-offset-m>
			<y-offset-m>0.688</y-offset-m>
			<z-offset-m>3.7</z-offset-m>
			<field-of-view>15.25</field-of-view>
		</view>
	</step>

	<step>
		<message>On the first line, you have :
The battery switch
The alternator switch
The alternator reset switch
The auxiliary fuel pump switch
The ignition  switch
The starter switch
The 0V test switch
</message>
	</step>
	
	<step>
		<message>On the second line, you have :
The strobe light switch
The position light switch
The beacon light switch
The left landing light switch
The left landing position light switch
The right landing position light switch
The right landing light switch
</message>
	</step>
	
	<step>
		 <message>Click on the beacon switch.</message>
		<exit>
			<condition>
				<equals>
					<property>/controls/switches/light_beacon-click</property>
					<value>1</value>
				</equals>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>On the third line, you have :
The instrument lights knob
The instrument lights switch
The cabin light switch</message>
	</step>

	<step>
		<message>You can see and change the radio call.
You can see the stall warning, click on it to test it</message>
		<view>
			<heading-offset-deg>15.3</heading-offset-deg>
			<pitch-offset-deg>-19.5</pitch-offset-deg>
			<x-offset-m>-0.265</x-offset-m>
			<y-offset-m>0.688</y-offset-m>
			<z-offset-m>3.7</z-offset-m>
			<field-of-view>15.25</field-of-view>
		</view>
		<exit>
			<condition>
				<equals>
					<property>/sim/alarms/stall-warning</property>
					<value>0</value>
				</equals>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>Here, you can see the elevator trim indicator.</message>
		<view>
			<field-of-view>9.5</field-of-view>
			<heading-offset-deg>17</heading-offset-deg>
			<pitch-offset-deg>-22.28</pitch-offset-deg>

			<x-offset-m>-0.265</x-offset-m>
			<y-offset-m>0.688</y-offset-m>
			<z-offset-m>3.7</z-offset-m>
		</view>
	</step>
	
	<step>
		<message>From left to right, you can see :
The airspeed indicator
The attitude indicator
The altimeter (in ft)</message>
		<view>
			<field-of-view>27.95</field-of-view>
			<heading-offset-deg>1.48</heading-offset-deg>
			<pitch-offset-deg>-14.68</pitch-offset-deg>

			<x-offset-m>-0.265</x-offset-m>
			<y-offset-m>0.688</y-offset-m>
			<z-offset-m>3.7</z-offset-m>
		</view>
	</step>
	
	<step>
		<message>On top of it, you have the warning and the caution warning light.
Click on the caution light to switch off it.</message>
		<exit>
			<condition>
				<equals>
					<property>/sim/alarms/caution-warning</property>
					<value>0</value>
				</equals>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>From left to right, you can see :
The turn and bank indicator
The gyro-compas indicator
The vertical speed indicator</message>
		<view>
			<field-of-view>27.95</field-of-view>
			<heading-offset-deg>1.76</heading-offset-deg>
			<pitch-offset-deg>-30.07</pitch-offset-deg>
			<x-offset-m>-0.265</x-offset-m>
			<y-offset-m>0.688</y-offset-m>
			<z-offset-m>3.7</z-offset-m>
		</view>
	</step>
	
	<step>
		<message>And below it, 
A gps
An altimeter in meter (a skydiver altimeter)</message>
	</step>
  
	<step>
		<message>Here is the magnetic compass</message>
		<view>
			<field-of-view>27.95</field-of-view>
			<heading-offset-deg>335.8</heading-offset-deg>
			<pitch-offset-deg>-7.08</pitch-offset-deg>
			<x-offset-m>-0.265</x-offset-m>
			<y-offset-m>0.688</y-offset-m>
			<z-offset-m>3.7</z-offset-m>
		</view>
	</step>
	
	<step>
		<message>Here is the engine indicators :
The torque indicator
The ITT (Inter turbine Temperature) indicator
The propeller RPM indicator
The turbine RPM indicator (in %)
The fuel flow indicator
The oil temperature and pressure indicator	</message>
		<view>
			<field-of-view>21.15</field-of-view>
			<heading-offset-deg>345.04</heading-offset-deg>
			<pitch-offset-deg>-19</pitch-offset-deg>
			<x-offset-m>-0.265</x-offset-m>
			<y-offset-m>0.688</y-offset-m>
			<z-offset-m>3.7</z-offset-m>
		</view>
	</step>
	
	<step>
		<message>There, you can see the annunciators panel
and at the first plan, the levers, from left to right
the feather lever
the power lever
the condition (fuel control) lever</message>
		<view>
			<field-of-view>18.93</field-of-view>
			<heading-offset-deg>342.85</heading-offset-deg>
			<pitch-offset-deg>-31.73</pitch-offset-deg>
			<x-offset-m>-0.265</x-offset-m>
			<y-offset-m>0.688</y-offset-m>
			<z-offset-m>3.7</z-offset-m>
		</view>
	</step>	
	
	<step>
		<message>On the right, you have an ELT
and on the bottom, the parking brake, click on it</message>
		<view>
			<field-of-view>11.76</field-of-view>
			<heading-offset-deg>333.82</heading-offset-deg>
			<pitch-offset-deg>-27.1</pitch-offset-deg>
			<x-offset-m>-0.265</x-offset-m>
			<y-offset-m>0.688</y-offset-m>
			<z-offset-m>3.7</z-offset-m>
		</view>
		<exit>
			<condition>
				<equals>
					<property>/controls/gear/brake-parking</property>
					<value>0</value>
				</equals>
			</condition>
		</exit>
	</step>	
	
	<step>
		<message>There is 3 knob, the first on the left controls the oil temperature.
The 2 others control the cabin temperature</message>
		<view>
			<field-of-view>13.98</field-of-view>
			<heading-offset-deg>321.98</heading-offset-deg>
			<pitch-offset-deg>-13.01</pitch-offset-deg>
			<x-offset-m>-0.265</x-offset-m>
			<y-offset-m>0.688</y-offset-m>
			<z-offset-m>3.7</z-offset-m>
		</view>
	</step>	
	
	<step>
		<message>In the middle, you can see
The fuel used indicator
The fuel quantity in the to tanks
The ammeter and the voltemeter</message>
	</step>	
	
	<step>
		<message>Here is some switches, two control the electricity alimentation of the radio stack.
The ICS button is used by the copilot to speak with the pilot...</message>
		<view>
			<field-of-view>13.39</field-of-view>
			<heading-offset-deg>319.15</heading-offset-deg>
			<pitch-offset-deg>-22.65</pitch-offset-deg>
			<x-offset-m>-0.265</x-offset-m>
			<y-offset-m>0.688</y-offset-m>
			<z-offset-m>3.7</z-offset-m>
		</view>
	</step>
	
	<step>
		<message>Here is the alternate elevator trim command. The primary command is bound on the joystick</message>
		<view>
			<field-of-view>13.39</field-of-view>
			<heading-offset-deg>326.36</heading-offset-deg>
			<pitch-offset-deg>-30.25</pitch-offset-deg>
			<x-offset-m>-0.265</x-offset-m>
			<y-offset-m>0.688</y-offset-m>
			<z-offset-m>3.7</z-offset-m>
		</view>
	</step>
	
	<step>
		<message>Here is the right circuit breakers panel, which controls radio instruments.</message>
		<view>
			<field-of-view>15.92</field-of-view>
			<heading-offset-deg>306.46</heading-offset-deg>
			<pitch-offset-deg>-36.74</pitch-offset-deg>
			<x-offset-m>-0.265</x-offset-m>
			<y-offset-m>0.688</y-offset-m>
			<z-offset-m>3.7</z-offset-m>
		</view>
	</step>
	
	<step>
		<message>This knob controls the ailerons trim.</message>
		<view>
			<field-of-view>27.41</field-of-view>
			<heading-offset-deg>253.92</heading-offset-deg>
			<pitch-offset-deg>28.65</pitch-offset-deg>
			<x-offset-m>-0.265</x-offset-m>
			<y-offset-m>0.688</y-offset-m>
			<z-offset-m>3.7</z-offset-m>
		</view>
	</step>
	
	<step>
		<message>And this controls the flaps : 4 turn for take off and 11 for landing.</message>
		<view>
			<field-of-view>62.35</field-of-view>
			<heading-offset-deg>249.12</heading-offset-deg>
			<pitch-offset-deg>50.15</pitch-offset-deg>
			<x-offset-m>-0.265</x-offset-m>
			<y-offset-m>0.688</y-offset-m>
			<z-offset-m>3.7</z-offset-m>
		</view>
	</step>
	

	
	<end>
		<message>You now know the instruments functions, you're ready to fly.</message>
	</end>
</PropertyList>
