## Description

This track depicts gaps in the assembly.

Gaps are represented as black boxes in this track. If the relative order and orientation of the contigs on either side of the gap is supported by read pair data, it is a bridged gap and a white line is drawn through the black box representing the gap.

This assembly contains the following principal types of gaps:

- Contig - gaps of size 50 Kb or fewer.
- Scaffold - gaps greater then 50 Kb in size.