<PropertyList>
  <name>Engine Prestart Check</name>
  <description>This tutorial teaches the EC130/H130 Engine Prestart Check procedure</description>

  <init>
    <set>
      <property>/sim/current-view/view-number</property>
      <value>0</value>
    </set>
  </init>

  <step>
    <view>
    </view>

    <marker>
    </marker>

    <message>

      Make sure you have enough fuel.
      If necessary fill up tank (Alt-o) ...

    </message>
    <exit>
      <condition>
        <greater-than>
         <property>/consumables/fuel/tank/level-lbs</property>
         <value>106</value>
        </greater-than>
      </condition>
    </exit>
  </step>

  <step>
    <view>
      <heading-offset-deg>299.8</heading-offset-deg>
      <pitch-offset-deg>4.1</pitch-offset-deg>
      <roll-offset-deg>0.0</roll-offset-deg>
      <x-offset-m>-0.7</x-offset-m>
      <y-offset-m>0.0</y-offset-m>
      <z-offset-m>-3.9</z-offset-m>
      <field-of-view>65</field-of-view>
    </view>

    <marker>
      <x-m>-4.1175</x-m>
      <y-m>-0.1851</y-m>
      <z-m>0.1300</z-m>
      <scale>6.000</scale>
    </marker>

    <message>

      Release Rotorbrake (Alt-r), push the Lever forward and lock Rotorbrake again:
      Move Lever: point and drag with LMB pressed or (Shift-R)

    </message>
    <exit>
      <condition>
      <less-than>
        <property>/controls/rotor/brake</property>
        <value>0.1</value>
      </less-than>
      <property>/controls/rotor/brake-locked</property>
      </condition>
    </exit>
  </step>

  <step>
    <view>
      <heading-offset-deg>292.8</heading-offset-deg>
      <pitch-offset-deg>15.8</pitch-offset-deg>
      <roll-offset-deg>0.0</roll-offset-deg>
      <x-offset-m>-0.7</x-offset-m>
      <y-offset-m>0.0</y-offset-m>
      <z-offset-m>-3.9</z-offset-m>
      <field-of-view>37.1</field-of-view>
    </view>

    <marker>
      <x-m>-4.0788</x-m>
      <y-m>-0.2</y-m>
      <z-m>0.1970</z-m>
      <scale>3.500</scale>
    </marker>

    <message>
    -
    Push the Cutoff lever forward (Alt-c)
    apply Guard (AltGr-c)

    </message>
    <exit>
      <condition>
      <less-than>
        <property>/controls/engines/engine/cutoff</property>
        <value>0.1</value>
      </less-than>
      <property>/controls/engines/engine/cutoffguard</property>
      </condition>
    </exit>
  </step>

  <step>
    <view>
      <heading-offset-deg>4.5</heading-offset-deg>
      <pitch-offset-deg>-13.1</pitch-offset-deg>
      <roll-offset-deg>0.0</roll-offset-deg>
      <x-offset-m>-0.67</x-offset-m>
      <y-offset-m>0.03</y-offset-m>
      <z-offset-m>-3.93</z-offset-m>
      <field-of-view>40</field-of-view>
    </view>

    <message>
      -
      The fuel tank is below the engine - due to gravitity fuellines are empty.
      You need electric power "EC130"-Menu "Toggle External Power" (Alt-p)

    </message>

    <exit>
      <condition>
        <property>/controls/electric/external-power</property>
      </condition>
    </exit>
  </step>

  <step>
    <message>
      -
      switch on "BAT EPU" and "GENE"

    </message>
    <view>
      <heading-offset-deg>323.3</heading-offset-deg>
      <pitch-offset-deg>-51.6</pitch-offset-deg>
      <roll-offset-deg>0.0</roll-offset-deg>
      <x-offset-m>-0.7</x-offset-m>
      <y-offset-m>0.0</y-offset-m>
      <z-offset-m>-3.9</z-offset-m>
      <field-of-view>35.5</field-of-view>
    </view>

    <marker>
      <x-m>-4.3555</x-m>
      <y-m>-0.4008</y-m>
      <z-m>-0.6626</z-m>
      <scale>4.0000</scale>
    </marker>

    <exit>
      <condition>
        <property>/controls/electric/battery-switch</property>
        <property>/controls/electric/engine/generator</property>
      </condition>
    </exit>
  </step>

  <wait>5</wait>

  <step>
    <view>
      <heading-offset-deg>332.00</heading-offset-deg>
      <pitch-offset-deg>-21.7</pitch-offset-deg>
      <field-of-view>35.5</field-of-view>
    </view>
    <message>
      -
      On VEMD you should see the Engine start page, after a testing phase- 3 arcs with Torque, Ng (aka N2) and T4.
      -
      Continue with "Engine Starting Tutorial"
      -
    </message>
  </step>

  <wait>10</wait>

  <end>
  </end>
</PropertyList>
