<PropertyList>
  <name>Run Up and Before Takeoff Tutorial</name>
  <description>This tutorial teaches the EC130 B4 Run Up and Before Takeoff  procedure</description>

  <init>
    <set>
      <property>/sim/current-view/view-number</property>
      <value>0</value>
    </set>
  </init>

  <step>
    <view>
      <heading-offset-deg>29</heading-offset-deg>
      <pitch-offset-deg>-69.5</pitch-offset-deg>
      <roll-offset-deg>0.0</roll-offset-deg>
      <x-offset-m>-0.67</x-offset-m>
      <y-offset-m>0.03</y-offset-m>
      <z-offset-m>-3.93</z-offset-m>
      <field-of-view>37</field-of-view>
    </view>

    <message>
      Set Engine State to "Flight" (100%) by dragging the mouse up with MMB pressed or
      by Twist Grip animation on Collective or (Alt-t repeated).
    </message>
    <error>
      <message>Twist Grip not set to Flight!</message>
      <condition>
        <less-than>
          <property>/controls/engines/engine/power</property>
          <value>0.99</value>
        </less-than>
      </condition>
    </error>
    <exit>
      <condition>
      <greater-than>
        <property>/controls/engines/engine/power</property>
        <value>0.99</value>
      </greater-than>
      </condition>
    </exit>
  </step>

  <step>
    <view>
      <heading-offset-deg>322</heading-offset-deg>
      <pitch-offset-deg>-57.2</pitch-offset-deg>
      <roll-offset-deg>0.0</roll-offset-deg>
      <x-offset-m>-0.7</x-offset-m>
      <y-offset-m>0.0</y-offset-m>
      <z-offset-m>-3.9</z-offset-m>
      <field-of-view>32.7</field-of-view>
    </view>

    <marker>
      <x-m>-4.3322</x-m>
      <y-m>-0.4017</y-m>
      <z-m>-0.6669</z-m>
      <scale>1.8000</scale>
    </marker>

    <message>
      -
      "AVIONIC"  On

    </message>
    <exit>
      <condition>
        <property>/controls/electric/avionics-switch</property>
      </condition>
    </exit>
  </step>

  <step>
    <view>
      <heading-offset-deg>332</heading-offset-deg>
      <pitch-offset-deg>-54.2</pitch-offset-deg>
      <roll-offset-deg>0.0</roll-offset-deg>
      <x-offset-m>-0.7</x-offset-m>
      <y-offset-m>0.0</y-offset-m>
      <z-offset-m>-3.9</z-offset-m>
      <field-of-view>32.7</field-of-view>
    </view>

    <marker>
      <x-m>-4.3570</x-m>
      <y-m>-0.3248</y-m>
      <z-m>-0.6669</z-m>
      <scale>1.80000</scale>
    </marker>

    <message>
      -
      "HORN"  On (Alt-h) - sounds if rotor rpm is &lt;360

    </message>
    <exit>
      <condition>
        <property>/controls/electric/horn</property>
      </condition>
    </exit>
  </step>

  <step>
    <view>
      <heading-offset-deg>322.2</heading-offset-deg>
      <pitch-offset-deg>-55.2</pitch-offset-deg>
      <roll-offset-deg>0.0</roll-offset-deg>
      <x-offset-m>-0.7</x-offset-m>
      <y-offset-m>0.0</y-offset-m>
      <z-offset-m>-3.9</z-offset-m>
      <field-of-view>32.7</field-of-view>
    </view>

    <marker>
      <x-m>-4.3074</x-m>
      <y-m>-0.3248</y-m>
      <z-m>-0.6719</z-m>
      <scale>1.8000</scale>
    </marker>

    <message>
      -
      "GYRO"  On

    </message>
    <exit>
      <condition>
        <property>/controls/electric/gyrocompass</property>
      </condition>
    </exit>
  </step>

  <step>
    <view>
      <heading-offset-deg>322.2</heading-offset-deg>
      <pitch-offset-deg>-55.2</pitch-offset-deg>
      <roll-offset-deg>0.0</roll-offset-deg>
      <x-offset-m>-0.7</x-offset-m>
      <y-offset-m>0.0</y-offset-m>
      <z-offset-m>-3.9</z-offset-m>
      <field-of-view>32.7</field-of-view>
    </view>

    <marker>
      <x-m>-4.3074</x-m>
      <y-m>-0.3512</y-m>
      <z-m>-0.6719</z-m>
      <scale>1.8</scale>
    </marker>

    <message>
      -
      "HORIZON"  On

    </message>
    <exit>
      <condition>
        <property>/instrumentation/attitude-indicator/serviceable</property>
      </condition>
    </exit>
  </step>

  <step>
    <view>
      <heading-offset-deg>322.2</heading-offset-deg>
      <pitch-offset-deg>-55.2</pitch-offset-deg>
      <roll-offset-deg>0.0</roll-offset-deg>
      <x-offset-m>-0.7</x-offset-m>
      <y-offset-m>0.0</y-offset-m>
      <z-offset-m>-3.9</z-offset-m>
      <field-of-view>32.7</field-of-view>
    </view>

    <marker>
      <x-m>-4.3074</x-m>
      <y-m>-0.3760</y-m>
      <z-m>-0.6719</z-m>
      <scale>1.8</scale>
    </marker>

    <message>
      -
      "PITOTS"  On

    </message>
    <exit>
      <condition>
        <property>/controls/anti-ice/pitot-heat</property>
      </condition>
    </exit>
  </step>

  <step>
    <view>
      <heading-offset-deg>322.2</heading-offset-deg>
      <pitch-offset-deg>-57.2</pitch-offset-deg>
      <roll-offset-deg>0.0</roll-offset-deg>
      <x-offset-m>-0.7</x-offset-m>
      <y-offset-m>0.0</y-offset-m>
      <z-offset-m>-3.9</z-offset-m>
      <field-of-view>32.7</field-of-view>
    </view>

    <marker>
      <x-m>-4.3074</x-m>
      <y-m>-0.4149</y-m>
      <z-m>-0.6769</z-m>
      <scale>2.8</scale>
    </marker>

    <message>
      -
      "INST L1"  On
      "INST L2"  On

    </message>
    <exit>
      <condition>
        <property>/controls/lighting/instrument-lights</property>
        <property>/controls/lighting/instrument-lights2</property>
      </condition>
    </exit>
  </step>

  <step>
    <view>
      <heading-offset-deg>322.2</heading-offset-deg>
      <pitch-offset-deg>-57.2</pitch-offset-deg>
      <roll-offset-deg>0.0</roll-offset-deg>
      <x-offset-m>-0.7</x-offset-m>
      <y-offset-m>0.0</y-offset-m>
      <z-offset-m>-3.9</z-offset-m>
      <field-of-view>32.7</field-of-view>
    </view>

    <marker>
      <x-m>-4.3280</x-m>
      <y-m>-0.3248</y-m>
      <z-m>-0.6680</z-m>
      <scale>1.8</scale>
    </marker>

    <message>
      -
      "POS LT"  On

    </message>
    <exit>
      <condition>
        <property>/controls/lighting/nav-lights</property>
      </condition>
    </exit>
  </step>

  <step>
    <view>
      <heading-offset-deg>322.2</heading-offset-deg>
      <pitch-offset-deg>-57.2</pitch-offset-deg>
      <roll-offset-deg>0.0</roll-offset-deg>
      <x-offset-m>-0.7</x-offset-m>
      <y-offset-m>0.0</y-offset-m>
      <z-offset-m>-3.9</z-offset-m>
      <field-of-view>32.7</field-of-view>
    </view>

    <marker>
      <x-m>-4.2834</x-m>
      <y-m>-0.3017</y-m>
      <z-m>-0.6776</z-m>
      <scale>1.8</scale>
    </marker>

    <message>
      -
      only if equipped with emergency floats:
      -
      "FLOAT ARM"  On

    </message>
    <exit>
      <condition>

      </condition>
    </exit>
  </step>

  <wait>10</wait>

  <step>
    <message>
      -
      Ready! You are cleared for Takeoff!
      -
    </message>
    <view>
      <heading-offset-deg>0</heading-offset-deg>
      <pitch-offset-deg>-9</pitch-offset-deg>
      <field-of-view>55</field-of-view>
    </view>
  </step>

  <wait>5</wait>

  <end>
  </end>

</PropertyList>
