<PropertyList>
	<name>Engine Starting Tutorial</name>
	<description>This tutorial teaches the EC130 B4 engine starting Check procedure</description>

	<init>
		<set>
			<property>/sim/current-view/view-number</property>
			<value>0</value>
		</set>
		
		
	</init>

	<step>
		<view>
			<heading-offset-deg>317.3</heading-offset-deg>
			<pitch-offset-deg>-49.1</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.7</x-offset-m>
			<y-offset-m>0.0</y-offset-m>
			<z-offset-m>-3.9</z-offset-m>
			<field-of-view>26.2</field-of-view>
		</view>

		<marker>
			<x-m>-4.3331</x-m>
			<y-m>-0.3124</y-m>
			<z-m>-0.6702</z-m>
			<scale>4.0000</scale>
		</marker>

		<message>
		A/Col-Light: On
		Press Fuel P button.
		It needs about 30 sec. On the real thing you don't see any effect. 
		On this model the FUEL-P sign on the warning panel may dissapear.
		</message>
		<error>
			<message>You have to wait at least 30sec for the fuelpump to fill up the lines!</message>
			<condition>
				<less-than>
					<property>/controls/fuel/tank/fuellines_filled</property>
					<value>0.99</value>
				</less-than>
			</condition>
		</error>
		<exit>
			<condition>
			<and>
			<greater-than>
				<property>/controls/fuel/tank/fuellines_filled</property>
			<value>0.98</value>
			</greater-than>
			<property>/controls/lighting/beacon</property>
			</and>
			</condition>
		</exit>
	</step>
	
	
	<step>
		<view>
			<heading-offset-deg>326.9</heading-offset-deg>
			<pitch-offset-deg>-37.2</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.7</x-offset-m>
			<y-offset-m>0.0</y-offset-m>
			<z-offset-m>-3.9</z-offset-m>
			<field-of-view>32.6</field-of-view>
		</view>

		<marker>
			<x-m>-4-4892</x-m>
			<y-m>-0.3207</y-m>
			<z-m>-0.5174</z-m>
			<scale>2.0000</scale>
		</marker>

		<message>
		Open the guard and switch the Start Selector to "On"
		</message>
		<exit>
			<condition>
			<property>/controls/engines/engine/switchguard</property>
			<property>/controls/engines/engine/startselector</property>
			</condition>
		</exit>
	</step>
	

	
<step>
		<view>
			<heading-offset-deg>331.4</heading-offset-deg>
			<pitch-offset-deg>-22.8</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.7</x-offset-m>
			<y-offset-m>0.03</y-offset-m>
			<z-offset-m>-3.9</z-offset-m>
			<field-of-view>44.1</field-of-view>
		</view>

		

		<message>
		The engine will spool up now!
		</message>
		<exit>
			<condition>
			<greater-than>
			<property>/engines/engine/n2-pct</property>
			<value>66</value>
			</greater-than>
			</condition>
		</exit>
	</step>	
	
<step>
		<view>
			<heading-offset-deg>338</heading-offset-deg>
			<pitch-offset-deg>-33</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.67</x-offset-m>
			<y-offset-m>0.03</y-offset-m>
			<z-offset-m>-3.93</z-offset-m>
			<field-of-view>52.3</field-of-view>
		</view>

		

		<message>
		External power isn't needed anymore- deselect "Supply External Power" if needed
		</message>
		<exit>
			<condition>
			<not>
			<property>/controls/electric/external-power</property>
			</not>
			</condition>
		</exit>
	</step>
	
<step>
		<view>
			<heading-offset-deg>320</heading-offset-deg>
			<pitch-offset-deg>-46</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.7</x-offset-m>
			<y-offset-m>0.0</y-offset-m>
			<z-offset-m>-3.9</z-offset-m>
			<field-of-view>31</field-of-view>
		</view>

		<marker>
			<x-m>-4.3322</x-m>
			<y-m>-0.2992</y-m>
			<z-m>-0.6669</z-m>
			<scale>1.7</scale>
		</marker>

		<message>
		set Fuel P off
		
		Not needed anymore- the engines sucks now the fuel.
		</message>
		<exit>
			<condition>
			<not>
			<property>/controls/electric/external-power</property>
			</not>
			</condition>
		</exit>
	</step>
	
	

	<end>
		<message>
The engine is running in Idle now- but you can't fly yet!. </message>
		<view>
			<heading-offset-deg>347</heading-offset-deg>
			<pitch-offset-deg>-25</pitch-offset-deg>
			<field-of-view>55</field-of-view>
		</view>
	</end>
</PropertyList>
