<PropertyList>
	<name>Run Up and Before Takeoff Tutorial</name>
	<description>This tutorial teaches the EC130 B4 Run up and Before Takeoff  procedure</description>

	<init>
		<set>
			<property>/sim/current-view/view-number</property>
			<value>0</value>
		</set>
		
		
	</init>

	<step>
		<view>
			<heading-offset-deg>325</heading-offset-deg>
			<pitch-offset-deg>-55.5</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.67</x-offset-m>
			<y-offset-m>0.03</y-offset-m>
			<z-offset-m>-3.93</z-offset-m>
			<field-of-view>37</field-of-view>
		</view>

		
		<message>
		Set Engine State to "Flight" (100%) by dragging the mouse up with MMB pressed.</message>
		<error>
			<message>Twist Grip not set to Flight!</message>
			<condition>
				<less-than>
					<property>/controls/engines/engine/power</property>
					<value>0.99</value>
				</less-than>
			</condition>
		</error>
		<exit>
			<condition>
			<greater-than>
				<property>/controls/engines/engine/power</property>
					
			<value>0.99</value>
			</greater-than>
			</condition>
		</exit>
	</step>
	
	<step>
		<view>
			<heading-offset-deg>322</heading-offset-deg>
			<pitch-offset-deg>-57.2</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.7</x-offset-m>
			<y-offset-m>0.0</y-offset-m>
			<z-offset-m>-3.9</z-offset-m>
			<field-of-view>32.7</field-of-view>
		</view>

		<marker>
			<x-m>-4.3322</x-m>
			<y-m>-0.4017</y-m>
			<z-m>-0.6669</z-m>
			<scale>1.8000</scale>
		</marker>

		<message>
				    
		Avionic: On
		
		
		</message>
		<exit>
			<condition>
			<property>/controls/electric/avionics-switch</property>
			
			</condition>
		</exit>
	</step>
	
<step>
		<view>
			<heading-offset-deg>332</heading-offset-deg>
			<pitch-offset-deg>-57.2</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.7</x-offset-m>
			<y-offset-m>0.0</y-offset-m>
			<z-offset-m>-3.9</z-offset-m>
			<field-of-view>32.7</field-of-view>
		</view>

		<marker>
			<x-m>-4.3570</x-m>
			<y-m>-0.3248</y-m>
			<z-m>-0.6669</z-m>
			<scale>1.80000</scale>
		</marker>

		<message>
				    
		Horn: On 
		
		
		</message>
		<exit>
			<condition>
			<property>/controls/electric/horn</property>
			
			</condition>
		</exit>
	</step>
	
<step>
		<view>
			<heading-offset-deg>322.2</heading-offset-deg>
			<pitch-offset-deg>-57.2</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.7</x-offset-m>
			<y-offset-m>0.0</y-offset-m>
			<z-offset-m>-3.9</z-offset-m>
			<field-of-view>32.7</field-of-view>
		</view>

		<marker>
			<x-m>-4.3074</x-m>
			<y-m>-0.3248</y-m>
			<z-m>-0.6719</z-m>
			<scale>1.8000</scale>
		</marker>

		<message>
				    
		Gyro: On 
		
		
		</message>
		<exit>
			<condition>
			<property>/controls/electric/gyrocompass</property>
			
			</condition>
		</exit>
	</step>
	
<step>
		<view>
			<heading-offset-deg>322.2</heading-offset-deg>
			<pitch-offset-deg>-57.2</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.7</x-offset-m>
			<y-offset-m>0.0</y-offset-m>
			<z-offset-m>-3.9</z-offset-m>
			<field-of-view>32.7</field-of-view>
		</view>

		<marker>
			<x-m>-4.3074</x-m>
			<y-m>-0.3512</y-m>
			<z-m>-0.6719</z-m>
			<scale>1.8</scale>
		</marker>

		<message>
				    
		Horizon: On 
		
		
		</message>
		<exit>
			<condition>
			<property>/instrumentation/attitude-indicator/serviceable</property>
			</condition>
		</exit>
	</step>
	
<step>
		<view>
			<heading-offset-deg>322.2</heading-offset-deg>
			<pitch-offset-deg>-57.2</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.7</x-offset-m>
			<y-offset-m>0.0</y-offset-m>
			<z-offset-m>-3.9</z-offset-m>
			<field-of-view>32.7</field-of-view>
		</view>

		<marker>
			<x-m>-4.3074</x-m>
			<y-m>-0.3760</y-m>
			<z-m>-0.6719</z-m>
			<scale>1.8</scale>
		</marker>

		<message>
				    
		Pitots: On 
		
		
		</message>
		<exit>
			<condition>
			<property>/controls/anti-ice/pitot-heat</property>
			
			</condition>
		</exit>
	</step>
	
<step>
		<view>
			<heading-offset-deg>322.2</heading-offset-deg>
			<pitch-offset-deg>-57.2</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.7</x-offset-m>
			<y-offset-m>0.0</y-offset-m>
			<z-offset-m>-3.9</z-offset-m>
			<field-of-view>32.7</field-of-view>
		</view>

		<marker>
			<x-m>-4.3074</x-m>
			<y-m>-0.4149</y-m>
			<z-m>-0.6769</z-m>
			<scale>2.8</scale>
		</marker>

		<message>
				    
		INSTL 1: On 
		INSTL 2: On 
		
		
		</message>
		<exit>
			<condition>
			<property>/controls/lighting/instrument-lights</property>
			<property>/controls/lighting/instruments-lights2</property>
			</condition>
		</exit>
	</step>
	
<step>
		<view>
			<heading-offset-deg>322.2</heading-offset-deg>
			<pitch-offset-deg>-57.2</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.7</x-offset-m>
			<y-offset-m>0.0</y-offset-m>
			<z-offset-m>-3.9</z-offset-m>
			<field-of-view>32.7</field-of-view>
		</view>

		<marker>
			<x-m>-4.2950</x-m>
			<y-m>-0.3124</y-m>
			<z-m>-0.6769</z-m>
			<scale>5.2</scale>
		</marker>

		<message>
				    
		POS LT: On 
		
		
		
		</message>
		<exit>
			<condition>
			<property>/controls/lighting/nav-lights</property>
			</condition>
		</exit>
	</step>
	
<step>
		<view>
			<heading-offset-deg>322.2</heading-offset-deg>
			<pitch-offset-deg>-57.2</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.7</x-offset-m>
			<y-offset-m>0.0</y-offset-m>
			<z-offset-m>-3.9</z-offset-m>
			<field-of-view>32.7</field-of-view>
		</view>

		<marker>
			<x-m>-4.2834</x-m>
			<y-m>-0.3017</y-m>
			<z-m>-0.6776</z-m>
			<scale>1.8</scale>
		</marker>

		<message>
				    
		only If equipped with emergency floats: 
		FLOAT ARM: On 
		
		
		</message>
		<exit>
			<condition>
			
			</condition>
		</exit>
	</step>
	
	

	

	


	<end>
		<message>
Ready! You are cleared for Takeoff! </message>
		<view>
			<heading-offset-deg>0</heading-offset-deg>
			<pitch-offset-deg>-9</pitch-offset-deg>
			<field-of-view>55</field-of-view>
		</view>
	</end>
</PropertyList>
