<PropertyList>
	<name>Engine Prestart Check</name>
	<description>This tutorial teaches the EC130 B4 engine Prestart Check procedure</description>

	<init>
		<set>
			<property>/sim/current-view/view-number</property>
			<value>0</value>
		</set>
		
		
	</init>

	<step>
		<view>
			<heading-offset-deg>299.8</heading-offset-deg>
			<pitch-offset-deg>4.1</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.7</x-offset-m>
			<y-offset-m>0.0</y-offset-m>
			<z-offset-m>-3.9</z-offset-m>
			<field-of-view>65</field-of-view>
		</view>

		<marker>
			<x-m>-4.1175</x-m>
			<y-m>-0.1851</y-m>
			<z-m>0.1300</z-m>
			<scale>3.0000</scale>
		</marker>

		<message>
		Push the Rotorbrake lever forward by point and drag with LMB pressed
		</message>
		<exit>
			<condition>
			<less-than>
				<property>/controls/rotor/brake</property>
			<value>0.1</value>
			</less-than>
			</condition>
		</exit>
	</step>
	
	<step>
		<view>
			<heading-offset-deg>292.8</heading-offset-deg>
			<pitch-offset-deg>15.8</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.7</x-offset-m>
			<y-offset-m>0.0</y-offset-m>
			<z-offset-m>-3.9</z-offset-m>
			<field-of-view>37.1</field-of-view>
		</view>

		<marker>
			<x-m>-4.0588</x-m>
			<y-m>-0.2</y-m>
			<z-m>0.1870</z-m>
			<scale>3.0000</scale>
		</marker>

		<message>
		Push the Cutoff lever forward
		</message>
		<exit>
			<condition>
			<less-than>
			<property>/controls/engines/engine/cutoff</property>
			<value>0.1</value>
			</less-than>
			</condition>
		</exit>
	</step>
	
	<step>
		<view>
			<heading-offset-deg>4.5</heading-offset-deg>
			<pitch-offset-deg>-13.1</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.67</x-offset-m>
			<y-offset-m>0.03</y-offset-m>
			<z-offset-m>-3.93</z-offset-m>
			<field-of-view>40</field-of-view>
		</view>

		

		<message>
		The fuel tank sits below the engine- due to gravitity the fuellines are empty.
                     So you need first electrical power-press F10-key, go to "EC130" and select "Supply External Power":
		</message>
		<exit>
			<condition>
			
				<property>/controls/electric/external-power</property>
			
			</condition>
		</exit>
	</step>

	<step>
		<message>
		BAT EPU on and GENE on 
		</message>
		<view>
			<heading-offset-deg>323.3</heading-offset-deg>
			<pitch-offset-deg>-51.6</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.7</x-offset-m>
			<y-offset-m>0.0</y-offset-m>
			<z-offset-m>-3.9</z-offset-m>
			<field-of-view>35.5</field-of-view>
		</view>
		
		<marker>
			<x-m>-4.3555</x-m>
			<y-m>-0.4008</y-m>
			<z-m>-0.6626</z-m>
			<scale>4.0000</scale>
		</marker>

		<exit>
			<condition>
			<property>/controls/electric/battery-switch</property>
			<property>/controls/electric/engine/generator</property>					
			</condition>
		</exit>
	</step>

	<end>
		<message>On the VEMD after a testing phase you should see the Enginestartpage- 3 halfcircles with Torque, Ng (aka N2) and T4.</message>
		<view>
			<heading-offset-deg>332.00</heading-offset-deg>
			<pitch-offset-deg>-21.7</pitch-offset-deg>
			<field-of-view>35.5</field-of-view>
		</view>
		
	</end>
</PropertyList>
