<PropertyList>
  <name>Start Up</name>
  <description>
This tutorial will take you through the engine startup sequence for the Vulcan.

This is based ona  startup using a ground cart to provide power.
  </description>
  <audio-dir>Aircraft/vulcanb2/Tutorials/</audio-dir>
  <timeofday>morning</timeofday>
<!--  
  <presets>
    <airport-id>KLVK</airport-id>
    <on-ground>1</on-ground>
    <runway>12</runway>
    <altitude-ft>-9999</altitude-ft>
    <latitude-deg>37.6952</latitude-deg>
    <longitude-deg>-121.8167</longitude-deg>
    <heading-deg>175.0</heading-deg>
    <airspeed-kt>0</airspeed-kt>
    <glideslope-deg>0</glideslope-deg>
    <offset-azimuth-deg>0</offset-azimuth-deg>
    <offset-distance-nm>0</offset-distance-nm>
  </presets>
-->
  <presets/>
  
  <init>
    <set>
      <property>/controls/gear/brake-parking</property>
      <value>1</value>
    </set>
    <set>
      <property>/controls/flight/flaps</property>
      <value>0.0</value>
    </set>
    <set>
      <property>/instrumentation/adf/frequencies/selected-khz</property>
      <value>340</value>
    </set>
    <set>
      <property>/controls/flight/elevator-trim</property>
      <value>0.17</value>
    </set>
    <nasal>
      # Reset to a cold start.
      starter.setMasterOff();
    </nasal>
  </init>
  
  <step>
    <message>In this tutorial, we'll start up the engines on the Vulcan.</message>
  </step>
  
  <step>
    <message>This is the engine start console.</message>
    <view>
      <heading-offset-deg>67.5</heading-offset-deg>
      <pitch-offset-deg>-49.1</pitch-offset-deg>
      <roll-offset-deg>0.0</roll-offset-deg>
      <x-offset-m>-0.3</x-offset-m>
      <y-offset-m>1.1</y-offset-m>
      <z-offset-m>4.8</z-offset-m>
      <field-of-view>26.4</field-of-view>
    </view>
    
    <marker>
      <x-m>4.6875</x-m>
      <y-m>-0.6358</y-m>
      <z-m>0.5442</z-m>
      <scale>4.9833</scale>
    </marker>
  </step>
  
  <step>
    <message>First, switch the engine master ON, by selecting this switch.</message>

    <view>
      <heading-offset-deg>69.5</heading-offset-deg>
      <pitch-offset-deg>-53.2</pitch-offset-deg>
      <roll-offset-deg>0.0</roll-offset-deg>
      <x-offset-m>-0.3</x-offset-m>
      <y-offset-m>1.1</y-offset-m>
      <z-offset-m>4.8</z-offset-m>
      <field-of-view>14.4</field-of-view>
    </view>
    
    <marker>
      <x-m>4.6742</x-m>
      <y-m>-0.6167</y-m>
      <z-m>0.5292</z-m>
      <scale>1.1500</scale>
    </marker>

    <error>
      <message>Select the engine master switch</message>
      <condition>
        <less-than>
          <property>/controls/engines/master</property>
          <value>1</value>
        </less-than>
      </condition>
    </error>
    <exit>
      <condition>
        <equals>
          <property>/controls/engines/master</property>
          <value>1</value>
        </equals>
      </condition>
    </exit>
  </step>
  
  <step>
    <message>This is the engine start selector switch. Currently engine #1 is selected.</message>
    <view>
      <heading-offset-deg>69.5</heading-offset-deg>
      <pitch-offset-deg>-53.2</pitch-offset-deg>
      <roll-offset-deg>0.0</roll-offset-deg>
      <x-offset-m>-0.3</x-offset-m>
      <y-offset-m>1.1</y-offset-m>
      <z-offset-m>4.8</z-offset-m>
      <field-of-view>14.4</field-of-view>
    </view>
    
    <marker>
      <x-m>4.7058</x-m>
      <y-m>-0.6492</y-m>
      <z-m>0.5308</z-m>
      <scale>2.1333</scale>
    </marker>
  </step>
  
  <step>
    <message>Start the engine by selecting the start button.</message>
    <view>
      <heading-offset-deg>69.5</heading-offset-deg>
      <pitch-offset-deg>-53.2</pitch-offset-deg>
      <roll-offset-deg>0.0</roll-offset-deg>
      <x-offset-m>-0.3</x-offset-m>
      <y-offset-m>1.1</y-offset-m>
      <z-offset-m>4.8</z-offset-m>
      <field-of-view>14.4</field-of-view>
    </view>
    
    <marker>
      <x-m>4.6583</x-m>
      <y-m>-0.6492</y-m>
      <z-m>0.5308</z-m>
      <scale>1.8167</scale>
    </marker>
  </step>
  
  <step>
    <message>The start button will rise when the engine has started. Watch as the RPM rises.</message>
    <view>
      <heading-offset-deg>345.7</heading-offset-deg>
      <pitch-offset-deg>-24.0</pitch-offset-deg>
      <roll-offset-deg>0.0</roll-offset-deg>
      <x-offset-m>-0.2</x-offset-m>
      <y-offset-m>1.1</y-offset-m>
      <z-offset-m>4.8</z-offset-m>
      <field-of-view>25.3</field-of-view>
    </view>
    
    <marker>
      <x-m>4.1450</x-m>
      <y-m>-0.1400</y-m>
      <z-m>0.7217</z-m>
      <scale>3.2000</scale>
    </marker>
  </step>
  
  <end>
    <message>The other engines may be starting in turn by clicking on the engine selector switch, and pressing the start button.</message>
  </end>
</PropertyList>
