/****************************************************************************
**
** This file is part of Qt Creator
**
** Copyright (C) 2016 Blackberry
**
** Contact: Blackberry (qt@blackberry.com)
** Contact: KDAB (info@kdab.com)
**
** This file is part of Qt Creator.
**
** Commercial License Usage
** Licensees holding valid commercial Qt licenses may use this file in
** accordance with the commercial license agreement provided with the
** Software or, alternatively, in accordance with the terms contained in
** a written agreement between you and The Qt Company. For licensing terms
** and conditions see https://www.qt.io/terms-conditions. For further
** information use the contact form at https://www.qt.io/contact-us.
**
** GNU Free Documentation License Usage
** Alternatively, this file may be used under the terms of the GNU Free
** Documentation License version 1.3 as published by the Free Software
** Foundation and appearing in the file included in the packaging of
** this file. Please review the following information to ensure
** the GNU Free Documentation License version 1.3 requirements
** will be met: https://www.gnu.org/licenses/fdl-1.3.html.
** $QT_END_LICENSE$
**
****************************************************************************/

/*!
    \contentspage {Qt Creator Manual}
    \previouspage creator-developing-ios.html
    \page creator-developing-qnx.html
    \nextpage creator-developing-winrt.html

    \title Connecting QNX Devices

    You can connect QNX devices to the development PC to deploy, run and debug
    applications on them from within \QC.

    \section1 Adding a QNX Neutrino Device in \QC

    Adding a QNX Neutrino device is very similar to \l{Connecting Embedded
    Linux Devices}, except you need to select \uicontrol {QNX Device} in the
    \uicontrol {Device Configuration} wizard.
*/
