/****************************************************************************
**
** Copyright (C) 2018 The Qt Company Ltd.
** Contact: https://www.qt.io/licensing/
**
** This file is part of the Qt Creator documentation.
**
** Commercial License Usage
** Licensees holding valid commercial Qt licenses may use this file in
** accordance with the commercial license agreement provided with the
** Software or, alternatively, in accordance with the terms contained in
** a written agreement between you and The Qt Company. For licensing terms
** and conditions see https://www.qt.io/terms-conditions. For further
** information use the contact form at https://www.qt.io/contact-us.
**
** GNU Free Documentation License Usage
** Alternatively, this file may be used under the terms of the GNU Free
** Documentation License version 1.3 as published by the Free Software
** Foundation and appearing in the file included in the packaging of
** this file. Please review the following information to ensure
** the GNU Free Documentation License version 1.3 requirements
** will be met: https://www.gnu.org/licenses/fdl-1.3.html.
**
****************************************************************************/

// **********************************************************************
// NOTE: the sections are not ordered by their logical order to avoid
// reshuffling the file each time the index order changes (i.e., often).
// Run the fixnavi.pl script to adjust the links to the index order.
// **********************************************************************

/*!
    \contentspage index.html
    \page creator-connecting-mobile.html
    \previouspage creator-deployment-qnx.html
    \nextpage creator-developing-android.html

    \title Connecting Devices

    You can connect \l{glossary-device}{devices} to the development PC to run, debug,
    and analyze applications built for them from \QC. When you install Qt for a
    target platform, such as Android, QNX, or Universal Windows Platform (UWP),
    the build and run settings for the development targets might be set up
    automatically in \QC.

    You can connect the device to the development PC using a USB connection.
    Additionally, you can connect Linux-based devices by using a WLAN
    connection.

    \list

        \li \l{Connecting Android Devices}

            Qt applications for Android are compiled as \c {shared objects} that
            are loaded by a Java launcher that is part of Qt.
            This is totally transparent to users. As Qt is composed of libraries
            referencing each other, Qt 4 applications are only supported on
            Android version 1.6, or later, and Qt 5 applications on version
            4.1 (API level 16), or later. You must install a Qt version
            targeting Android and the Android SDK and NDK to develop for
            Android devices.

        \if defined(qtcreator)
        \li \l{Connecting Bare Metal Devices}

            You can connect bare metal devices to the development PC and use \QC
            to debug applications on them with GDB or a hardware debugger.
        \endif

        \li \l{Connecting Embedded Linux Devices}

            If you have a tool chain for building applications for embedded
            Linux devices installed on the development
            PC, you can add it and the device to \QC.

        \if defined(qtcreator)
        \li \l{Connecting iOS Devices}

            You use the tools delivered with Xcode to connect devices to \QC.
            \QC detects the tools and configured devices automatically and uses
            the tools to build, deploy, and run applications.

        \li \l{Connecting QNX Devices}

            You can connect QNX devices to the development PC to deploy, run and
            debug applications on them from within \QC. This is currently only
            supported for QNX Neutrino devices, and requires the QNX SDK to be
            installed on the development PC.
        \endif

    \endlist

    \if defined(qtcreator)
    \section1 Related Topics

    \list

        \li \l{Connecting Devices by Serial Ports}

            You can connect devices by serial ports in the
            \uicontrol {Serial Terminal} output pane. These
            ports can be real RS-232 ports, or virtual serial
            ports provided by USB chipsets.

        \li \l{https://doc.qt.io/qtcreator/creator-overview-qtasam.html}
            {Qt Creator Plugin for Qt Application Manager}

            You can use the experimental Qt Application Manager plugin
            (commercial only) to deploy, run, and debug applications on the
            local Linux PC, remote generic SSH Linux targets, or
            \l{Embedded Devices}{embedded devices}.
    \endlist
    \endif
*/
