/****************************************************************************
**
** Copyright (C) 2022 The Qt Company Ltd.
** Contact: https://www.qt.io/licensing/
**
** This file is part of the Qt Creator documentation.
**
** Commercial License Usage
** Licensees holding valid commercial Qt licenses may use this file in
** accordance with the commercial license agreement provided with the
** Software or, alternatively, in accordance with the terms contained in
** a written agreement between you and The Qt Company. For licensing terms
** and conditions see https://www.qt.io/terms-conditions. For further
** information use the contact form at https://www.qt.io/contact-us.
**
** GNU Free Documentation License Usage
** Alternatively, this file may be used under the terms of the GNU Free
** Documentation License version 1.3 as published by the Free Software
** Foundation and appearing in the file included in the packaging of
** this file. Please review the following information to ensure
** the GNU Free Documentation License version 1.3 requirements
** will be met: https://www.gnu.org/licenses/fdl-1.3.html.
**
****************************************************************************/

// **********************************************************************
// NOTE: the sections are not ordered by their logical order to avoid
// reshuffling the file each time the index order changes (i.e., often).
// Run the fixnavi.pl script to adjust the links to the index order.
// **********************************************************************

/*!
    \page creator-deployment-embedded-linux.html
    \previouspage creator-deployment-b2qt.html
    \if defined(qtdesignstudio)
    \nextpage creator-connecting-mobile.html
    \else
    \nextpage creator-deployment-qnx.html
    \endif

    \title Deploying Applications to Generic Remote Linux Devices

    You can specify settings for deploying applications to generic remote
    Linux devices in the project configuration file and in the
    \uicontrol Projects mode, in \uicontrol {Run Settings}.

    \image qtcreator-embedded-linux-deployment-details.png "Deploy to embedded Linux"

    The files to be installed are listed in the \uicontrol {Deployment} step,
    the \uicontrol {Files to deploy} field. The \uicontrol {Local File Path}
    field displays the location of the file on the development PC. The
    \uicontrol {Remote Directory} field displays the directory where the file is
    installed on the device. Text in red color indicates that the information is
    missing.

    \section1 Adding Missing Files

    The process to add files to deploy depends on the build system you use.

    \section2 CMake Builds

    When using CMake as the build system, use the \l{CMake: install command}
    {install} command in the CMakeLists.txt file to add the missing files.

    For example, add the following lines to the CMakeLists.txt file to install
    the binary of your project to the \c /opt directory on the remote device:

    \badcode
    set(INSTALL_DESTDIR "/opt")

    install(TARGETS <target>
        RUNTIME DESTINATION "${INSTALL_DESTDIR}"
        BUNDLE DESTINATION "${INSTALL_DESTDIR}"
        LIBRARY DESTINATION "${INSTALL_DESTDIR}"
    )
    \endcode

    \section2 qmake Builds

    When using qmake, edit the \l{Variables#installs}{INSTALLS variable} in
    the project \c .pro file.

    When you run the application, \QC copies the necessary files to the device
    and starts the application on it.

    For example, add the following lines to the \c .pro file to copy the binary
    of your project to the \c /opt directory on the remote device:

    \code
      target.path = /opt
      INSTALLS += target
    \endcode

    To deploy additional files, add them to further targets that you also add
    to \c INSTALLS.

    \section1 Deploy Steps

    When you run the application on the device, \QC first uploads the
    necessary files to it, as specified by the deploy steps.

    \section2 Finding Configured Devices

    The \uicontrol {Check for a configured device} step looks for a device that
    is ready for deployment.

    \section2 Checking for Free Disk Space

    The \uicontrol {Check for free disk space} step is by default the first
    deploy step. Use it to find out whether the remote file system has enough
    space left to deploy your project. Errors due to lack of disk space can
    otherwise be hard to detect.

    \note If the SFTP upload fails, make sure that the remote device has SFTP
    enabled in its SSH daemon. Some versions of Dropbear that come without SFTP
    support will crash when an SFTP upload is being attempted. This is not a bug
    in \QC.

    \section2 Uploading Files

    By default, \QC copies the application files to the device by
    using the SSH file transfer protocol (SFTP), as specified by
    the \uicontrol {Upload files via SFTP} step.

    If you have a lot of data to copy, select \uicontrol Details in the
    \uicontrol {Upload Files via SFTP} step, and then select the
    \uicontrol {Incremental deployment} check box. \QC takes note of the
    deployment time and only copies files that have changed since the last
    deployment. However, when you make major changes on the device, such as
    removing files from the device manually or flashing a new disk image, or
    when you use another device with the same IP address, deselect the check box
    once, to have \QC deploy all files again.

    \section2 Creating a Tarball

    To only create a tarball and not copy the files to the device, select
    \uicontrol {Add Deploy Step} > \uicontrol {Create tarball}. Then remove all
    other deploy steps.

    The \uicontrol {Deploy tarball via SFTP upload} step specifies that \QC
    uploads the tarball to the device and extracts it.
*/
